AdapterId 06FE5h

AdapterName "DigiBoard PS-COM/8"

NumBytes 1

NamedItem

Prompt "UART Address Range"

choice "0xDB80 -> 0xDBC0"
	      pos[0]=xxxx000xb
	      io 0db80h-0dbc0h
choice "0xDC00 -> 0xDC40"
	      pos[0]=xxxx001xb
	      io 0dc00h-0dc40h
choice "0xBB80 -> 0xBBC0"
	      pos[0]=xxxx010xb
	      io 0bb80h-0bbc0h
choice "0xBC00 -> 0xBC40"
	      pos[0]=xxxx011xb
	      io 0bc00h-0bc40h
choice "0xAB80 -> 0xABC0"
	      pos[0]=xxxx100xb
	      io 0ab80h-0abc0h
choice "0xAC00 -> 0xAC40"
	      pos[0]=xxxx101xb
	      io 0ac00h-0ac40h
choice "0xCB80 -> 0xCBC0"
	      pos[0]=xxxx110xb
	      io 0cb80h-0cbc0h


Help

"No Help Available"


NamedItem

Prompt "Com2 Status"

choice "Disabled"
	      pos[0]=0xxxxxxxb
choice "Enabled"
	      pos[0]=1xxxxxxxb
	      io 02f8h-02ffh
Help

"No help is Available"

NamedItem

Prompt "Interrupt Select"

choice "INT 3" pos[0]=x000xxxxb   int 3
choice "INT 4" pos[0]=x001xxxxb   int 4
choice "INT 5" pos[0]=x010xxxxb   int 5
choice "INT 7" pos[0]=x011xxxxb   int 7
choice "INT 10" pos[0]=x100xxxxb  int 10
choice "INT 11" pos[0]=x101xxxxb  int 11
choice "INT 12" pos[0]=x110xxxxb  int 12
choice "INT 15" pos[0]=x111xxxxb  int 15

Help

"No Help is currently available"
