;***************************************************************************
;* Copyright (C) 1992 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

AdapterId 0812Eh

AdapterName "NCR 3350/3355 HPG Video Adapter (w/o ROM)"

NumBytes 4

FixedResources
        pos[0]=XXXXXXXXb

NamedItem
    Prompt "Adapter Enable"
      choice "Enable"		pos[0]=XXXXXXX1b
      choice "Disable"		pos[0]=XXXXXXX0b	
  Help
"Select Disable to prevent use of high resolution video modes. 
Select Enable for normal operation."

NamedItem
    Prompt "I/O Address Select"
      choice "6C80h"    pos[0]=00XXXXXXb	io 06C80h-06C8Fh
      choice "6E80h"    pos[0]=01XXXXXXb	io 06E80h-06E8Fh
      choice "7C80h"    pos[0]=10XXXXXXb	io 07C80h-07C8Fh
      choice "7E80h"    pos[0]=11XXXXXXb	io 07E80h-07E8Fh
  Help
"Set the Board I/O address so it will not conflict with 
other devices."

NamedItem
  Prompt "Interrupt Level"
      choice "IRQ Level 9"	pos[0]=XXXXX00Xb  int 9
      choice "IRQ Level 7"	pos[0]=XXXXX01Xb  int 7
      choice "IRQ Level 5"	pos[0]=XXXXX10Xb  int 5
      choice "IRQ Level 3"	pos[0]=XXXXX11Xb  int 3

  Help
"Select the interrupt request level so it will not conflict
with other devices."

NamedItem
   Prompt "On-Board ROM Starting Address"
	choice "DISABLE"	pos[0]=XXXXXXXXb
   Help
"The On-Board ROM has been disabled by hardware switch 1.  You should not
enable the On-Board ROM (with switch 1) unless a ROM module is installed
in the socket. Enabling the ROM will cause the adapter ID to change to
817EH."

NamedItem
   Prompt "Frame Buffer Cacheable"
	choice "Cacheable"            pos[1]=XXXXX1XXb
	choice "Not Cacheable"        pos[1]=XXXXX0XXb
   Help
"Set to Cacheable to allow cacheing of the Frame Buffer, otherwise 
select Not Cacheable.  Usually best performance is acheived when
the frame buffer is set to cacheable."

NamedItem
   Prompt "Memory Map Select"
	choice "512M"           pos[1]=XXXXXX01b  mem 20000000h-203FFFFFh
	choice "640M"           pos[1]=XXXXXX10b  mem 28000000h-283FFFFFh
	choice "768M"           pos[1]=XXXXXX11b  mem 30000000h-303FFFFFh
	choice "Disable"        pos[1]=XXXXXX00b
   Help
"Select the location for video memory so it will not conflict with other
devices."
