
AdapterId 05333h

AdapterName "National Instruments MC-GPIB IEEE-488 Interface"

NumBytes 2

NamedItem
        Prompt "I/O Base Address for MC-GPIB"
     choice "IOBASE 0E00" pos[0]=0000111Xb  io 00e00h-00fffh
     choice "IOBASE 1E00" pos[0]=0001111Xb  io 01e00h-01fffh
     choice "IOBASE 2E00" pos[0]=0010111Xb  io 02e00h-02fffh
     choice "IOBASE 3E00" pos[0]=0011111Xb  io 03e00h-03fffh
     choice "IOBASE 4E00" pos[0]=0100111Xb  io 04e00h-04fffh
     choice "IOBASE 5E00" pos[0]=0101111Xb  io 05e00h-05fffh
     choice "IOBASE 6E00" pos[0]=0110111Xb  io 06e00h-06fffh
     choice "IOBASE 7E00" pos[0]=0111111Xb  io 07e00h-07fffh
     choice "IOBASE 8E00" pos[0]=1000111Xb  io 08e00h-08fffh
     choice "IOBASE 9E00" pos[0]=1001111Xb  io 09e00h-09fffh
     choice "IOBASE AE00" pos[0]=1010111Xb  io 0ae00h-0afffh
     choice "IOBASE BE00" pos[0]=1011111Xb  io 0be00h-0bfffh
     choice "IOBASE CE00" pos[0]=1100111Xb  io 0ce00h-0cfffh
     choice "IOBASE DE00" pos[0]=1101111Xb  io 0de00h-0dfffh
     choice "IOBASE EE00" pos[0]=1110111Xb  io 0ee00h-0efffh
     choice "IOBASE FE00" pos[0]=1111111Xb  io 0fe00h-0ffffh
Help
   "This interface can be assigned 16 different I/O base
    addresses.  Use the F5=Previous and the F6=Next keys to
    change the MC-GPIB Base I/O address assignment if you are in
    the 'Change configuration' window.  Conflicting assignments
    are marked with an asterisk and must be changed to use the
    adapter."

NamedItem
        Prompt "Interrupt Level for MC-GPIB"
      choice "Int_3"     pos[1]=010XXXXXb int 3
      choice "Int_5"     pos[1]=011XXXXXb int 5
      choice "Int_10"    pos[1]=100XXXXXb int 10
      choice "Int_11"    pos[1]=101XXXXXb int 11
      choice "Int_15"    pos[1]=110XXXXXb int 15
      choice "Not Used"  pos[1]=000XXXXXb 
   Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change the interrupt level assignments if you are in the
      'Change configuration' window."

NamedItem
        Prompt "Arbitration Level for MC-GPIB"
      choice "Level_0"   pos[1]=XXXX0000b  arb  0
      choice "Level_1"   pos[1]=XXXX0001b  arb  1
      choice "Level_2"   pos[1]=XXXX0010b  arb  2
      choice "Level_3"   pos[1]=XXXX0011b  arb  3
      choice "Level_4"   pos[1]=XXXX0100b  arb  4
      choice "Level_5"   pos[1]=XXXX0101b  arb  5
      choice "Level_6"   pos[1]=XXXX0110b  arb  6
      choice "Level_7"   pos[1]=XXXX0111b  arb  7
      choice "Level_8"   pos[1]=XXXX1000b  arb  8
      choice "Level_9"   pos[1]=XXXX1001b  arb  9
      choice "Level_10"  pos[1]=XXXX1010b  arb 10
      choice "Level_11"  pos[1]=XXXX1011b  arb 11
      choice "Level_12"  pos[1]=XXXX1100b  arb 12
      choice "Level_13"  pos[1]=XXXX1101b  arb 13
      choice "Level_14"  pos[1]=XXXX1110b  arb 14
      choice "No DMA"    pos[1]=XXXX1111b
Help
      "This assignment need only be changed if it is in conflict
      with another assignment.  Conflicting assignments are marked
      with an asterisk.  Use the F5=Previous and the F6=Next keys
      to change arbitration level assignments if you are in the
      'Change configuration' window."

nameditem
        Prompt  "Fairness On/Off"
          Choice  "On"
            pos[1]=XXX1XXXXb
          Choice  "Off"
            pos[1]=XXX0XXXXb
        Help
        "Bus Arbitration Fairness.  This controls whether the adapter will
         release control of the bus when it has been using it exclusively.
         Under normal circumstances, select <On>."
