AdapterId 07001h

AdapterName "AST Advantage/2 With Dual Serial Port Option"

NumBytes 4

NamedItem
     Prompt "WAIT STATE"
      choice "1 wait state " pos[1]=0XXXXXXXb
      choice "0 wait state " pos[1]=1XXXXXXXb
   Help
 "MEMORY WAIT STATE SELECTION"

NamedItem
	Prompt "MEMORY CONFIGURATION"
      choice "DISABLED"   pos[0]=0000000Xb
      choice ".5M,0K,0K,0K    TOTAL = 0.5 MB" pos[0]=0001001Xb
      choice " 2M,0K,0K,0K    TOTAL = 2.0 MB" pos[0]=0010001Xb
      choice ".5M,.5M,0K,0K   TOTAL = 1.0 MB" pos[0]=0011001Xb
      choice ".5M,2M,0K,0K    TOTAL = 2.5 MB" pos[0]=0100001Xb
      choice " 2M,2M,0K,0K    TOTAL = 4.0 MB" pos[0]=0101001Xb
      choice ".5M,.5M,.5M,0K  TOTAL = 1.5 MB" pos[0]=0110001Xb
      choice ".5M,.5M,2M,0K   TOTAL = 3.0 MB" pos[0]=0111001Xb
      choice ".5M,2M,2M,0K    TOTAL = 4.5 MB" pos[0]=1000001Xb
      choice " 2M,2M,2M,0K    TOTAL = 6.0 MB" pos[0]=1001001Xb
      choice ".5M,.5M,.5M,.5M TOTAL = 2.0 MB" pos[0]=1010001Xb
      choice ".5M,.5M,.5M,2M  TOTAL = 3.5 MB" pos[0]=1011001Xb
      choice ".5M,.5M,2M,2M   TOTAL = 5.0 MB" pos[0]=1100001Xb
      choice ".5M,2M,2M,2M    TOTAL = 6.5 MB" pos[0]=1101001Xb
      choice " 2M,2M,2M,2M    TOTAL = 8.0 MB" pos[0]=1110001Xb
   Help
"This is memory configuration on your ADVANTAGE/2
starting from top of the board BANK0,BANK1,BANK2,BANK3"

NamedItem
     Prompt "Connector 1"
	choice "SERIAL_1" 
                      pos[2]=1000XXXXb 
                      pos[3]=xx1xxxxxb
                      io 03f8h-03ffh int 4	
	choice "SERIAL_2" 
                      pos[2]=1001XXXXb 
                      pos[3]=xx1xxxxxb
                      io 02f8h-02ffh int 3	
	choice "SERIAL_3" 
                      pos[2]=1010XXXXb 
                      pos[3]=xx1xxxxxb
                      io 3220h-3227h int 3
	choice "SERIAL_4" 
                      pos[2]=1011XXXXb 
                      pos[3]=xx1xxxxxb
                      io 3228h-322fh int 3	
	choice "SERIAL_5" 
                      pos[2]=1100XXXXb 
                      pos[3]=xx1xxxxxb
                      io 4220h-4227h int 3	
	choice "SERIAL_6" 
                      pos[2]=1101XXXXb 
                      pos[3]=xx1xxxxxb
                      io 4228h-422fh int 3	
	choice "SERIAL_7" 
                      pos[2]=1110XXXXb 
                      pos[3]=xx1xxxxxb
                      io 5220h-5227h int 3	
	choice "SERIAL_8" 
                      pos[2]=1111XXXXb 
                      pos[3]=xx1xxxxxb
                      io 5228h-522fh int 3	
        choice "DISABLE" 
                      pos[3]=xx0xxxxxb 
     Help
	"Connector 1 of the AST Advantage/2 Dual Serial Port 
        Option can have any one of the Serial 1 to  Serial 8 
        assignments and can also be disabled.  Use the F5=
        Previous and  F6=Next keys to change the Connector 1
        Serial Port assignment  when you are in the  'Change 
	Configuration' window.  Conflicting  assignments are 
	marked with an asterisk and should be changed."

NamedItem
     Prompt "Connector 2"
	choice "SERIAL_1" 
                      pos[2]=XXXX000Xb 
                      pos[3]=xxx1xxxxb
                      io 03f8h-03ffh int 4	
	choice "SERIAL_2" 
                      pos[2]=XXXX001Xb 
                      pos[3]=xxx1xxxxb
                      io 02f8h-02ffh int 3	
	choice "SERIAL_3" 
                      pos[2]=XXXX010Xb 
                      pos[3]=xxx1xxxxb
                      io 3220h-3227h int 3	
	choice "SERIAL_4" 
                      pos[2]=XXXX011Xb 
                      pos[3]=xxx1xxxxb
                      io 3228h-322fh int 3	
	choice "SERIAL_5" 
                      pos[2]=XXXX100Xb 
                      pos[3]=xxx1xxxxb
                      io 4220h-4227h int 3	
	choice "SERIAL_6" 
                      pos[2]=XXXX101Xb 
                      pos[3]=xxx1xxxxb
                      io 4228h-422fh int 3	
	choice "SERIAL_7" 
                      pos[2]=XXXX110Xb 
                      pos[3]=xxx1xxxxb
                      io 5220h-5227h int 3	
	choice "SERIAL_8" 
                      pos[2]=XXXX111Xb 
                      pos[3]=xxx1xxxxb
                      io 5228h-522fh int 3	
        choice "DISABLE" 
                      pos[3]=xxx0xxxxb
     Help
	"Connector 2 of the AST Advantage/2 Dual Serial Port 
        Option can have any one of the Serial 1 to  Serial 8 
        assignments and can also be disabled.  Use the F5=
        Previous and F6=Next keys to change the  Connector 2
        Serial Port assignment  when you are in the  'Change 
        Configuration' window.  Conflicting  assignments are 
	marked with an asterisk and should be changed."


