; rev.02 2/22/93

AdapterId 0678Bh

AdapterName " NeoTecH Dual RS-232 Async. Adapter"

Numbytes 2

NamedItem
        Prompt "Upper connector address"
        choice "SERIAL_2 (02f8h)" pos[0]=XXXX001Xb io 02f8h-02ffh 
        choice "SERIAL_3 (3220h)" pos[0]=XXXX010Xb io 3220h-3227h 
        choice "SERIAL_4 (3228h)" pos[0]=XXXX011Xb io 3228h-322fh 
        choice "SERIAL_5 (4220h)" pos[0]=XXXX100Xb io 4220h-4227h 
        choice "SERIAL_6 (4228h)" pos[0]=XXXX101Xb io 4228h-422fh 
        choice "SERIAL_7 (5220h)" pos[0]=XXXX110Xb io 5220h-5227h 
        choice "SERIAL_8 (5228h)" pos[0]=XXXX111Xb io 5228h-522fh 
        choice "SERIAL_1 (03f8h)" pos[0]=XXXX000Xb io 03f8h-03ffh

Help
"This connector can be assigned to Serial 1-8. Use F5=Previous and the 
F6=Next keys to change serial port assignments if you are in the 'Change 
configuration' window. Conflicting assignments are marked with an asterisk 
and must be changed to use the adapter."

NamedItem
        Prompt "Upper connector interrupt"
        choice "Int 3" pos[0]=XX00XXXXb int 3
        choice "Int 4" pos[0]=XX01XXXXb int 4
        choice "Int 7" pos[0]=XX10XXXXb int 7
        choice "Int 9" pos[0]=XX11XXXXb int 9

Help
"This connector can be assigned to Interrupt level 3, 4, 7, or 9. Use 
F5=Previous and the F6=Next keys to change serial port assignments if you are 
in the 'Change configuration' window. Conflicting assignments are marked 
with an asterisk and must be changed to use the adapter."


NamedItem
        Prompt "Lower connector address"
        choice "SERIAL_3 (3220h)" pos[1]=XXXX010Xb io 3220h-3227h 
        choice "SERIAL_4 (3228h)" pos[1]=XXXX011Xb io 3228h-322fh 
        choice "SERIAL_5 (4220h)" pos[1]=XXXX100Xb io 4220h-4227h 
        choice "SERIAL_6 (4228h)" pos[1]=XXXX101Xb io 4228h-422fh 
        choice "SERIAL_7 (5220h)" pos[1]=XXXX110Xb io 5220h-5227h 
        choice "SERIAL_8 (5228h)" pos[1]=XXXX111Xb io 5228h-522fh 
        choice "SERIAL_1 (03f8h)" pos[1]=XXXX000Xb io 03f8h-03ffh 
        choice "SERIAL_2 (02f8h)" pos[1]=XXXX001Xb io 02f8h-02ffh 

Help
"This connector can be assigned to Serial 1-8. Use F5=Previous and the 
F6=Next keys to change serial port assignments if you are in the 'Change 
configuration' window. Conflicting assignments are marked with an asterisk 
and must be changed to use the adapter."


NamedItem
        Prompt "Lower connector interrupt"
        choice "Int 3" pos[1]=XX00XXXXb int 3
        choice "Int 4" pos[1]=XX01XXXXb int 4
        choice "Int 7" pos[1]=XX10XXXXb int 7
        choice "Int 9" pos[1]=XX11XXXXb int 9

Help
"This connector can be assigned to Interrupt level 3, 4, 7, or 9. Use 
F5=Previous and the F6=Next keys to change serial port assignments if you are 
in the 'Change configuration' window. Conflicting assignments are marked 
with an asterisk and must be changed to use the adapter."


