AdapterID 0800Dh

AdapterName  "PIXELWORKS PS/2 Ultra Clipper Graphics Subsystem V1.1"

NumBytes 2

Nameditem
        Prompt  "Interrupt Level"
          choice  "Level 10"  pos[0]=XXXX001Xb   int 10
          choice  "Level 11"  pos[0]=XXXX010Xb   int 11
          choice  "Level 15"  pos[0]=XXXX100Xb   int 15
          choice  "No Ints "  pos[0]=XXXX000Xb
        Help
        "This selects the interrupt level used by the Ultra Clipper/MCA to
         gain processor attention.  Under normal circumstances, select
         <Level 10>."

Nameditem
        Prompt  "I/O Address"
          choice  "0330-0337"  pos[0]=XX01XXXXb   io 0330h-0337h
          choice  "0340-0347"  pos[0]=XX10XXXXb   io 0340h-0347h
          choice  "0300-0307"  pos[0]=XX00XXXXb   io 0300h-0307h
          choice  "0370-0377"  pos[0]=XX11XXXXb   io 0370h-0377h
        Help
        "This selects the Microchannel IO bus address the Ultra Clipper/MCA
         will respond to.  Under normal circumstances, select <0330h-0337h>."

Nameditem
        Prompt  "DMA Arbitration Level"
          choice  "Level 6"   pos[1]=XX11001Xb   arb 6
          choice  "Level 7"   pos[1]=XX11000Xb   arb 7
          choice  "Level 8"   pos[1]=XX10111Xb   arb 8
          choice  "Level 9"   pos[1]=XX10110Xb   arb 9
          choice  "Level 10"  pos[1]=XX10101Xb   arb 10
          choice  "Level 11"  pos[1]=XX10100Xb   arb 11
          choice  "Level 12"  pos[1]=XX10011Xb   arb 12
          choice  "Level 13"  pos[1]=XX10010Xb   arb 13
          choice  "Level 14"  pos[1]=XX10001Xb   arb 14
          choice  "Level 4"   pos[1]=XX11011Xb   arb 4
          choice  "Level 5"   pos[1]=XX11010Xb   arb 5
        Help
        "This selects the DMA channel the Ultra Clipper/MCA will use to
         transfer data. Under normal circumstances, select <Level 6>.
         Please READ your Pixelworks driver documentation for exact
         information on how to configure the Ultra Clipper/MCA for a
         specific application package.  Call 1-603-880-1322 for 
         technical assistance."

Nameditem
        Prompt  "Single Screen Display"
          choice  "On"   pos[1]=X1XXXXXXb
          choice  "Off"  pos[1]=X0XXXXXXb
        Help
        "This selects the power up mode of the Ultra Clipper/MCA Screen.
	 If a monitor is directly connected to the Motherboard VGA select
         <OFF>.  The Ultra Clipper/MCA must be connected to a MULTISYNC 
         monitor (30khz-64khz) for this feature to work properly."
