AdapterId 07082h

AdapterName "AST Advantage/2 -386 Adapter"

NumBytes 4

NamedItem
      Prompt "Memory size configuration "
      choice "MEMORY DISABLED"  POS[0]=X000XXXXb
      choice "1 MEGABYTES"      POS[0]=X001XXXXb
      choice "2 MEGABYTES"      POS[0]=X010XXXXb
      choice "4 MEGABYTES"      POS[0]=X011XXXXb
      choice "5 MEGABYTES"      POS[0]=X100XXXXb
      choice "8 MEGABYTES"      POS[0]=X101XXXXb


Help
" Memory Size Configuration indicates the amount of memory in
Bank0 and Bank1.  For one megabyte (MB), Bank0 is populated only.
Two MB's consists of Bank0 and Bank1 having one MB each.  Four MB's
consists of 4 MB's in Bank0 and none in Bank1.  Five MB's will have
one MB in Bank0 and four MB's in Bank1.  Eight MB's consists of four
MB's in Bank0 and four MB's in Bank1.   "

NamedItem
      Prompt "Wait State selection"
      choice "0 WAIT STATES"  pos[1]=1XXXXXXXb
      choice "1 WAIT STATE"   pos[1]=0XXXXXXXb

Help
" An additional wait state is inserted during any memory access when
  the choice '1 WAIT STATE' is made ."

NamedItem
     Prompt "Connector 1"
      choice "SERIAL_1"
		       pos[2]=xxxx000xb
		       pos[3]=xxx1xxxxb
		       io 03f8h-03ffh int 4
      choice "SERIAL_2"
		       pos[2]=xxxx001xb
		       pos[3]=xxx1xxxxb
		       io 02f8h-02ffh int 3
      choice "SERIAL_3"
		       pos[2]=xxxx010xb
		       pos[3]=xxx1xxxxb
		       io 3220h-3227h int 3
      choice "SERIAL_4"
		       pos[2]=xxxx011xb
		       pos[3]=xxx1xxxxb
		       io 3228h-322fh int 3
      choice "SERIAL_5"
		       pos[2]=xxxx100xb
		       pos[3]=xxx1xxxxb
		       io 4220h-4227h int 3
      choice "SERIAL_6"
		       pos[2]=xxxx101xb
		       pos[3]=xxx1xxxxb
		       io 4228h-422fh int 3
      choice "SERIAL_7"
		       pos[2]=xxxx110xb
		       pos[3]=xxx1xxxxb
		       io 5220h-5227h int 3
      choice "SERIAL_8"
		       pos[2]=xxxx111xb
		       pos[3]=xxx1xxxxb
		       io 5228h-522fh int 3
      choice "DISABLE"
		       pos[3]=xxx0xxxxb
   Help
      "Connector 1 of  Advantage/2 Serial  and  Parallel Port
      Option can have  any one of the  Serial 1  to  Serial 8
      assignments  and	can  also  be  disabled.  Use the F5=
      Previous and the F6=Next keys to change the Connector 1
      Serial port assignments  when  you  are  in the 'Change
      Configuration'  window.   Conflicting  assignments  are
      marked with an Asterisk and should be changed."

NamedItem
   Prompt "Connector 2"
	choice "PARALLEL_1" pos[0]=xxxx01xxb io 03bch-03bfh int 7
	choice "PARALLEL_2" pos[0]=xxxx10xxb io 0378h-037fh int 7
	choice "PARALLEL_3" pos[0]=xxxx11xxb io 0278h-027fh int 7
	choice "DISABLE"    pos[0]=xxxx00xxb
   Help
      "Connector 2  of the  Advantage/2  Serial  and Parallel
      Port Option can  have  any  one  of  the	Parallel 1 to
      Parallel 3 assignments and can  also  be disabled.  Use
      the  F5=Previous	and  the F6=Next  keys	to change the
      Connector 2 Parallel Port  assignments  when you are in
      the 'Change Configuration' window.   Conflicting assig-
      nments  are  marked  with  an  Asterisk  and  should be
      changed."
