
AdapterID 0DF9Fh

AdapterName  "Integrated Fixed Disk and Controller"

NumBytes 3

fixedresources
        pos[1]=00XXXXXXb
        int 0eh
        exec

nameditem
        Prompt  "DMA Arbitration Level"
          Choice  "Level 5"
            pos[0]=XX0101XXb
            arb 5
          Choice  "Level 6"
            pos[0]=XX0110XXb
            arb 6
          Choice  "Level 7"
            pos[0]=XX0111XXb
            arb 7
          Choice  "Level 0"
            pos[0]=XX0000XXb
            arb 0
          Choice  "Level 1"
            pos[0]=XX0001XXb
            arb 1
          Choice  "Level 3"
            pos[0]=XX0011XXb
            arb 3
          Choice  "Level 4"
            pos[0]=XX0100XXb
            arb 4
        Help
        "This selects the DMA channel the adapter will use to transfer data.
         Under normal circumstances, select <Level 5>.  Use the F5=Previous
         or the F6=Next keys to change this assignment in the 'Change
         configuration' window."

nameditem
        Prompt  "DMA Burst Pacing Interval"
          Choice  "24 Microseconds"
            pos[1]=XX10XXXXb
          Choice  "31 Microseconds"
            pos[1]=XX11XXXXb
          Choice  "16 Microseconds"
            pos[1]=XX01XXXXb
          Choice  "Burst Disabled"
            pos[1]=XX00XXXXb
        Help
        "This is the time interval between DMA transfer bursts during
         which the Micro Channel is released by the fixed disk controller
         for use by the processor.  Under normal circumstances, select
         <24 Microseconds>.  Use the F5=Previous or the F6=Next keys to
         change this assignment in the 'Change configuration' window."

nameditem
        Prompt  "DMA Pacing Control"
          Choice  vcheck  "Disabled"
            pos[2]=XXXXXXX1b
          Choice  vcheck  "Enabled"
            pos[2]=XXXXXXX0b
        Help
        "This enables or disables the 'DMA Burst Pacing Interval.' If the
         'DMA Burst Pacing Interval' is set to <Burst Disabled>, the DMA
         Pacing Control will be disabled.  Under normal circumstances,
         select <Disabled>.  Use the F5=Previous or the F6=Next keys to
         change this assignment in the 'Change configuration' window."

nameditem
        Prompt  "Time to Release"
          Choice  vcheck  "6 Microseconds"
            pos[2]=XXXXX1XXb
          Choice  vcheck  "3 Microseconds"
            pos[2]=XXXXX01Xb
          Choice  vcheck  "Immediate"
            pos[2]=XXXXX00Xb
        Help
        "This controls the amount of time that the fixed disk controller
         will keep the Micro Channel after being preempted. If the 'DMA
         Pacing Control' is set to <Enabled>, the Time to Release will default
         to immediate.  Under normal circumstances, select <6 Microseconds>.
         Use the F5=Previous or the F6=Next keys to change this assignment
         in the 'Change configuration' window."

nameditem
        Prompt  "Fairness On/Off"
          Choice  "On"
            pos[0]=X1XXXXXXb
          Choice  "Off"
            pos[0]=X0XXXXXXb
        Help
        "Bus Arbitration Fairness.  This controls whether the adapter will
         release control of the bus when it has been using it exclusively.
         Under normal circumstances, select <On>.  Use the F5=Previous or
         the F6=Next keys to change this assignment in the 'Change
         configuration' window."

nameditem
        Prompt  "Primary/Alternate Port Addresses"
          Choice  "Primary"
            pos[0]=XXXXXX0Xb
            io 3510h-3517h
          Choice  "Alternate"
            pos[0]=XXXXXX1Xb
            io 3518h-351fh
        Help
        "Primary/Alternate Port Addresses.  This assigns the port addresses
         used by the adapter.  Either <Primary> or <Alternate> will work
         equally well.  If there are two integrated fixed disks, then select
         <Primary> for one and <Alternate> for the other.  Use the F5=Previous
         or the F6=Next keys to change this assignment in the 'Change
         configuration' window."
