AdapterID 05F77h

AdapterName  "Future Domain SCSI Adapter"

NumBytes 2

nameditem
        Prompt  "Adapter Memory Location"
          Choice "Segment CA00" pos[1]=xxxx0000b mem 0ca00h-0cbffh
          Choice "Segment C000" pos[1]=xxxx0001b mem 0c000h-0c1ffh
          Choice "Segment C200" pos[1]=xxxx0010b mem 0c200h-0c3ffh
          Choice "Segment C400" pos[1]=xxxx0011b mem 0c400h-0c5ffh
          Choice "Segment C600" pos[1]=xxxx0100b mem 0c600h-0c7ffh
          Choice "Segment C800" pos[1]=xxxx0101b mem 0c800h-0c9ffh
          Choice "Segment CC00" pos[1]=xxxx0110b mem 0cc00h-0cdffh
          Choice "Segment CE00" pos[1]=xxxx0111b mem 0ce00h-0cfffh
          Choice "Segment D000" pos[1]=xxxx1000b mem 0d000h-0d1ffh
          Choice "Segment D200" pos[1]=xxxx1001b mem 0d200h-0d3ffh
          Choice "Segment D400" pos[1]=xxxx1010b mem 0d400h-0d5ffh
          Choice "Segment D600" pos[1]=xxxx1011b mem 0d600h-0d7ffh
          Choice "Segment D800" pos[1]=xxxx1100b mem 0d800h-0d9ffh
          Choice "Segment DA00" pos[1]=xxxx1101b mem 0da00h-0dbffh
          Choice "Segment DC00" pos[1]=xxxx1110b mem 0dc00h-0ddffh
          Choice "Segment DE00" pos[1]=xxxx1111b mem 0de00h-0dfffh
        Help
"To configure this adapter you must choose the memory location the
adapter will use for it's BIOS ROM.  There are sixteen memory locations
that may be selected from.  Under normal circumstances, select
(Segment CA00)."

nameditem
        Prompt  "DMA Arbitration Level"
          Choice  "Level 6" pos[0]=0110xxxxb arb 6
          Choice  "Level 7" pos[0]=0111xxxxb arb 7
          Choice  "Level 5" pos[0]=0101xxxxb arb 5
          Choice  "Level 0" pos[0]=0000xxxxb arb 0
          Choice  "Level 1" pos[0]=0001xxxxb arb 1
          Choice  "Level 3" pos[0]=0011xxxxb arb 3
          Choice  "Level 4" pos[0]=0100xxxxb arb 4
        Help
"Select the DMA channel the adapter will use to transfer data.
Under normal circumstances, select (Level 6)."

nameditem
        Prompt  "Select Interrupt Line"
          Choice  "Interrupt 5 (Reserved)"         pos[1]=x000xxxxb int 5
          Choice  "Interrupt 3 (Serial Alternate)" pos[1]=x001xxxxb int 3
          Choice  "Interrupt 10 (Reserved)"        pos[1]=x010xxxxb int 10
          Choice  "Interrupt 11 (Reserved)"        pos[1]=x011xxxxb int 11
          Choice  "Interrupt 12 (Mouse)"           pos[1]=x100xxxxb int 12
          Choice  "Interrupt 14 (Fixed Disk)"      pos[1]=x110xxxxb int 14
          Choice  "Interrupt 15 (Reserved)"        pos[1]=x111xxxxb int 15
        Help
"Select the interrupt to be used by the SCSI controller.  The
system interrupt assignment is given in parenthesis to help in a
selection that will not interfere with other equipment installed in
your PS2 system.  Under normal circumstances, select (Int 5)."

nameditem
        Prompt "Use Front Panel Disk Busy Light"
          Choice  "Use Front Panel Light"   pos[0]=xxxxxx1xb
          Choice  "Do Not Use Panel Light"  pos[0]=xxxxxx0xb
        Help
"Select whether the front panel light is to be used by the SCSI
devices to indicate that a SCSI device is busy.  The same light
is also used by the internally installed hard drive.  There is
no conflict if the same light is used by both devices."

nameditem
         Prompt "Use Microchannel Wait (IBM Model 80)"
           Choice  "Use Wait State (Model 80)"  pos[1]=1xxxxxxxb
           Choice  "Do Not Use Wait State"      pos[1]=0xxxxxxxb
         Help
"Select the extended synchronous bus cycle is to be used as the
default fastest cycle on the transfer of DMA data to the SCSI
device.  The Model 80 will not support full speed DMA writes
via the uChannel bus, so this option is required for high speed
devices on the Model 80."

