AdapterId 07002h

AdapterName  "AST ADVANTAGE/2 With Serial & Parallel Port Option"

NumBytes 4

NamedItem
     Prompt "WAIT STATE"
      choice "1 wait state " pos[1]=0XXXXXXXb
      choice "0 wait state " pos[1]=1XXXXXXXb
   Help
 "MEMORY WAIT STATE SELECTION"

NamedItem
	Prompt "MEMORY CONFIGURATION"
      choice "DISABLED"   pos[0]=0000000Xb
      choice ".5M,0K,0K,0K    TOTAL = 0.5 MB" pos[0]=0001XX1Xb
      choice " 2M,0K,0K,0K    TOTAL = 2.0 MB" pos[0]=0010XX1Xb
      choice ".5M,.5M,0K,0K   TOTAL = 1.0 MB" pos[0]=0011XX1Xb
      choice ".5M,2M,0K,0K    TOTAL = 2.5 MB" pos[0]=0100XX1Xb
      choice " 2M,2M,0K,0K    TOTAL = 4.0 MB" pos[0]=0101XX1Xb
      choice ".5M,.5M,.5M,0K  TOTAL = 1.5 MB" pos[0]=0110XX1Xb
      choice ".5M,.5M,2M,0K   TOTAL = 3.0 MB" pos[0]=0111XX1Xb
      choice ".5M,2M,2M,0K    TOTAL = 4.5 MB" pos[0]=1000XX1Xb
      choice " 2M,2M,2M,0K    TOTAL = 6.0 MB" pos[0]=1001XX1Xb
      choice ".5M,.5M,.5M,.5M TOTAL = 2.0 MB" pos[0]=1010XX1Xb
      choice ".5M,.5M,.5M,2M  TOTAL = 3.5 MB" pos[0]=1011XX1Xb
      choice ".5M,.5M,2M,2M   TOTAL = 5.0 MB" pos[0]=1100XX1Xb
      choice ".5M,2M,2M,2M    TOTAL = 6.5 MB" pos[0]=1101XX1Xb
      choice " 2M,2M,2M,2M    TOTAL = 8.0 MB" pos[0]=1110XX1Xb
   Help
"This is memory configuration on your ADVANTAGE/2
starting from top of the board BANK0,BANK1,BANK2,BANK3"

NamedItem
     Prompt "Connector 1"
      choice "SERIAL_1" 
                       pos[2]=xxxx000xb 
                       pos[3]=xxx1xxxxb
                       io 03f8h-03ffh int 4
      choice "SERIAL_2" 
                       pos[2]=xxxx001xb
                       pos[3]=xxx1xxxxb 
                       io 02f8h-02ffh int 3
      choice "SERIAL_3" 
                       pos[2]=xxxx010xb 
                       pos[3]=xxx1xxxxb
                       io 3220h-3227h int 3
      choice "SERIAL_4" 
                       pos[2]=xxxx011xb 
                       pos[3]=xxx1xxxxb
                       io 3228h-322fh int 3
      choice "SERIAL_5" 
                       pos[2]=xxxx100xb 
                       pos[3]=xxx1xxxxb
                       io 4220h-4227h int 3
      choice "SERIAL_6" 
                       pos[2]=xxxx101xb 
                       pos[3]=xxx1xxxxb
                       io 4228h-422fh int 3
      choice "SERIAL_7" 
                       pos[2]=xxxx110xb 
                       pos[3]=xxx1xxxxb
                       io 5220h-5227h int 3
      choice "SERIAL_8" 
                       pos[2]=xxxx111xb 
                       pos[3]=xxx1xxxxb
                       io 5228h-522fh int 3 
      choice "DISABLE" 
                       pos[3]=xxx0xxxxb
   Help
      "Connector 1 of  Advantage/2 Serial  and  Parallel Port
      Option can have  any one of the  Serial 1  to  Serial 8 
      assignments  and  can  also  be  disabled.  Use the F5=
      Previous and the F6=Next keys to change the Connector 1
      Serial port assignments  when  you  are  in the 'Change
      Configuration'  window.   Conflicting  assignments  are  
      marked with an Asterisk and should be changed."	

NamedItem
   Prompt "Connector 2"
        choice "PARALLEL_1" pos[0]=xxxx01xxb io 03bch-03bfh int 7
        choice "PARALLEL_2" pos[0]=xxxx10xxb io 0378h-037fh int 7
	choice "PARALLEL_3" pos[0]=xxxx11xxb io 0278h-027fh int 7
        choice "DISABLE"    pos[0]=xxxx00xxb 
   Help
      "Connector 2  of the  Advantage/2  Serial  and Parallel 
      Port Option can  have  any  one  of  the  Parallel 1 to 
      Parallel 3 assignments and can  also  be disabled.  Use  
      the  F5=Previous  and  the F6=Next  keys  to change the 
      Connector 2 Parallel Port  assignments  when you are in
      the 'Change Configuration' window.   Conflicting assig-
      nments  are  marked  with  an  Asterisk  and  should be 
      changed."
