
AdapterID 06E7Dh

AdapterName  "DCA Smart Alec 5250/90"

NumBytes 1

fixedresources
        pos[0]=11XXXXXXb

nameditem
        Prompt  "I/O Base Address"
          Choice "228 (Hex)"
            pos[0]=XXXX001Xb
            io 228h-22fh
          Choice "230 (Hex)"
            pos[0]=XXXX010Xb
            io 230h-237h
          Choice "238 (Hex)"
            pos[0]=XXXX011Xb
            io 238h-23fh
          Choice "240 (Hex)"
            pos[0]=XXXX100Xb
            io 240h-247h
          Choice "248 (Hex)"
            pos[0]=XXXX101Xb
            io 248h-24fh
          Choice "250 (Hex)"
            pos[0]=XXXX110Xb
            io 250h-257h
          Choice "258 (Hex)"
            pos[0]=XXXX111Xb
            io 258h-25fh
        Help
        "To configure this adapter you must choose the base address for the 
         I/O ports used by the adapter.  There are seven base addresses which
         can be selected.  Under normal circumstances, select <228 (Hex)>."

nameditem
        Prompt  "Interrupt Level"
          Choice "Level 11"
            pos[0]=XX01XXXXb
            int 0bh
          Choice "Level 10"
            pos[0]=XX11XXXXb
            int 0ah
        Help
        "To configure this adapter you must choose the interrupt level to be
         used by the adapter.  There are two interrupt levels which can be
         selected.  Under normal circumstances, select <Level 10>."


