AdapterId       07A7Ah

AdapterName "Boca Research BOCARAM/2 PLUS Memory Expansion Board"

NumBytes        2

NamedItem

Prompt "Memory On BOCARAM/2 PLUS"

choice " 2M (2 SIMM modules) " pos[0]=XXXX001Xb
choice " 4M (4 SIMM modules) " pos[0]=XXXX011Xb
choice " 8M (8 SIMM modules) " pos[0]=XXXX101Xb

Help
"  This card may be configured as either a 2,4 or 8 Mbyte memory
expansion unit.  If only one bank (Bank 0) of SIMMs is installed
then the unit should be configured as a 2Mbyte add-on.  If 2
banks (Banks 0 and 1) have been installed then it should be
configured as a 4M board.  If the board is entirely populated
(Banks 0,1,2 and 3), then choose the 8M option."

NamedItem

Prompt "Starting Address"

choice " 1Meg plus 256K (1280K)"   pos[1]=11101011b MEM 0140000H - 053FFFFH
choice " 1Meg plus 384K (1408K)"   pos[1]=11101001b MEM 0160000H - 055FFFFH
choice " 1Meg plus 512K (1536K)"   pos[1]=11100111b MEM 0180000H - 057FFFFH
choice " 1Meg plus 640K (1664K)"   pos[1]=11100101b MEM 01A0000H - 059FFFFH
choice " 1Meg plus 768K (1792K)"   pos[1]=11100011b MEM 01C0000H - 05BFFFFH
choice " 1Meg plus 896K (1920K)"   pos[1]=11100001b MEM 01E0000H - 05DFFFFH
choice " 2Meg (2048K)"             pos[1]=11011111b MEM 0200000H - 05FFFFFH
choice " 2Meg plus 128K (2176K)"   pos[1]=11011101b MEM 0220000H - 061FFFFH
choice " 2Meg plus 256K (2304K)"   pos[1]=11011011b MEM 0240000H - 063FFFFH
choice " 2Meg plus 384K (2432K)"   pos[1]=11011001b MEM 0260000H - 065FFFFH
choice " 2Meg plus 512K (2560K)"   pos[1]=11010111b MEM 0280000H - 067FFFFH
choice " 2Meg plus 640K (2688K)"   pos[1]=11010101b MEM 02A0000H - 069FFFFH
choice " 2Meg plus 768K (2816K)"   pos[1]=11010011b MEM 02C0000H - 06BFFFFH
choice " 2Meg plus 896K (2944K)"   pos[1]=11010001b MEM 02E0000H - 06DFFFFH
choice " 3Meg (3072K)"             pos[1]=11001111b MEM 0300000H - 06FFFFFH
choice " 3Meg plus 128K (3200K)"   pos[1]=11001101b MEM 0320000H - 071FFFFH
choice " 3Meg plus 256K (3328K)"   pos[1]=11001011b MEM 0340000H - 073FFFFH
choice " 3Meg plus 384K (3456K)"   pos[1]=11001001b MEM 0360000H - 075FFFFH
choice " 3Meg plus 512K (3584K)"   pos[1]=11000111b MEM 0380000H - 077FFFFH
choice " 3Meg plus 640K (3712K)"   pos[1]=11000101b MEM 03A0000H - 079FFFFH
choice " 3Meg plus 768K (3840K)"   pos[1]=11000011b MEM 03C0000H - 07BFFFFH
choice " 3Meg plus 896K (3968K)"   pos[1]=11000001b MEM 03E0000H - 07DFFFFH
choice " 4Meg (4096K)"             pos[1]=10111111b MEM 0400000H - 07FFFFFH
choice " 4Meg plus 128K (4224K)"   pos[1]=10111101b MEM 0420000H - 081FFFFH
choice " 4Meg plus 256K (4352K)"   pos[1]=10111011b MEM 0440000H - 083FFFFH
choice " 4Meg plus 384K (4480K)"   pos[1]=10111001b MEM 0460000H - 085FFFFH
choice " 4Meg plus 512K (4608K)"   pos[1]=10110111b MEM 0480000H - 087FFFFH
choice " 4Meg plus 640K (4736K)"   pos[1]=10110101b MEM 04A0000H - 089FFFFH
choice " 4Meg plus 768K (4864K)"   pos[1]=10110011b MEM 04C0000H - 08BFFFFH
choice " 4Meg plus 896K (4992K)"   pos[1]=10110001b MEM 04E0000H - 08DFFFFH
choice " 5Meg (5120K)"             pos[1]=10101111b MEM 0500000H - 08FFFFFH
choice " 5Meg plus 128K (5248K)"   pos[1]=10101101b MEM 0520000H - 091FFFFH
choice " 5Meg plus 256K (5376K)"   pos[1]=10101011b MEM 0540000H - 093FFFFH
choice " 5Meg plus 384K (5504K)"   pos[1]=10101001b MEM 0560000H - 095FFFFH
choice " 5Meg plus 512K (5632K)"   pos[1]=10100111b MEM 0580000H - 097FFFFH
choice " 5Meg plus 640K (5760K)"   pos[1]=10100101b MEM 05A0000H - 099FFFFH
choice " 5Meg plus 768K (5888K)"   pos[1]=10100011b MEM 05C0000H - 09BFFFFH
choice " 5Meg plus 896K (6016K)"   pos[1]=10100001b MEM 05E0000H - 09DFFFFH
choice " 6Meg (6144K)"             pos[1]=10011111b MEM 0600000H - 09FFFFFH
choice " 6Meg plus 128K (6272K)"   pos[1]=10011101b MEM 0620000H - 0A1FFFFH
choice " 6Meg plus 256K (6400K)"   pos[1]=10011011b MEM 0640000H - 0A3FFFFH
choice " 6Meg plus 384K (6528K)"   pos[1]=10011001b MEM 0660000H - 0A5FFFFH
choice " 6Meg plus 512K (6656K)"   pos[1]=10010111b MEM 0680000H - 0A7FFFFH
choice " 6Meg plus 640K (6784K)"   pos[1]=10010101b MEM 06A0000H - 0A9FFFFH
choice " 6Meg plus 768K (6912K)"   pos[1]=10010011b MEM 06C0000H - 0ABFFFFH
choice " 6Meg plus 896K (7040K)"   pos[1]=10010001b MEM 06E0000H - 0ADFFFFH
choice " 7Meg (7168K)"             pos[1]=10001111b MEM 0700000H - 0AFFFFFH
choice " 7Meg plus 128K (7296K)"   pos[1]=10001101b MEM 0720000H - 0B1FFFFH
choice " 7Meg plus 256K (7424K)"   pos[1]=10001011b MEM 0740000H - 0B3FFFFH
choice " 7Meg plus 384K (7552K)"   pos[1]=10001001b MEM 0760000H - 0B5FFFFH
choice " 7Meg plus 512K (7680K)"   pos[1]=10000111b MEM 0780000H - 0B7FFFFH
choice " 7Meg plus 640K (7808K)"   pos[1]=10000101b MEM 07A0000H - 0B9FFFFH
choice " 7Meg plus 768K (7936K)"   pos[1]=10000011b MEM 07C0000H - 0BBFFFFH
choice " 7Meg plus 896K (8064K)"   pos[1]=10000001b MEM 07E0000H - 0BDFFFFH
choice " 8Meg (8192K)"             pos[1]=01111111b MEM 0800000H - 0BFFFFFH
choice " 8Meg plus 128K (8320K)"   pos[1]=01111101b MEM 0820000H - 0C1FFFFH
choice " 8Meg plus 256K (8448K)"   pos[1]=01111011b MEM 0840000H - 0C3FFFFH
choice " 8Meg plus 384K (8576K)"   pos[1]=01111001b MEM 0860000H - 0C5FFFFH
choice " 8Meg plus 512K (8704K)"   pos[1]=01110111b MEM 0880000H - 0C7FFFFH
choice " 8Meg plus 640K (8832K)"   pos[1]=01110101b MEM 08A0000H - 0C9FFFFH
choice " 8Meg plus 768K (8960K)"   pos[1]=01110011b MEM 08C0000H - 0CBFFFFH
choice " 8Meg plus 896K (9088K)"   pos[1]=01110001b MEM 08E0000H - 0CDFFFFH
choice " 9Meg (9216K)"             pos[1]=01101111b MEM 0900000H - 0CFFFFFH
choice " 9Meg plus 128K (9344K)"   pos[1]=01101101b MEM 0920000H - 0D1FFFFH
choice " 9Meg plus 256K (9472K)"   pos[1]=01101011b MEM 0940000H - 0D3FFFFH
choice " 9Meg plus 384K (9600K)"   pos[1]=01101001b MEM 0960000H - 0D5FFFFH
choice " 9Meg plus 512K (9728K)"   pos[1]=01100111b MEM 0980000H - 0D7FFFFH
choice " 9Meg plus 640K (9856K)"   pos[1]=01100101b MEM 09A0000H - 0D9FFFFH
choice " 9Meg plus 768K (9984K)"   pos[1]=01100011b MEM 09C0000H - 0DBFFFFH
choice " 9Meg plus 896K (10112K)"  pos[1]=01100001b MEM 09E0000H - 0DDFFFFH
choice "10Meg (10240K)"            pos[1]=01011111b MEM 0A00000H - 0DFFFFFH
choice "10Meg plus 128K (10368K)"  pos[1]=01011101b MEM 0A20000H - 0E1FFFFH
choice "10Meg plus 256K (10496K)"  pos[1]=01011011b MEM 0A40000H - 0E3FFFFH
choice "10Meg plus 384K (10624K)"  pos[1]=01011001b MEM 0A60000H - 0E5FFFFH
choice "10Meg plus 512K (10752K)"  pos[1]=01010111b MEM 0A80000H - 0E7FFFFH
choice "10Meg plus 640K (10880K)"  pos[1]=01010101b MEM 0AA0000H - 0E9FFFFH
choice "10Meg plus 768K (11008K)"  pos[1]=01010011b MEM 0AC0000H - 0EBFFFFH
choice "10Meg plus 896K (11136K)"  pos[1]=01010001b MEM 0AE0000H - 0EDFFFFH
choice "11Meg (11264K)"            pos[1]=01001111b MEM 0B00000H - 0EFFFFFH
choice "11Meg plus 128K (11392K)"  pos[1]=01001101b MEM 0B20000H - 0F1FFFFH
choice "11Meg plus 256K (11520K)"  pos[1]=01001011b MEM 0B40000H - 0F3FFFFH
choice "11Meg plus 384K (11648K)"  pos[1]=01001001b MEM 0B60000H - 0F5FFFFH
choice "11Meg plus 512K (11776K)"  pos[1]=01000111b MEM 0B80000H - 0F7FFFFH
choice "11Meg plus 640K (11904K)"  pos[1]=01000101b MEM 0BA0000H - 0F7FFFFH
choice "11Meg plus 768K (12032K)"  pos[1]=01000011b MEM 0BC0000H - 0F7FFFFH
choice "11Meg plus 896K (12160K)"  pos[1]=01000001b MEM 0BE0000H - 0F7FFFFH
choice "12Meg (12288K)"            pos[1]=00111111b MEM 0C00000H - 0F7FFFFH
choice "12Meg plus 128K (12416K)"  pos[1]=00111101b MEM 0C20000H - 0F7FFFFH
choice "12Meg plus 256K (12544K)"  pos[1]=00111011b MEM 0C40000H - 0F7FFFFH
choice "12Meg plus 384K (12672K)"  pos[1]=00111001b MEM 0C60000H - 0F7FFFFH
choice "12Meg plus 512K (12800K)"  pos[1]=00110111b MEM 0C80000H - 0F7FFFFH
choice "12Meg plus 640K (12928K)"  pos[1]=00110101b MEM 0CA0000H - 0F7FFFFH
choice "12Meg plus 768K (13056K)"  pos[1]=00110011b MEM 0CC0000H - 0F7FFFFH
choice "12Meg plus 896K (13184K)"  pos[1]=00110001b MEM 0CE0000H - 0F7FFFFH
choice "13Meg (13312K)"            pos[1]=00101111b MEM 0D00000H - 0F7FFFFH
choice "13Meg plus 128K (13440K)"  pos[1]=00101101b MEM 0D20000H - 0F7FFFFH
choice "13Meg plus 256K (13568K)"  pos[1]=00101011b MEM 0D40000H - 0F7FFFFH
choice "13Meg plus 384K (13696K)"  pos[1]=00101001b MEM 0D60000H - 0F7FFFFH
choice "13Meg plus 512K (13824K)"  pos[1]=00100111b MEM 0D80000H - 0F7FFFFH
choice "13Meg plus 640K (13952K)"  pos[1]=00100101b MEM 0DA0000H - 0F7FFFFH
choice "13Meg plus 768K (14080K)"  pos[1]=00100011b MEM 0DC0000H - 0F7FFFFH
choice "13Meg plus 896K (14208K)"  pos[1]=00100001b MEM 0DE0000H - 0F7FFFFH
choice "14Meg (14336K)"            pos[1]=00011111b MEM 0E00000H - 0F7FFFFH
choice "14Meg plus 128K (14464K)"  pos[1]=00011101b MEM 0E20000H - 0F7FFFFH
choice "14Meg plus 256K (14592K)"  pos[1]=00011011b MEM 0E40000H - 0F7FFFFH
choice "14Meg plus 384K (14720K)"  pos[1]=00011001b MEM 0E60000H - 0F7FFFFH
choice "14Meg plus 512K (14848K)"  pos[1]=00010111b MEM 0E80000H - 0F7FFFFH


Help
" Use the F5 and F6 keys to toggle through the addresses (an
asterisk denotes a conflict). Note however, the Set Configuration
should have chosen the proper default values."
