
;
; IBM IEEE 488 Adapter/A Description File
;
; Version:	1.00
;
; (C) Copyright International Business Machines Corporation 1988
; All rights reserved.
;


       AdapterID 0DF3Fh

       AdapterName "IEEE-488 ADAPTER"

       NumBytes 2

       FixedResources
       pos[3]=xxx00100b

       NamedItem
       Prompt "Adapter No."
       choice "Adapter 1"  pos[0]=XXXXXX0Xb  io  09c0h-09cfh
       choice "Adapter 2"  pos[0]=XXXXXX1Xb  io  09d0h-09dfh
       help
       "To configure this adapter you must choose the port
       address. There are two addresses that can be selected.
       <Adapter 1> is preferred, but the adapter can operate
       on any of the two addresses.
       Use the F5=Previous and F6=Next keys to change this
       assignment. Conflicting assignments are marked with
       an asterisk and must be changed."


       NamedItem
       Prompt "Interrupt Level"
       choice "Level 3"  pos[0]=XXXX00XXb   int  3
       choice "Level 7"  pos[0]=XXXX01XXb   int  7
       choice "Level 10"  pos[0]=XXXX10XXb   int 10
       choice "Level 11"  pos[0]=XXXX11XXb   int 11
       help

       "To configure this adapter you must choose the
       interrupt level. There are four levels that can be
       selected. <Level 3> is preferred, but the adapter
       can operate on any of the four levels.
       Use the F5=Previous and F6=Next keys to change this
       assignment. Conflicting assignments are marked with
       an asterisk and must be changed."


       NamedItem
       Prompt "DMA ARB LEVEL"
       choice "Level 7"  pos[0]=0111XXXXb   arb 7
       choice "Level 1"  pos[0]=0001XXXXb   arb 1
       choice "Level 3"  pos[0]=0011XXXXb   arb 3
       choice "Level 5"  pos[0]=0101XXXXb   arb 5
       choice "Level 4"  pos[0]=0100XXXXb   arb 4
       choice "Level 0"  pos[0]=0000XXXXb   arb 0
       help
       "To configure this adapter you must choose the DMA
       channel for the data transmission. There are six
       levels that can be selected. <Level 7> is preferred,
       but the adapter can operate on any of the six levels.
       Use the F5=Previous and F6=Next keys to change this
       assignment. Conflicting assignments are marked with
       an asterisk and must be changed."

