;
;	$Revision:   1.4  $
;	$Date:   23 Sep 1988 13:14:44  $
;
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  This program           *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;***************************************************************************
; @0021.ADF
; This file contains the end-user features for the C&T250 chipset.
; Its appended to the end of the @0000.ADF.

;******************************************************************
; CMOS 7ah - BIOS information.
;          bit 0 = Shadow BIOS ROM
;          bit 1 = Enable Bad Block Remap
;          bit 2 = Enable Dynamic Memory Determination
;          bit 3 = Reserved
;          bit 4 = Reserved
;          bit 5 = Reserved
;          bit 6 = Reserved
;          bit 7 = Reserved
; CMOS 7bh - Shadow Adapter ROMs:
;          00 = No shadow
;          FF = Shadow
;******************************************************************
NamedItem
        Cmos 7ah
	Prompt "Phoenix BIOS ROM shadowing"
	Choice "Disabled" pos[0]=XXXXXXX0b
	Choice "Enabled"  pos[0]=XXXXXXX1b
	Help
"If BIOS ROM shadowing is enabled, the Phoenix ROM BIOS will attempt to
execute from a copy of itself in RAM. Since the RAM is faster than ROM,
programs that use BIOS functions will subsequently execute faster. If you
have less than 1 Megabyte (1024 KB) of memory, shadowing cannot be enabled."

NamedItem
        Cmos 7bh
	Prompt "Adapter ROM shadowing"
	Choice "Disabled" pos[0]=00000000b
	Choice "Enabled"  pos[0]=11111111b
	Help
"If Adapter ROM shadowing is enabled, and the Adapter board permits shadowing
to occur, the Phoenix BIOS will copy the Adapter ROM into faster RAM. This
will result in faster execution of the programs on the Adapter boards. If you
have less than 1 Megabyte (1024 KB) of memory, shadowing cannot be enabled."

NamedItem
        Cmos 7ah
	Prompt "Bad Memory Block Remapping"
	Choice "Disabled" pos[0]=XXXXXX0Xb
	Choice "Enabled"  pos[0]=XXXXXX1Xb
	Help
"If Bad Block Remapping is enabled then the ROM BIOS will attempt to relocate
good memory into memory that fails parity checks. This will permit all the
good memory to be sequentially addressable and the failing memory will be 
disabled. If this feature is disabled then memory will not be available
beyond the first failing memory block." 
