
AdapterId 08FDBh

AdapterName "XGA Video Adapter"

NumBytes 4

FixedResources
        pos[1]=0XXXXXX0b
        pos[3]=1100XXXXb exec

address 32

Begin Device 03h 02h 00h NoDMA

NamedItem Prompt "Video I/O Address"
        choice "Instance 6: 2160h - 216Fh"
                pos[0]=XXXX110Xb io 02160h-0216fh
;       choice "Instance 7: 2170h - 217Fh"
;               pos[0]=XXXX111Xb io 02170h-0217fh
;       choice "Instance 0: 2100h - 210Fh"
;               pos[0]=XXXX000Xb io 02100h-0210fh
        choice "Instance 1: 2110h - 211Fh"
                pos[0]=XXXX001Xb io 02110h-0211fh
        choice "Instance 2: 2120h - 212Fh"
                pos[0]=XXXX010Xb io 02120h-0212fh
        choice "Instance 3: 2130h - 213Fh"
                pos[0]=XXXX011Xb io 02130h-0213fh
        choice "Instance 4: 2140h - 214Fh"
                pos[0]=XXXX100Xb io 02140h-0214fh
        choice "Instance 5: 2150h - 215Fh"
                pos[0]=XXXX101Xb io 02150h-0215fh

        Help
        "The Video I/O address selects a particular I/O address range for the
         Display Controller Registers. This field also affects the exact
         location of the video coprocessor registers."

NamedItem Prompt "Video Arbitration Level"
        choice "Arbitration level 13" pos[1]=X1101XXXb arb 0dh
        choice "Arbitration level 12" pos[1]=X1100XXXb arb 0ch
        choice "Arbitration level 11" pos[1]=X1011XXXb arb 0bh
        choice "Arbitration level 10" pos[1]=X1010XXXb arb 0ah
        choice "Arbitration level  9" pos[1]=X1001XXXb arb 9
        choice "Arbitration level  8" pos[1]=X1000XXXb arb 8
        choice "Arbitration level 14" pos[1]=X1110XXXb arb 0eh

        Help
        "The video sub-system can be assigned any one of the
        available arbitration levels 8 through 14. Use the
        F5=Previous and the F6=Next keys to change arbitration
        level assignments if you are in the 'Change configuration'
        window.  Conflicting assignments are marked with an asterisk
        and should be changed."

NamedItem Prompt "Video Fairness"
        choice "Fairness On"  pos[1]=XXXXX1XXb
        choice "Fairness Off" pos[1]=XXXXX0XXb

        Help
        "Video Fairness indicates whether or not the video
        sub-system coprocessor will follow the fairness algorithm
        for bus usage. This setting can be changed if you are in
        the 'Change Configuration' window by using the
        F5=Previous and F6=Next keys."

End
