
AdapterId 06eddh

AdapterName  "U.S. Robotics Courier PS/2 Modem"

NumBytes 2

NamedItem
        Prompt "Serial(COM) Address"
      choice "SERIAL_1"  pos[0]=XXX0000Xb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=XXX0001Xb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=XXX0010Xb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=XXX0011Xb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=XXX0100Xb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=XXX0101Xb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=XXX0110Xb  io 5220h-5227h  int 3
      choice "SERIAL_8"  pos[0]=XXX0111Xb  io 5228h-522fh  int 3
   Help
"The Courier Dual Standard can be assigned to use Serial 1
through Serial 8.  Use the F5=Previous and the F6=Next keys
to change serial port assignments. Conflicting assignments 
are marked with an asterisk. Conflicts must be resolved to 
use the adapter."

NamedItem
	Prompt "Carrier Detect Operations"
     choice "CD on connect only" pos[0]=1xxxxxxxb
     choice "CD override" pos[0]=0xxxxxxxb
  Help
"Use this setting to specify normal CD operation:
courier sends CD signal when it connects with another
modem, drops CD on disconnect.  Using the CD override
setting choice assures that CD is always on.  Toggle
between the choices with the F5=Previous or F6=Next keys."

NamedItem
	Prompt "Data Terminal Ready Operations"
     choice "Normal DTR operation" pos[1]=x1xxxxxxb
     choice "DTR override" pos[1]=x0xxxxxxb
  Help
"Use this setting to specify normal DTR operation:
computer must provide DTR signal for modem to accept
commands; dropping DTR terminates a call.  Using the
DTR override setting choice assures that DTR is
always on.  Toggle between the choices with the
F5=Previous or F6=Next keys."

NamedItem
	Prompt "Auto Answer"
     choice "Answers on first ring" pos[1]=xxxxx1xxb
     choice "Disabled" pos[1]=xxxxx0xxb
  Help
"Use this setting to specify whether the modem       
auto answer is enabled or disabled.  Toggle
between the choices with the F5=Previous or F6=Next keys."

NamedItem
	Prompt "Command Mode Local Echo"
     choice "Keyboard commands displayed" pos[1]=xxxxxx1xb
     choice "Echo suppressed" pos[1]=xxxxxx0xb
  Help
"Use this setting to specify whether the modem       
local echo is enabled or suppressed.  Toggle
between the choices with the F5=Previous or F6=Next keys."

NamedItem
	Prompt "Result Codes"
     choice "Disabled" pos[1]=xxxxxxx1b
     choice "Enabled" pos[1]=xxxxxxx0b
  Help
"Use this setting to specify whether the modem       
display result codes or suppresses them.  Toggle
between the choices with the F5=Previous or F6=Next keys."

NamedItem
	Prompt "Verbal/Numeric Result Codes"
     choice "Verbal (word) results" pos[0]=x1xxxxxxb
     choice "Numeric results" pos[0]=x0xxxxxxb
  Help
"Use this setting to specify whether the modem uses  
verbal or numeric result codes.  Toggle between the
choices with the F5=Previous or F6=Next keys."

NamedItem
	Prompt "Auxiliary, Result Codes"
     choice "Results in orig & ans mode" pos[1]=1xxxxxxxb
     choice "Results in ans mode disabled" pos[1]=0xxxxxxxb
  Help
"Use this setting to specify whether the modem       
displays result codes in originate and answer mode or 
originate mode only.  Toggle between the choices with
the F5=Previous or F6=Next keys."

NamedItem
	Prompt "Power-on Defaults"
     choice "Boot NVRAM defaults" pos[1]=xx1xxxxxb
     choice "Boot factory defaults" pos[1]=xx0xxxxxb
  Help
"Use this setting to specify whether the modem uses its 
internal non-volatile memory to initialize its settings
on power-up. Using the FACTORY SETTINGS choice assures 
that the modem is always initialized to known settings,
regardless of previous use. Toggle between the choices
with the F5=Previous or F6=Next keys."

NamedItem
	Prompt "AT Command Recognition"
     choice "Disabled (Dumb modem)" pos[1]=xxxx1xxxb
     choice "Enabled (Smart modem)" pos[1]=xxxx0xxxb
  Help
"Use this setting to enable or disable the modem's command set.
When set to 'DUMB', the modem cannot originate calls, but will
answer the phone. This could be useful for applications needing 
restricted access to the phone lines. Toggle between the choices
with the F5=Previous or F6=Next keys."

NamedItem
	Prompt "Escape Code (+++) Response"
     choice "Hangs up" pos[1]=xxx1xxxxb
     choice "Maintains connection" pos[1]=xxx0xxxxb
  Help
"Use this setting to specify whether the modem escape
code response hangs up or maintains a connection.  Toggle
between the choices with the F5=Previous or F6=Next keys."





