AdapterID 05500h

AdapterName "COREtape Controller"

NumBytes 2

NamedItem
Prompt	"I/O Port Address Range"
choice	"Primary 300h-30fh"     pos[1]=00110000b io 0300h-030fh
choice	"Alternate 280h-28fh"   pos[1]=00101000b io 0280h-028fh
choice	"Alternate 290h-29fh"   pos[1]=00101001b io 0290h-029fh
choice	"Alternate 2a0h-2afh"   pos[1]=00101010b io 02a0h-02afh
choice	"Alternate 310h-31fh"   pos[1]=00110001b io 0310h-031fh
choice	"Alternate 320h-32fh"   pos[1]=00110010b io 0320h-032fh
Help
"Use the F5 (previous) or F6 (next) keys to select the primary or alternate
port address range.  Conflicting assignments are marked with an asterisk and
must be changed."

NamedItem
Prompt	"Arbitration Level/DMA Channel"
choice	"DMA 1"         pos[0]=XXXXX01Xb        arb 1
choice	"DMA 3"         pos[0]=XXXXX11Xb        arb 3
choice	"DMA 2"         pos[0]=XXXXX10Xb        arb 2
choice	"DMA 0"         pos[0]=XXXXX00Xb        arb 0
Help
"Use the F5 (previous) or F6 (next) keys to select the DMA channel/arbitration
level.	Conflicting assignments are marked with an asterisk and must be changed."

NamedItem
Prompt	"Interrupt Channel"
choice	"IRQ 3"         pos[0]=XX011XXXb        int 3
choice	"IRQ 4"         pos[0]=XX100XXXb        int 4
choice	"IRQ 5"         pos[0]=XX101XXXb        int 5
choice	"IRQ 6"         pos[0]=XX110XXXb        int 6
choice	"IRQ 7"         pos[0]=XX111XXXb        int 7
choice	"IRQ 9"         pos[0]=XX000XXXb        int 9
choice	"IRQ 10"        pos[0]=XX001XXXb        int 10
choice	"IRQ 11"        pos[0]=XX010XXXb        int 11
Help
"Use the F5 (previous) or F6 (next) keys to select the primary or alternate
interrupt channel.  Conflicting assignments are marked with an asterisk and
must be changed."

NamedItem
Prompt	"Parity Select"
choice	"Parity disable"        pos[0]=X1XXXXXXb
choice	"Parity enable"         pos[0]=X0XXXXXXb
Help
"Use the F5 (previous) or F6 (next) keys to select or deselect the parity
feature."
