;
;  ADF file for CDI-210H CD-ROM Controller (Hitachi drives)
;

AdapterID 05025h

AdapterName  "Online CDI-210H (Hitachi) CD-ROM Controller"

NumBytes 2

nameditem
 Prompt  "I/O Address"
  Choice  "4580h-4583h"    pos[0]=011100XXb    io 4580h-4583h
  Choice  "4400h-4403h"    pos[0]=010000XXb    io 4400h-4403h
  Choice  "4500h-4503h"    pos[0]=011000XXb    io 4500h-4503h
  Choice  "45C0h-45C3h"    pos[0]=011110XXb    io 45C0h-45C3h
  Choice  "8400h-8403h"    pos[0]=110000XXb    io 8400h-8403h
  Choice  "8500h-8503h"    pos[0]=111000XXb    io 8500h-8503h
  Choice  "8580h-8583h"    pos[0]=111100XXb    io 8580h-8583h
  Choice  "85C0h-85C3h"    pos[0]=111110XXb    io 85C0h-85C3h
 Help
  "This selects the I/O address the adapter will use.
   Under normal circumstances, select <4580-4583>.
   Use the F5=Previous and the F6=Next keys to change
   this assignment. Conflicting assignments are marked
   with an asterisk and must be changed."

nameditem
 Prompt  "DMA Arbitration Level"
  Choice  "Level 5"    pos[1]=XXXX0101b    arb 5
  Choice  "Level 6"    pos[1]=XXXX0110b    arb 6
  Choice  "Level 7"    pos[1]=XXXX0111b    arb 7
  Choice  "Level 0"    pos[1]=XXXX0000b    arb 0
  Choice  "Level 1"    pos[1]=XXXX0001b    arb 1
  Choice  "Level 2"    pos[1]=XXXX0010b    arb 2
  Choice  "Level 3"    pos[1]=XXXX0011b    arb 3
  Choice  "Level 4"    pos[1]=XXXX0100b    arb 4
 Help
  "This selects the DMA channel the adapter will use to transfer
   data. Under normal circumstances, select <Level 5>.
   Use the F5=Previous and the F6=Next keys to change
   this assignment. Conflicting assignments are marked
   with an asterisk and must be changed."

nameditem
 Prompt  "Interrupt Level"
  Choice  "Level 15"   pos[1]=1111XXXXb    int 15
  Choice  "Level 11"   pos[1]=1011XXXXb    int 11
  Choice  "Level 10"   pos[1]=1010XXXXb    int 10
  Choice  "Level  5"   pos[1]=0101XXXXb    int  5
  Choice  "Level 12"   pos[1]=1100XXXXb    int 12
  Choice  "Level  9"   pos[1]=1001XXXXb    int  9
  Choice  "Level  7"   pos[1]=0111XXXXb    int  7
  Choice  "Level  3"   pos[1]=0011XXXXb    int  3
  Choice  "Level  4"   pos[1]=0100XXXXb    int  4
  Choice  "Level  6"   pos[1]=0110XXXXb    int  6
  Choice  "Level 14"   pos[1]=1110XXXXb    int 14
 Help
  "This selects the Interrupt Level the adapter will use.
   Under normal circumstances, select <Level 3>.
   Use the F5=Previous and the F6=Next keys to change
   this assignment. Conflicting assignments are marked
   with an asterisk and must be changed."

