;       Adapter Description File for Artist XJS MC
;
;       Artist Graphics
;       March 28, 1991
;       Version 1.1

AdapterId 080C3H

AdapterName "Artist Graphics - Artist XJS MC "

NumBytes 2

NamedItem

Prompt "I/O Address Range"

choice "Range 03EXh" pos[1]=00111110b io 03E0h-03EFh
choice "Range 02CXh" pos[1]=00101100b io 02C0h-02Cfh
choice "Range 02DXh" pos[1]=00101101b io 02D0h-02DFh
choice "Range 02EXh" pos[1]=00101110b io 02E0h-02EFh
choice "Range 06EXh" pos[1]=01101110b io 06E0h-06EFh
choice "Range 07EXh" pos[1]=01111110b io 07E0h-07EFh


Help

"This assignment need only be changed if it is in conflict
with another installed adapter.  Conflicting assignments are
marked with an asterisk and must be changed for proper adapter
operation.
Use the F5=Previous and the F6=Next keys to change the adapter's
I/O Address Range."

NamedItem

Prompt "Memory Address Range"

choice "Segment CC00" pos[1]=XXXXXXXXb mem 0CC000h-0CFFFFh
choice "Segment C000" pos[1]=XXXXXXXXb mem 0C0000h-0C3FFFh
choice "Segment C400" pos[1]=XXXXXXXXb mem 0C4000h-0C7FFFh
choice "Segment C800" pos[1]=XXXXXXXXb mem 0C8000h-0C8FFFh
choice "Segment D000" pos[1]=XXXXXXXXb mem 0D0000h-0D3FFFh
choice "Segment D400" pos[1]=XXXXXXXXb mem 0D4000h-0D4FFFh
choice "Segment D800" pos[1]=XXXXXXXXb mem 0D8000h-0D8FFFh
choice "Segment DC00" pos[1]=XXXXXXXXb mem 0DC000h-0DFFFFh

Help
"The base address should only be changed if there is a conflict with
another installed adapter. A default address of 0xCC00 is recommended.
This 16Kbyte block in PC memory maps to two 8Kbyte windows in the
34020 memory space. These 8 Kbyte windows can each be mapped to start
at any 8 Kbyte boundary in the 34020 memory space.

This ADF file allows the user to select the memory segment that will be used
for the XJS MC. The selection of the proper segment allows the computer
to check for any possible memory conflicts. It should be noted
that the programmer must also declare the proper memory segment by
programming the memory mapping I/O registers on the XJS MC.

Use the F5=Previous and the F6=Next keys to change the adapters memory address
range. "



NamedItem

Prompt "Interrupt Request Option"

choice "No Interrupts   " pos[0]=XXXXXXXXb
choice "Interrupt -IRQ10" pos[0]=0XXXXXXXb int 10
choice "Interrupt -IRQ11" pos[0]=1XXXXXXXb int 11

Help
"This graphics controller can be configured to send either hardware
interrupt IRQ10 OR IRQ11 from the 34020 Graphics Processor to the
microchannel bus. Theses interrupts can be either disabled or sent
to one of the three interupt request lines.
The default setting is for interupts disabled.
Use the F5=previous and the F6=Next keys to change the adapters
interupt selection."
