; CuRAM 2 Megabyte Expanded/Extended Memory Adapter
; Copyright (c) Cumulus Corporation 1987, 1988. All rights reserved

AdapterId 7020h

AdapterName "Cumulus 2 Meg Expanded/Extended Memory Multifunction Adapter V1.0"

Numbytes 3

NamedItem
	Prompt "Expanded Memory Auto Selected at Port" 
	choice " 208h "
		pos[2]=x0000001b
		io 208h - 20fh 4208h - 420fh 8208h - 820fh
	choice " 218h "
		pos[2]=x0000011b
		io 218h - 21fh 4218h - 421fh 8218h - 821fh
	choice " 228h "
 		pos[2]=x0000101b
  		io 228h - 22fh 4228h - 422fh 8228h - 822fh
	choice " 238h "
		pos[2]=x0000111b
		io 238h - 23fh 4238h - 423fh 8238h - 823fh
	choice " 248h "
 		pos[2]=x0001001b
  		io 248h - 24fh 4248h - 424fh 8248h - 824fh
	choice " 258h "
		pos[2]=x00001011b
		io 258h - 25fh 4258h - 425fh 8258h - 825fh
	choice " 268h "
		pos[2]=x0001101b
		io 268h - 26fh 4268h - 426fh 8268h - 826fh
	choice " 278h "
		pos[2]=x0001111b
		io 278h - 27fh 4278h - 427fh 8278h - 827fh
	choice " 288h "
		pos[2]=x0010000b
		io 288h - 28fh 4288h - 428fh 8288h - 828fh
	choice " 298h "
		pos[2]=x0010010b
		io 298h - 29fh 4298h - 429fh 8298h - 829fh
	choice " Disable I/O ports "
		pos[2]=x1xxxxxxb
	Help

	"The expanded memory port address is the I/O port address
	used to control expanded memory page mapping registers.
	[Disable I/O Ports] should only be selected if the entire
	CuRAM memory is configured as EXTENDED memory."



NamedItem

	Prompt "Extended Memory Enable"

	choice "2 Meg starting at 1,408 Kb"
		pos[3]=110010xxb
		mem 160000h - 35ffffh
	choice "2 Meg starting at 3,456 Kb"
		pos[3]=110011xxb
		mem 360000h - 55ffffh
	choice "No extended memory"
		pos[3]=111100xxb

	Help
	"Select the amount of CuRAM memory  to be reserved as
	extended memory (memory above 1 Megabyte) and its starting
	address. If you wish to use all CuRAM memory as expanded
	memory, select the [No extended memory] option."	 

NamedItem

	Prompt "Serial Port Enable "

	choice 	"Disable Serial Port"
		pos[0]=xxxxx0xxb

	choice "COM2 configuration"
		pos[0]=xxxx11xxb
		io 2f8h - 2ffh
		int 3	
	choice "COM1 configuration"
		pos[0]=xxxx01xxb
		io 3f8h - 3ffh
		int 4

	Help
	"If an optional Serial Communications Port is installed select 
	the desired COM port setting. Otherwise, please select the
	[Disable Serial Port] option"

NamedItem

	Prompt "Parallel Port Enable"

	choice "Disable parallel port"
		pos[0]=xxx0xxxxb

	choice "LPT2"
		pos[0]=1011xxxxb
		io 378h - 37bh
		int 7

	choice "LPT2 extended"
		pos[0]=0011xxxxb
		io 378h - 37bh
		int 7

	choice "LPT3"
		pos[0]=1101xxxxb
		io 278h - 27bh
		int 7

	choice "LPT3 extended"
		pos[0]=0101xxxxb
		io 278h - 27bh
		int 7

	choice "LPT1"
		pos[0]=1001xxxxb
		io 3BCh - 3BFh
		int 7

	choice "LPT1 extended"
		pos[0]=0001xxxxb
		io 3BCh - 3BFh
		int 7


	Help
	"If an optional Parallel Communications Port is installed select 
	the desired LPT port setting. Otherwise, please select the
	[Disable Parallel Port] option"
