;*****************************************************************************
;*                       Tiara Computer Systems, Inc.                        *
;*         2700 Garcia Avenue  Mountain View, California  94043              *
;*              LANcard/A-II ARCnet Adapter Configuration File               *
;*                     Part #70-00366-1000     ECO #129                      *
;*                                                                           *
;*   Revision History:                                                       *
;*   08/05/87 - File Creation                                                *
;*   09/09/87 - Fix network response time settings                           *
;*   09/23/87 - Add PROM disable selection                                   *
;*   09/28/87 - Pilot Pre-release                                            *
;*              Beef-up help files and change node ID from hex to decimal.   *
;*              Change default seetings so that auto-setup will configure    *
;*              the card as follows:                                         *
;*              a. Node ID = 000                                             *
;*              b. Boot Device = Removable Drive A                           *
;*              c. PROM = Disabled                                           *
;*              d. Network Response Time = 78us                              *
;*              e. Base I/O Port Address = 02E0h                             *
;*              f. Interrupt Request = IRQ2                                  *
;*              g. RIM Buffer Base Address = 0D000h                          *
;*   10/13/87 - Pilot Release                                                *
;*              Clarify Boot Device Sequence and Extended Timeout selections.*
;*              Continue scrubbing the help files so that they will be of    *
;*              assistance to the average user.                              *
;*   10/26/87 - Changed the sequence of named items to place the most        *
;*              often used first.  Also changed the automatic configuration  *
;*              to set the node id to 0 instead of 1                         *
;*   10/29/87 - Beta Release- ECO #120: Fix boot device select bug that      *
;*              would not enable the PROM!                                   * 
;*   11/25/87 - Production Release-ECO #134: Incorporate PROM enable/disable *
;*              with PROM offset select, get rid of boot device sequence     *
;*              select.                                                      * 
;*                                                                           *
;*   Source File: @605F.ADF                                                  *
;*   Engineer: William Karwacki - Hardware Engineering                       *
;*   Concurrance: Barry Rose - Technical Support                             *
;*                                                                           *
;*****************************************************************************

        adapterid 0605Fh

        adaptername "Tiara Computer Systems, Inc. LANcard/A-II ARCnet Adapter"

        numbytes 4

        nameditem
                prompt "Node Identification Select"
                        choice "Node Identification = 000"
                                pos[2]=00000000b
                        choice "Node Identification = 001"
                                pos[2]=00000001b
                        choice "Node Identification = 002"
                                pos[2]=00000010b
                        choice "Node Identification = 003"
                                pos[2]=00000011b
                        choice "Node Identification = 004"
                                pos[2]=00000100b
                        choice "Node Identification = 005"
                                pos[2]=00000101b
                        choice "Node Identification = 006"
                                pos[2]=00000110b
                        choice "Node Identification = 007"
                                pos[2]=00000111b
                        choice "Node Identification = 008"
                                pos[2]=00001000b
                        choice "Node Identification = 009"
                                pos[2]=00001001b
                        choice "Node Identification = 010"
                                pos[2]=00001010b
                        choice "Node Identification = 011"
                                pos[2]=00001011b
                        choice "Node Identification = 012"
                                pos[2]=00001100b
                        choice "Node Identification = 013"
                                pos[2]=00001101b
                        choice "Node Identification = 014"
                                pos[2]=00001110b
                        choice "Node Identification = 015"
                                pos[2]=00001111b
                        choice "Node Identification = 016"
                                pos[2]=00010000b
                        choice "Node Identification = 017"
                                pos[2]=00010001b
                        choice "Node Identification = 018"
                                pos[2]=00010010b
                        choice "Node Identification = 019"
                                pos[2]=00010011b
                        choice "Node Identification = 020"
                                pos[2]=00010100b
                        choice "Node Identification = 021"
                                pos[2]=00010101b
                        choice "Node Identification = 022"
                                pos[2]=00010110b
                        choice "Node Identification = 023"
                                pos[2]=00010111b
                        choice "Node Identification = 024"
                                pos[2]=00011000b
                        choice "Node Identification = 025"
                                pos[2]=00011001b
                        choice "Node Identification = 026"
                                pos[2]=00011010b
                        choice "Node Identification = 027"
                                pos[2]=00011011b
                        choice "Node Identification = 028"
                                pos[2]=00011100b
                        choice "Node Identification = 029"
                                pos[2]=00011101b
                        choice "Node Identification = 030"
                                pos[2]=00011110b
                        choice "Node Identification = 031"
                                pos[2]=00011111b
                        choice "Node Identification = 032"
                                pos[2]=00100000b
                        choice "Node Identification = 033"
                                pos[2]=00100001b
                        choice "Node Identification = 034"
                                pos[2]=00100010b
                        choice "Node Identification = 035"
                                pos[2]=00100011b
                        choice "Node Identification = 036"
                                pos[2]=00100100b
                        choice "Node Identification = 037"
                                pos[2]=00100101b
                        choice "Node Identification = 038"
                                pos[2]=00100110b
                        choice "Node Identification = 039"
                                pos[2]=00100111b
                        choice "Node Identification = 040"
                                pos[2]=00101000b
                        choice "Node Identification = 041"
                                pos[2]=00101001b
                        choice "Node Identification = 042"
                                pos[2]=00101010b
                        choice "Node Identification = 043"
                                pos[2]=00101011b
                        choice "Node Identification = 044"
                                pos[2]=00101100b
                        choice "Node Identification = 045"
                                pos[2]=00101101b
                        choice "Node Identification = 046"
                                pos[2]=00101110b
                        choice "Node Identification = 047"
                                pos[2]=00101111b
                        choice "Node Identification = 048"
                                pos[2]=00110000b
                        choice "Node Identification = 049"
                                pos[2]=00110001b
                        choice "Node Identification = 050"
                                pos[2]=00110010b
                        choice "Node Identification = 051"
                                pos[2]=00110011b
                        choice "Node Identification = 052"
                                pos[2]=00110100b
                        choice "Node Identification = 053"
                                pos[2]=00110101b
                        choice "Node Identification = 054"
                                pos[2]=00110110b
                        choice "Node Identification = 055"
                                pos[2]=00110111b
                        choice "Node Identification = 056"
                                pos[2]=00111000b
                        choice "Node Identification = 057"
                                pos[2]=00111001b
                        choice "Node Identification = 058"
                                pos[2]=00111010b
                        choice "Node Identification = 059"
                                pos[2]=00111011b
                        choice "Node Identification = 060"
                                pos[2]=00111100b
                        choice "Node Identification = 061"
                                pos[2]=00111101b
                        choice "Node Identification = 062"
                                pos[2]=00111110b
                        choice "Node Identification = 063"
                                pos[2]=00111111b
                        choice "Node Identification = 064"
                                pos[2]=01000000b
                        choice "Node Identification = 065"
                                pos[2]=01000001b
                        choice "Node Identification = 066"
                                pos[2]=01000010b
                        choice "Node Identification = 067"
                                pos[2]=01000011b
                        choice "Node Identification = 068"
                                pos[2]=01000100b
                        choice "Node Identification = 069"
                                pos[2]=01000101b
                        choice "Node Identification = 070"
                                pos[2]=01000110b
                        choice "Node Identification = 071"
                                pos[2]=01000111b
                        choice "Node Identification = 072"
                                pos[2]=01001000b
                        choice "Node Identification = 073"
                                pos[2]=01001001b
                        choice "Node Identification = 074"
                                pos[2]=01001010b
                        choice "Node Identification = 075"
                                pos[2]=01001011b
                        choice "Node Identification = 076"
                                pos[2]=01001100b
                        choice "Node Identification = 077"
                                pos[2]=01001101b
                        choice "Node Identification = 078"
                                pos[2]=01001110b
                        choice "Node Identification = 079"
                                pos[2]=01001111b
                        choice "Node Identification = 080"
                                pos[2]=01010000b
                        choice "Node Identification = 081"
                                pos[2]=01010001b
                        choice "Node Identification = 082"
                                pos[2]=01010010b
                        choice "Node Identification = 083"
                                pos[2]=01010011b
                        choice "Node Identification = 084"
                                pos[2]=01010100b
                        choice "Node Identification = 085"
                                pos[2]=01010101b
                        choice "Node Identification = 086"
                                pos[2]=01010110b
                        choice "Node Identification = 087"
                                pos[2]=01010111b
                        choice "Node Identification = 088"
                                pos[2]=01011000b
                        choice "Node Identification = 089"
                                pos[2]=01011001b
                        choice "Node Identification = 090"
                                pos[2]=01011010b
                        choice "Node Identification = 091"
                                pos[2]=01011011b
                        choice "Node Identification = 092"
                                pos[2]=01011100b
                        choice "Node Identification = 093"
                                pos[2]=01011101b
                        choice "Node Identification = 094"
                                pos[2]=01011110b
                        choice "Node Identification = 095"
                                pos[2]=01011111b
                        choice "Node Identification = 096"
                                pos[2]=01100000b
                        choice "Node Identification = 097"
                                pos[2]=01100001b
                        choice "Node Identification = 098"
                                pos[2]=01100010b
                        choice "Node Identification = 099"
                                pos[2]=01100011b
                        choice "Node Identification = 100"
                                pos[2]=01100100b
                        choice "Node Identification = 101"
                                pos[2]=01100101b
                        choice "Node Identification = 102"
                                pos[2]=01100110b
                        choice "Node Identification = 103"
                                pos[2]=01100111b
                        choice "Node Identification = 104"
                                pos[2]=01101000b
                        choice "Node Identification = 105"
                                pos[2]=01101001b
                        choice "Node Identification = 106"
                                pos[2]=01101010b
                        choice "Node Identification = 107"
                                pos[2]=01101011b
                        choice "Node Identification = 108"
                                pos[2]=01101100b
                        choice "Node Identification = 109"
                                pos[2]=01101101b
                        choice "Node Identification = 110"
                                pos[2]=01101110b
                        choice "Node Identification = 111"
                                pos[2]=01101111b
                        choice "Node Identification = 112"
                                pos[2]=01110000b
                        choice "Node Identification = 113"
                                pos[2]=01110001b
                        choice "Node Identification = 114"
                                pos[2]=01110010b
                        choice "Node Identification = 115"
                                pos[2]=01110011b
                        choice "Node Identification = 116"
                                pos[2]=01110100b
                        choice "Node Identification = 117"
                                pos[2]=01110101b
                        choice "Node Identification = 118"
                                pos[2]=01110110b
                        choice "Node Identification = 119"
                                pos[2]=01110111b
                        choice "Node Identification = 120"
                                pos[2]=01111000b
                        choice "Node Identification = 121"
                                pos[2]=01111001b
                        choice "Node Identification = 122"
                                pos[2]=01111010b
                        choice "Node Identification = 123"
                                pos[2]=01111011b
                        choice "Node Identification = 124"
                                pos[2]=01111100b
                        choice "Node Identification = 125"
                                pos[2]=01111101b
                        choice "Node Identification = 126"
                                pos[2]=01111110b
                        choice "Node Identification = 127"
                                pos[2]=01111111b
                        choice "Node Identification = 128"
                                pos[2]=10000000b
                        choice "Node Identification = 129"
                                pos[2]=10000001b
                        choice "Node Identification = 130"
                                pos[2]=10000010b
                        choice "Node Identification = 131"
                                pos[2]=10000011b
                        choice "Node Identification = 132"
                                pos[2]=10000100b
                        choice "Node Identification = 133"
                                pos[2]=10000101b
                        choice "Node Identification = 134"
                                pos[2]=10000110b
                        choice "Node Identification = 135"
                                pos[2]=10000111b
                        choice "Node Identification = 136"
                                pos[2]=10001000b
                        choice "Node Identification = 137"
                                pos[2]=10001001b
                        choice "Node Identification = 138"
                                pos[2]=10001010b
                        choice "Node Identification = 139"
                                pos[2]=10001011b
                        choice "Node Identification = 140"
                                pos[2]=10001100b
                        choice "Node Identification = 141"
                                pos[2]=10001101b
                        choice "Node Identification = 142"
                                pos[2]=10001110b
                        choice "Node Identification = 143"
                                pos[2]=10001111b
                        choice "Node Identification = 144"
                                pos[2]=10010000b
                        choice "Node Identification = 145"
                                pos[2]=10010001b
                        choice "Node Identification = 146"
                                pos[2]=10010010b
                        choice "Node Identification = 147"
                                pos[2]=10010011b
                        choice "Node Identification = 148"
                                pos[2]=10010100b
                        choice "Node Identification = 149"
                                pos[2]=10010101b
                        choice "Node Identification = 150"
                                pos[2]=10010110b
                        choice "Node Identification = 151"
                                pos[2]=10010111b
                        choice "Node Identification = 152"
                                pos[2]=10011000b
                        choice "Node Identification = 153"
                                pos[2]=10011001b
                        choice "Node Identification = 154"
                                pos[2]=10011010b
                        choice "Node Identification = 155"
                                pos[2]=10011011b
                        choice "Node Identification = 156"
                                pos[2]=10011100b
                        choice "Node Identification = 157"
                                pos[2]=10011101b
                        choice "Node Identification = 158"
                                pos[2]=10011110b
                        choice "Node Identification = 159"
                                pos[2]=10011111b
                        choice "Node Identification = 160"
                                pos[2]=10100000b
                        choice "Node Identification = 161"
                                pos[2]=10100001b
                        choice "Node Identification = 162"
                                pos[2]=10100010b
                        choice "Node Identification = 163"
                                pos[2]=10100011b
                        choice "Node Identification = 164"
                                pos[2]=10100100b
                        choice "Node Identification = 165"
                                pos[2]=10100101b
                        choice "Node Identification = 166"
                                pos[2]=10100110b
                        choice "Node Identification = 167"
                                pos[2]=10100111b
                        choice "Node Identification = 168"
                                pos[2]=10101000b
                        choice "Node Identification = 169"
                                pos[2]=10101001b
                        choice "Node Identification = 170"
                                pos[2]=10101010b
                        choice "Node Identification = 171"
                                pos[2]=10101011b
                        choice "Node Identification = 172"
                                pos[2]=10101100b
                        choice "Node Identification = 173"
                                pos[2]=10101101b
                        choice "Node Identification = 174"
                                pos[2]=10101110b
                        choice "Node Identification = 175"
                                pos[2]=10101111b
                        choice "Node Identification = 176"
                                pos[2]=10110000b
                        choice "Node Identification = 177"
                                pos[2]=10110001b
                        choice "Node Identification = 178"
                                pos[2]=10110010b
                        choice "Node Identification = 179"
                                pos[2]=10110011b
                        choice "Node Identification = 180"
                                pos[2]=10110100b
                        choice "Node Identification = 181"
                                pos[2]=10110101b
                        choice "Node Identification = 182"
                                pos[2]=10110110b
                        choice "Node Identification = 183"
                                pos[2]=10110111b
                        choice "Node Identification = 184"
                                pos[2]=10111000b
                        choice "Node Identification = 185"
                                pos[2]=10111001b
                        choice "Node Identification = 186"
                                pos[2]=10111010b
                        choice "Node Identification = 187"
                                pos[2]=10111011b
                        choice "Node Identification = 188"
                                pos[2]=10111100b
                        choice "Node Identification = 189"
                                pos[2]=10111101b
                        choice "Node Identification = 190"
                                pos[2]=10111110b
                        choice "Node Identification = 191"
                                pos[2]=10111111b
                        choice "Node Identification = 192"
                                pos[2]=11000000b
                        choice "Node Identification = 193"
                                pos[2]=11000001b
                        choice "Node Identification = 194"
                                pos[2]=11000010b
                        choice "Node Identification = 195"
                                pos[2]=11000011b
                        choice "Node Identification = 196"
                                pos[2]=11000100b
                        choice "Node Identification = 197"
                                pos[2]=11000101b
                        choice "Node Identification = 198"
                                pos[2]=11000110b
                        choice "Node Identification = 199"
                                pos[2]=11000111b
                        choice "Node Identification = 200"
                                pos[2]=11001000b
                        choice "Node Identification = 201"
                                pos[2]=11001001b
                        choice "Node Identification = 202"
                                pos[2]=11001010b
                        choice "Node Identification = 203"
                                pos[2]=11001011b
                        choice "Node Identification = 204"
                                pos[2]=11001100b
                        choice "Node Identification = 205"
                                pos[2]=11001101b
                        choice "Node Identification = 206"
                                pos[2]=11001110b
                        choice "Node Identification = 207"
                                pos[2]=11001111b
                        choice "Node Identification = 208"
                                pos[2]=11010000b
                        choice "Node Identification = 209"
                                pos[2]=11010001b
                        choice "Node Identification = 210"
                                pos[2]=11010010b
                        choice "Node Identification = 211"
                                pos[2]=11010011b
                        choice "Node Identification = 212"
                                pos[2]=11010100b
                        choice "Node Identification = 213"
                                pos[2]=11010101b
                        choice "Node Identification = 214"
                                pos[2]=11010110b
                        choice "Node Identification = 215"
                                pos[2]=11010111b
                        choice "Node Identification = 216"
                                pos[2]=11011000b
                        choice "Node Identification = 217"
                                pos[2]=11011001b
                        choice "Node Identification = 218"
                                pos[2]=11011010b
                        choice "Node Identification = 219"
                                pos[2]=11011011b
                        choice "Node Identification = 220"
                                pos[2]=11011100b
                        choice "Node Identification = 221"
                                pos[2]=11011101b
                        choice "Node Identification = 222"
                                pos[2]=11011110b
                        choice "Node Identification = 223"
                                pos[2]=11011111b
                        choice "Node Identification = 224"
                                pos[2]=11100000b
                        choice "Node Identification = 225"
                                pos[2]=11100001b
                        choice "Node Identification = 226"
                                pos[2]=11100010b
                        choice "Node Identification = 227"
                                pos[2]=11100011b
                        choice "Node Identification = 228"
                                pos[2]=11100100b
                        choice "Node Identification = 229"
                                pos[2]=11100101b
                        choice "Node Identification = 230"
                                pos[2]=11100110b
                        choice "Node Identification = 231"
                                pos[2]=11100111b
                        choice "Node Identification = 232"
                                pos[2]=11101000b
                        choice "Node Identification = 233"
                                pos[2]=11101001b
                        choice "Node Identification = 234"
                                pos[2]=11101010b
                        choice "Node Identification = 235"
                                pos[2]=11101011b
                        choice "Node Identification = 236"
                                pos[2]=11101100b
                        choice "Node Identification = 237"
                                pos[2]=11101101b
                        choice "Node Identification = 238"
                                pos[2]=11101110b
                        choice "Node Identification = 239"
                                pos[2]=11101111b
                        choice "Node Identification = 240"
                                pos[2]=11110000b
                        choice "Node Identification = 241"
                                pos[2]=11110001b
                        choice "Node Identification = 242"
                                pos[2]=11110010b
                        choice "Node Identification = 243"
                                pos[2]=11110011b
                        choice "Node Identification = 244"
                                pos[2]=11110100b
                        choice "Node Identification = 245"
                                pos[2]=11110101b
                        choice "Node Identification = 246"
                                pos[2]=11110110b
                        choice "Node Identification = 247"
                                pos[2]=11110111b
                        choice "Node Identification = 248"
                                pos[2]=11111000b
                        choice "Node Identification = 249"
                                pos[2]=11111001b
                        choice "Node Identification = 250"
                                pos[2]=11111010b
                        choice "Node Identification = 251"
                                pos[2]=11111011b
                        choice "Node Identification = 252"
                                pos[2]=11111100b
                        choice "Node Identification = 253"
                                pos[2]=11111101b
                        choice "Node Identification = 254"
                                pos[2]=11111110b
                        choice "Node Identification = 255"
                                pos[2]=11111111b
                help
                        "In order to access the network, a node identification number must be
assigned to this station. It is critical that the node identification selected be unique and
non-zero.  Please note that it is not possible for this configuration utility to determine if
the node ID selected is unique. Once an available node ID has been determined, hold the F5 or F6
key depressed to quickly scroll through the possible node identifications."

        nameditem
                prompt "RIM Buffer Base Address Offset Select"
                        choice "Offset 0D000"
                                pos[1]=XXXX1000b
                                mem 0D0000h-0D07FFh
                        choice "Offset 0D200"
                                pos[1]=XXXX1001b
                                mem 0D2000h-0D27FFh
                        choice "Offset 0D400"
                                pos[1]=XXXX1010b
                                mem 0D4000h-0D47FFh
                        choice "Offset 0D600"
                                pos[1]=XXXX1011b
                                mem 0D6000h-0D7FFFh
                        choice "Offset 0D800"
                                pos[1]=XXXX1100b
                                mem 0D8000h-0D87FFh
                        choice "Offset 0DA00"
                                pos[1]=XXXX1101b
                                mem 0DA000h-0DA7FFh
                        choice "Offset 0DC00"
                                pos[1]=XXXX1110b
                                mem 0DC000h-0DC7FFh
                        choice "Offset 0DE00"
                                pos[1]=XXXX1111b
                                mem 0DE000h-0DE7FFh
                        choice "Offset 0C000"
                                pos[1]=XXXX0000b
                                mem 0C0000h-0C07FFh
                        choice "Offset 0C200"
                                pos[1]=XXXX0001b
                                mem 0C2000h-0C27FFh
                        choice "Offset 0C400"
                                pos[1]=XXXX0010b
                                mem 0C4000h-0C47FFh
                        choice "Offset 0C600"
                                pos[1]=XXXX0011b
                                mem 0C6000h-0C7FFFh
                        choice "Offset 0C800"
                                pos[1]=XXXX0100b
                                mem 0C8000h-0C87FFh
                        choice "Offset 0CA00"
                                pos[1]=XXXX0101b
                                mem 0CA000h-0CA7FFh
                        choice "Offset 0CC00"
                                pos[1]=XXXX0110b
                                mem 0CC000h-0CC7FFh
                        choice "Offset 0CE00"
                                pos[1]=XXXX0111b
                                mem 0CE000h-0CE7FFh
                help
                        "In order for the RIM buffer to reside with any other
expansion RAM/ROM in the PS/2, a nonconflicting base address must be selected.
A conflict condition is indicated with an asterisk (*) at end of the base address
offset selected. Make note of the base address selected so that the proper network
shell can be installed. The default setting is offset 0D000."

        nameditem
                prompt "Base I/O Port Address Select"
                        choice "Base I/O Port 02E0"
                                pos[0]=XXXX010Xb
                                io 02E0h-02EFh
                        choice "Base I/O Port 0280"
                                pos[0]=XXXX000Xb
                                io 0280h-028Fh
                        choice "Base I/O Port 0260"
                                pos[0]=XXXX001Xb
                                io 0260h-026Fh
                        choice "Base I/O Port 0360"
                                pos[0]=XXXX011Xb
                                io 0360h-036Fh
                        choice "Base I/O Port 1280"
                                pos[0]=XXXX100Xb
                                io 1280h-128Fh
                        choice "Base I/O Port 3260"
                                pos[0]=XXXX101Xb
                                io 3260h-326Fh
                        choice "Base I/O Port 5280"
                                pos[0]=XXXX110Xb
                                io 5280h-528Fh
                        choice "Base I/O Port 7360"
                                pos[0]=XXXX111Xb
                                io 7360h-736Fh
                help
                        "In order for the LANcard/A-II to operate in the PS/2,
a nonconflicting base I/O port address must be selected. Under ordinary circumstances,
select the default address 02E0. A conflict condition is indicated with an asterisk (*)
at end of the base I/O port selected. Make note of the base port selected so that the
proper network shell can be installed."

        nameditem
                prompt "Interrupt Request Level Select"
                        choice "Interrupt Request IRQ2"
                                pos[3]=XXXXX000b
                                int 2
                        choice "Interrupt Request IRQ3"
                                pos[3]=XXXXX001b
                                int 3
                        choice "Interrupt Request IRQ4"
                                pos[3]=XXXXX010b
                                int 4
                        choice "Interrupt Request IRQ6"
                                pos[3]=XXXXX011b
                                int 6
                        choice "Interrupt Request IRQ7"
                                pos[3]=XXXXX100b
                                int 7
                        choice "Interrupt Request IRQ12"
                                pos[3]=XXXXX101b
                                int 12
                        choice "Interrupt Request IRQ14"
                                pos[3]=XXXXX110b
                                int 14
                        choice "Interrputs Disabled"
                                pos[3]=XXXXX111b
                help
                        "Normally, the default setting of IRQ2 is satisfactory for
the interrupt level request. Reference the Owner's Guide for more details regarding
choosing an interrupt level. Be sure to make note of the interrupt level selected
for the network shell installation. Warning! Do not attempt to access the network with
the interrupts disabled."

        nameditem
                prompt "Extended Timeout Select"
                        choice "Response Time = 74.7 us"
                                pos[1]=11XXXXXXb
                        choice "Response Time = 283.4 us"
                                pos[1]=10XXXXXXb
                        choice "Response Time = 561.8 us"
                                pos[1]=01XXXXXXb
                        choice "Response Time = 1118.6 us"
                                pos[1]=00XXXXXXb
                help
                        "To configure this adapter, the network extended timeout must be
selected. Under ordinary circumstances, select a 74.7 us response time. Warning!
All nodes must be configured with the same network response time. See the Owner's Guide
for more details."

        nameditem
                prompt "Boot PROM Base Address Select"
                        choice "PROM Disabled"
                                pos[1]=XX00XXXb
                        choice "Offset 0C000"
                                pos[0]=0000XXXXb
                                pos[1]=XX01XXXb
                                mem 0C0000h-0C07FFh
                        choice "Offset 0C200"
                                pos[0]=0001XXXXb
                                pos[1]=XX01XXXb
                                mem 0C2000h-0C27FFh
                        choice "Offset 0C400"
                                pos[0]=0010XXXXb
                                pos[1]=XX01XXXb
                                mem 0C4000h-0C47FFh
                        choice "Offset 0C600"
                                pos[0]=0011XXXXb
                                pos[1]=XX01XXXb
                                mem 0C6000h-0C7FFFh
                        choice "Offset 0C800"
                                pos[0]=0100XXXXb
                                pos[1]=XX01XXXb
                                mem 0C8000h-0C87FFh
                        choice "Offset 0CA00"
                                pos[0]=0101XXXXb
                                pos[1]=XX01XXXb
                                mem 0CA000h-0CA7FFh
                        choice "Offset 0CC00"
                                pos[0]=0110XXXXb
                                pos[1]=XX01XXXb
                                mem 0CC000h-0CC7FFh
                        choice "Offset 0CE00"
                                pos[0]=0111XXXXb
                                pos[1]=XX01XXXb
                                mem 0CE000h-0CE7FFh
                        choice "Offset 0D000"
                                pos[0]=1000XXXXb
                                pos[1]=XX01XXXb
                                mem 0D0000h-0D07FFh
                        choice "Offset 0D200"
                                pos[0]=1001XXXXb
                                pos[1]=XX01XXXb
                                mem 0D2000h-0D27FFh
                        choice "Offset 0D400"
                                pos[0]=1010XXXXb
                                pos[1]=XX01XXXb
                                mem 0D4000h-0D47FFh
                        choice "Offset 0D600"
                                pos[0]=1011XXXXb
                                pos[1]=XX01XXXb
                                mem 0D6000h-0D7FFFh
                        choice "Offset 0D800"
                                pos[0]=1100XXXXb
                                pos[1]=XX01XXXb
                                mem 0D8000h-0D87FFh
                        choice "Offset 0DA00"
                                pos[0]=1101XXXXb
                                pos[1]=XX01XXXb
                                mem 0DA000h-0DA7FFh
                        choice "Offset 0DC00"
                                pos[0]=1110XXXXb
                                pos[1]=XX01XXXb
                                mem 0DC000h-0DC7FFh
                        choice "Offset 0DE00"
                                pos[0]=1111XXXXb
                                pos[1]=XX01XXXb
                                mem 0DE000h-0DE7FFh
                help
                        "In order to perform a diskless boot, the adapter board must have
a boot PROM and a nonconflicting offset address between 0C000-0DE00 must be selected. A 
conflict condition is indicated with an asterisk (*) at end of the base address offset 
selected. Choose <PROM DISABLED> if there isn't a boot PROM on the board or to remove the 
PROM from the computer's address space."