
;
;  Copyright(c), 1988,1989. Computadoras Micron S.A. Mexico. 
;  Adapter File for TAMARIX/2 
;  Version Jan-9-1989  1.0
AdapterId	06F77h
AdapterName     "Lantana Technology Inc. Tamarix/2 Ethernet Adapter"
NumBytes        3

NamedItem
Prompt   "Adapter IO Space"
Choice   " IO Base 300h "    pos[0]=0011000Xb    io 0300h-031Fh
Choice   " IO Base 200h "    pos[0]=0010000Xb    io 0200h-021Fh
Choice   " IO Base 220h "    pos[0]=0010001Xb    io 0220h-023Fh
Choice   " IO Base 240h "    pos[0]=0010010Xb    io 0240h-025Fh
Choice   " IO Base 260h "    pos[0]=0010011Xb    io 0260h-027Fh
Choice   " IO Base 2A0h "    pos[0]=0010101Xb    io 02A0h-02BFh
Choice   " IO Base 2C0h "    pos[0]=0010110Xb    io 02C0h-02DFh
Choice   " IO Base 2E0h "    pos[0]=0010111Xb    io 02E0h-02FFh
Choice   " IO Base 280h "    pos[0]=0010100Xb    io 0280h-029Fh
Choice   " IO Base 320h "    pos[0]=0011001Xb    io 0320h-033Fh
Choice   " IO Base 340h "    pos[0]=0011010Xb    io 0340h-035Fh
Choice   " IO Base 360h "    pos[0]=0011011Xb    io 0360h-037Fh
Choice   " IO Base 380h "    pos[0]=0011100Xb    io 0380h-039Fh
Choice   " IO Base 3A0h "    pos[0]=0011101Xb    io 03A0h-03BFh
Choice   " IO Base 3C0h "    pos[0]=0011110Xb    io 03C0h-03DFh
Choice   " IO Base 3E0h "    pos[0]=0011111Xb    io 03E0h-03FFh
Help
"This selects the IO address space of the adapter.  Under normal circumstances,
 select < IO Base 300h >."

   
NamedItem
Prompt  "Shared Ram Space (16K)"
Choice   " Ram Base C4000h "   pos[1]=XXX10001b    mem 0C4000h-0C7FFFh
Choice   " Ram Base C0000h "   pos[1]=XXX10000b    mem 0C0000h-0C3FFFh
Choice   " Ram Base C8000h "   pos[1]=XXX10010b    mem 0C8000h-0CBFFFh
Choice   " Ram Base CC000h "   pos[1]=XXX10011b    mem 0CC000h-0CFFFFh
Choice   " Ram Base D0000h "   pos[1]=XXX10100b    mem 0D0000h-0D3FFFh
Choice   " Ram Base D4000h "   pos[1]=XXX10101b    mem 0D4000h-0D7FFFh
Choice   " Ram Base D8000h "   pos[1]=XXX10110b    mem 0D8000h-0DBFFFh
Choice   " Ram Base DC000h "   pos[1]=XXX10111b    mem 0DC000h-0DFFFFh
Help
"This selects the shared RAM memory address space.  Under normal circumstances,
 select < Ram Base C4000h >."


NamedItem
Prompt  "EPROM Type"
Choice   " EPROM Size  8K "   pos[2]=100XXXXXb
Choice   " EPROM Size 16K "   pos[2]=101XXXXXb
Choice   " EPROM Size 32K "   pos[2]=110XXXXXb
Choice   " EPROM Size 64K "   pos[2]=111XXXXXb
Help
"The EPROM can be either disabled or enabled.  When it is enabled, different
 sizes can be assigned. Under normal circumstances use <EPROM Size 8K>"

NamedItem
Prompt  "EPROM Space"
Choice   " EPROM Disabled " pos[2]=0XXXXXXXb     
Choice   " EPROM Base C0000h "   pos[2]=XXX10000b    mem 0C0000h-0C3FFFh
Choice   " EPROM Base C4000h "   pos[2]=XXX10001b    mem 0C4000h-0C7FFFh
Choice   " EPROM Base C8000h "   pos[2]=XXX10010b    mem 0C8000h-0CBFFFh
Choice   " EPROM Base CC000h "   pos[2]=XXX10011b    mem 0CC000h-0CFFFFh
Choice   " EPROM Base D0000h "   pos[2]=XXX10100b    mem 0D0000h-0D3FFFh
Choice   " EPROM Base D4000h "   pos[2]=XXX10101b    mem 0D4000h-0D7FFFh
Choice   " EPROM Base D8000h "   pos[2]=XXX10110b    mem 0D8000h-0DBFFFh
Choice   " EPROM Base DC000h "   pos[2]=XXX10111b    mem 0DC000h-0DFFFFh
Help
"The EPROM can be either disabled or enabled.  When it is enabled, different
 address spaces can be assigned.  Under normal circumstances, select
 <EPROM Disabled>."

NamedItem
Prompt  "Interrupt Level"
Choice   "Level 3"      pos[1]=010XXXXXb    int  3
Choice   "Level 4"      pos[1]=101XXXXXb    int  4
Choice   "Level 5"      pos[1]=100XXXXXb    int  5 
Choice   "Level 6"      pos[1]=011XXXXXb    int  6 
Choice   "Level 7"      pos[1]=110XXXXXb    int  7
Choice   "Level 9"      pos[1]=111XXXXXb    int  9
Choice   "Level 10"     pos[1]=001XXXXXb    int  10 
Choice   "Level 11"     pos[1]=000XXXXXb    int  11 
Help
"This selects the interrupt level this adapter will use.  Under normal 
 circumstances, select <Level 3>."

