
AdapterId 0DEFFh

AdapterName "IBM Multi-Protocol Communications Adapter"

NumBytes 2


NamedItem
	Prompt "Communications Port"
      choice "SDLC_1, Arb 1"    pos[0]=XXX1000Xb pos[1]=XXXX0001b
				io 0380h-038fh	int 3 4  arb 1
      choice "SDLC_1, Arb 7"    pos[0]=XXX1000Xb pos[1]=XXXX0111b
				io 0380h-038fh	int 3 4  arb 7
      choice "SDLC_1, Arb 0"    pos[0]=XXX1000Xb pos[1]=XXXX0000b
				io 0380h-038fh	int 3 4  arb 0
      choice "SDLC_1, Arb 3"    pos[0]=XXX1000Xb pos[1]=XXXX0011b
				io 0380h-038fh	int 3 4  arb 3
      choice "SDLC_1, Arb 4"    pos[0]=XXX1000Xb pos[1]=XXXX0100b
				io 0380h-038fh	int 3 4  arb 4
      choice "SDLC_1, Arb 5"    pos[0]=XXX1000Xb pos[1]=XXXX0101b
				io 0380h-038fh	int 3 4  arb 5
      choice "SDLC_1, Arb 6"    pos[0]=XXX1000Xb pos[1]=XXXX0110b
				io 0380h-038fh	int 3 4  arb 6
      choice "SDLC_1, Arb 8"    pos[0]=XXX1000Xb pos[1]=XXXX1000b
				io 0380h-038fh	int 3 4  arb 8
      choice "SDLC_1, Arb 9"    pos[0]=XXX1000Xb pos[1]=XXXX1001b
				io 0380h-038fh	int 3 4  arb 9
      choice "SDLC_1, Arb 10"   pos[0]=XXX1000Xb pos[1]=XXXX1010b
				io 0380h-038fh	int 3 4  arb 10
      choice "SDLC_1, Arb 11"   pos[0]=XXX1000Xb pos[1]=XXXX1011b
				io 0380h-038fh	int 3 4  arb 11
      choice "SDLC_1, Arb 12"   pos[0]=XXX1000Xb pos[1]=XXXX1100b
				io 0380h-038fh	int 3 4  arb 12
      choice "SDLC_1, Arb 13"   pos[0]=XXX1000Xb pos[1]=XXXX1101b
				io 0380h-038fh	int 3 4  arb 13
      choice "SDLC_1, Arb 14"   pos[0]=XXX1000Xb pos[1]=XXXX1110b
				io 0380h-038fh	int 3 4  arb 14

      choice "SDLC_2, Arb 1"    pos[0]=XXX1001Xb pos[1]=XXXX0001b
				io 03a0h-03afh	int 3 4  arb 1
      choice "SDLC_2, Arb 7"    pos[0]=XXX1001Xb pos[1]=XXXX0111b
				io 03a0h-03afh	int 3 4  arb 7
      choice "SDLC_2, Arb 0"    pos[0]=XXX1001Xb pos[1]=XXXX0000b
				io 03a0h-03afh	int 3 4  arb 0
      choice "SDLC_2, Arb 3"    pos[0]=XXX1001Xb pos[1]=XXXX0011b
				io 03a0h-03afh	int 3 4  arb 3
      choice "SDLC_2, Arb 4"    pos[0]=XXX1001Xb pos[1]=XXXX0100b
				io 03a0h-03afh	int 3 4  arb 4
      choice "SDLC_2, Arb 5"    pos[0]=XXX1001Xb pos[1]=XXXX0101b
				io 03a0h-03afh	int 3 4  arb 5
      choice "SDLC_2, Arb 6"    pos[0]=XXX1001Xb pos[1]=XXXX0110b
				io 03a0h-03afh	int 3 4  arb 6
      choice "SDLC_2, Arb 8"    pos[0]=XXX1001Xb pos[1]=XXXX1000b
				io 03a0h-03afh	int 3 4  arb 8
      choice "SDLC_2, Arb 9"    pos[0]=XXX1001Xb pos[1]=XXXX1001b
				io 03a0h-03afh	int 3 4  arb 9
      choice "SDLC_2, Arb 10"   pos[0]=XXX1001Xb pos[1]=XXXX1010b
				io 03a0h-03afh	int 3 4  arb 10
      choice "SDLC_2, Arb 11"   pos[0]=XXX1001Xb pos[1]=XXXX1011b
				io 03a0h-03afh	int 3 4  arb 11
      choice "SDLC_2, Arb 12"   pos[0]=XXX1001Xb pos[1]=XXXX1100b
				io 03a0h-03afh	int 3 4  arb 12
      choice "SDLC_2, Arb 13"   pos[0]=XXX1001Xb pos[1]=XXXX1101b
				io 03a0h-03afh	int 3 4  arb 13
      choice "SDLC_2, Arb 14"   pos[0]=XXX1001Xb pos[1]=XXXX1110b
				io 03a0h-03afh	int 3 4  arb 14

      choice "BISYNC_1"  pos[0]=XXX1100Xb  io 03a0h-03abh  int 3 4
      choice "BISYNC_2"  pos[0]=XXX1101Xb  io 0380h-038bh  int 3 4
      choice "SERIAL_1"  pos[0]=XXX0000Xb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=XXX0001Xb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=XXX0010Xb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=XXX0011Xb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=XXX0100Xb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=XXX0101Xb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=XXX0110Xb  io 5220h-5227h  int 3
      choice "SERIAL_8"  pos[0]=XXX0111Xb  io 5228h-522fh  int 3
   Help
"This port can be assigned as a:  primary (SDLC1) or
secondary (SDLC2) sdlc, primary (BISYNC1) or secondary
(BISYNC2) bisync, or as serial port (Serial 1 through Serial
8).  Use the F5=Previous and the F6=Next keys to change this
assignment in the 'Change configuration' window.  Conflicting
assignments are marked with an asterisk and must be changed to
use the adapter."

