; 
;	$Revision:   1.3  $
;	$Date:   09 Dec 1991 15:09:14  $
; 
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  			   *
;* Copyright (C) 1989 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

AdapterID 0df9fh

ADAPTERNAME  "Integrated Fixed Disk Controller"

NUMBYTES 2

FIXEDRESOURCES   int 0eh  io 3510h-3517h  pos[0]=XXXXXX0Xb  pos[1]=00XX1XXXb

NAMEDITEM 
	PROMPT	"DMA Arbitration Level"
	CHOICE  "Level 5"
		pos[0]=XX0101XXb  arb 5
	CHOICE  "Level 6"
		pos[0]=XX0110XXb  arb 6
	CHOICE  "Level 7"
		pos[0]=XX0111XXb  arb 7
	CHOICE  "Level 0"
		pos[0]=XX0000XXb  arb 0
	CHOICE  "Level 1"
		pos[0]=XX0001XXb  arb 1
	CHOICE  "Level 3"
		pos[0]=XX0011XXb  arb 3
	CHOICE  "Level 4"
		pos[0]=XX0100XXb  arb 4
	HELP
	   "This item selects the adapter's DMA channel used in
transferring data.  Under normal circumstances, where no conflicts
arise, use Level 5."

NAMEDITEM 
	PROMPT	"DMA Burst Pacing Interval"
	CHOICE  "24 microseconds"
		pos[1]=XX10XXXXb  
	CHOICE  "32 microseconds"
		pos[1]=XX11XXXXb  
	CHOICE  "16 microseconds"
		pos[1]=XX01XXXXb  
	CHOICE  "Burst Disabled"
		pos[1]=XX00XXXXb  
	HELP
	   "This item refers to the time interval between DMA transfer
bursts during which the processor gains control of the adapter card
bus.  Generally select 24 microseconds."

NAMEDITEM 
	PROMPT	"Fairness"
	CHOICE  "On"
		pos[0]=X1XXXXXXb  
	CHOICE  "Off"
		pos[0]=X0XXXXXXb  
	HELP
	   "This item determines whether the adapter will release
control of the bus when it has been using it exclusively.  Under
normal circumstances the fairness should be set to On."

