AdapterId 0704Eh

AdapterName "Video Capture Adapter/A"

NumBytes 4

fixedresources
       pos[1]=11111111b
       pos[2]=00000000b

NamedItem
        Prompt "Video Storage Address Select"
          Choice "D0000-DFFFF"
            pos[0]=0000XXXXb
            mem 0d0000h - 0dffffh
          Choice "D4000-DBFFF"
            pos[0]=0001XXXXb
            mem 0d4000h - 0dbfffh
          Choice "D8000-DFFFF"
            pos[0]=0010XXXXb
            mem 0d8000h - 0dffffh
          Choice "D0000-D3FFF,D8000-DBFFF"
            pos[0]=0011XXXXb
            mem 0d0000h-0d3fffh 0d8000h-0dbfffh
          Choice "D0000-D3FFF,DC000-DFFFF"
            pos[0]=0100XXXXb
            mem 0d0000h-0d3fffh 0dC000h-0dffffh
          Choice "D4000-D7FFF,DC000-DFFFF"
            pos[0]=0101XXXXb
            mem 0d4000h-0d7fffh 0dC000h-0dffffh
          Choice "D0000-D3FFF,CC000-CFFFF"
            pos[0]=0110XXXXb
            mem 0d0000h-0d3fffh 0CC000h-0Cffffh
          Choice "D0000-D3FFF,C0000-C3FFF"
            pos[0]=0111XXXXb
            mem 0d0000h-0d3fffh 0C0000h-0C3fffh
          Choice "D4000-D7FFF,C0000-C3FFF"
            pos[0]=1000XXXXb
            mem 0d4000h-0d7fffh 0C0000h-0C3fffh
          Choice "D4000-D7FFF,CC000-CFFFF"
            pos[0]=1001XXXXb
            mem 0d4000h-0d7fffh 0CC000h-0Cffffh
          Choice "D8000-DBFFF,C0000-C3FFF"
            pos[0]=1010XXXXb
            mem 0d8000h-0dbfffh 0C0000h-0C3fffh
          Choice "D8000-DBFFF,CC000-CFFFF"
            pos[0]=1011XXXXb
            mem 0d8000h-0dbfffh 0CC000h-0Cffffh
          Choice "CC000-CFFFF"
            pos[0]=1100XXXXb
            mem 0cc000h-0cffffh
          Choice "D8000-DBFFF"
            pos[0]=1101XXXXb
            mem 0d8000h-0dbfffh
          Choice "C0000-C3FFF"
            pos[0]=1110XXXXb
            mem 0C0000h - 0C3fffh
         Choice "F60000-FFFFFF,CC000-CFFFF"
            pos[0]=1111XXXXb
            mem 0f60000h-0ffffffh 0cc000h-0cffffh

   Help
         "This selects which system memory addresses will be dedicated
         to this adapter.  A choice of memory space at D0000 to D7FFFF
         is recommended.  This assignment need be changed only if it is
         in conflict with another assignment.  At least 2 16k blocks are
         recommended for card memory to card memory operations.
         Conflicting assignments are marked with an asterisk.  Use the
         F5=Previous and the F6=Next keys to change selection if you are
         in the 'Change configuration' window. If another choice must be
         made, try to use a selection with the most pages.  The protect
         mode selection may be used if your operating system supports
         'protect mode' such as OS/2.  DOS does not support 'protect
         mode'."

NamedItem
        Prompt "I/O Address Select"
      choice "5D00-5D0F"    pos[0]=XXXX000Xb   io 5D00h-5D0Fh
      choice "5D10-5D1F"    pos[0]=XXXX001Xb   io 5D10h-5D1Fh
      choice "7F00-7F0F"    pos[0]=XXXX010Xb   io 7F00h-7F0Fh
      choice "7F10-7F1F"    pos[0]=XXXX011Xb   io 7F10h-7F1Fh
      choice "DD00-DD0F"    pos[0]=XXXX100Xb  io 0DD00h-0DD0Fh
      choice "DD10-DD1F"    pos[0]=XXXX101Xb  io 0DD10h-0DD1Fh
      choice "FF00-FF0F"    pos[0]=XXXX110Xb  io 0FF00h-0FF0Fh
      choice "FF10-FF1F"    pos[0]=XXXX111Xb  io 0FF10h-0FF1Fh

   Help
         "This selects which I/O port addresses will be dedicated to
         this adapter.  The choice, 5D00-5D0F, is recommended.  This
         assignment need only be changed if it is in conflict with
         another assignment.  Conflicting assignments are marked with
         an asterisk.  Use the F5=Previous and the F6=Next keys to
         change the selection if you are in the 'Change
         configuration' window."

NamedItem
        Prompt "Interrupt Channel Select"

      choice "Interrupt  3 "   pos[3]=110000XXb  int  3
      choice "Interrupt  5 "   pos[3]=110010XXb  int  4
      choice "Interrupt  7 "   pos[3]=110100XXb  int  5
      choice "Interrupt  9 "   pos[3]=110110XXb  int  9
      choice "Interrupt  10"   pos[3]=111000XXb  int  10
      choice "Interrupt  11"   pos[3]=111010XXb  int  11
      choice "Interrupt  12"   pos[3]=111100XXb  int  12
      choice "Interrupt  15"   pos[3]=111110XXb  int  15

   Help
         "This selects which interrupt channel the adapter will use to
         signal an event.  The choice, interrupt 3, is recommended.
         This assignment need only be changed if it is in conflict
         with another assignment.  Conflicting assignments are marked
         with an asterisk.  Use the F5=Previous and the F6=Next keys
         to change the selection if you are in the 'Change
         configuration' window.  The selected interrupt is disabled."

