AdapterId 07FEAh

AdapterName "DigiBoard MC/Xi DOS RS422"

NumBytes 1

NamedItem

Prompt "Memory Start Address"

choice "0C0000" pos[0]=xxxxx00xb mem 00c0000h-00c7fffh

choice "0C8000" pos[0]=xxxxx01xb mem 00c8000h-00cffffh

choice "0D0000" pos[0]=xxxxx10xb mem 00d0000h-00d7fffh

choice "0D8000" pos[0]=xxxxx11xb mem 00d8000h-00dffffh 

Help

"Select one of four possible memory blocks of where Digiboards MC/Xi will
 reside in the hosts memory map"

NamedItem

Prompt "I/O PORT Address"

choice "F1F0h" pos[0]=xxx00xxxb io 0f1f0h-0f1f0h

choice "F2F0h" pos[0]=xxx01xxxb io 0f2f0h-0f2f0h

choice "F4F0h" pos[0]=xxx10xxxb io 0f4f0h-0f4f0h

choice "F8F0h" pos[0]=xxx11xxxb io 0f8f0h-0f8f0h

Help

"Select one of four possible I/O locations of where Digiboards MC/Xi will
 reside in the hosts I/O map"

NamedItem

Prompt "Interrupt Select"

choice "INT 11" pos[0]=111xxxxxb  int 11
choice "INT 10" pos[0]=110xxxxxb  int 10
choice "INT 5" pos[0]=010xxxxxb   int 5
choice "INT 4" pos[0]=001xxxxxb   int 4
choice "INT 9" pos[0]=101xxxxxb   int 9
choice "INT 7" pos[0]=100xxxxxb   int 7
choice "INT 6" pos[0]=011xxxxxb   int 6  
choice "INT 3" pos[0]=000xxxxxb   int 3  

Help

"Select one of eight possible Interrupt Request Lines which Digiboards 
 MC/Xi will interrupt the Host"