AdapterId 06DE0h

AdapterName "Sync-Up 2/V.32"

NumBytes 1

NamedItem
	Prompt "Asynchronous Modem Port" 
      choice "Serial_1"  pos[0]=1xx01xxxb io 03f8h-03ffh  int 4 
      choice "Serial_2"  pos[0]=1xx00xxxb io 02f8h-02ffh  int 3 
      choice "Serial_3"  pos[0]=1xx10xxxb io 3220h-3227h  int 3 
      choice "Serial_4"  pos[0]=1xx11xxxb io 3228h-322fh  int 3 
      choice "DISABLED"  pos[0]=0xx00xxxb 
 
Help 
"The Asynchronous portion of this modem 
can be assigned to use Serial_1 through Serial_
4 or DISABLED.  Use the F5=Previous and the 
F6=Next keys to change the assigment. 
Conflicting assignments are marked with an 
asterisk and must be changed." 
 
NamedItem 
	Prompt "Synchronous Modem Port" 
      choice "Sync-Up_1"	pos[0]=x10xx00xb io 0300h-030fh int 3 
      choice "Sync-Up_2"	pos[0]=x11xx00xb io 0300h-030fh int 4 
      choice "Sync-Up_3"	pos[0]=x10xx01xb io 0310h-031fh int 3 
      choice "Sync-Up_4"	pos[0]=x11xx01xb io 0310h-031fh int 4 
      choice "Sync-Up_5"	pos[0]=x10xx10xb io 0340h-034fh int 3 
      choice "Sync-Up_6"	pos[0]=x11xx10xb io 0340h-034fh int 4 
      choice "Sync-Up_7"	pos[0]=x10xx11xb io 0360h-036fh int 3 
      choice "Sync-Up_8"	pos[0]=x11xx11xb io 0360h-036fh int 4 
      choice "DISABLED" 	pos[0]=x00xx00xb 
 
Help 
"The Synchronous portion of this modem 
can be assigned to use Sync-Up_1 through Sync-Up_8 or 
DISABLED.  
Use the F5=Previous and the F6=Next keys to change 
the assigment.  Conflicting assignments are 
marked with an asterisk and must be changed." 
