
AdapterId 035FFh

AdapterName  " Dual UART Adapter"

NumBytes 1

NamedItem
        Prompt "Top Connector ( #1 )"
      choice "SERIAL_1"  pos[0]=XXXX000Xb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=XXXX001Xb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=XXXX010Xb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=XXXX011Xb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=XXXX100Xb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=XXXX101Xb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=XXXX110Xb  io 5220h-5227h  int 3
      choice "SERIAL_8"  pos[0]=XXXX111Xb  io 5228h-522fh  int 3
   Help
"This connector on the Dual UART Adapter can be selected
to use Serial 1 through Serial 8.  Use the F5=Previous and
the F6=Next keys to change serial port assignments if you
are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."

NamedItem
        Prompt "Bottom Connector -( # 2 ) "
      choice "SERIAL_1"  pos[0]=1000XXXXb  io 03f8h-03ffh  int 4
      choice "SERIAL_2"  pos[0]=1001XXXXb  io 02f8h-02ffh  int 3
      choice "SERIAL_3"  pos[0]=1010XXXXb  io 3220h-3227h  int 3
      choice "SERIAL_4"  pos[0]=1011XXXXb  io 3228h-322fh  int 3
      choice "SERIAL_5"  pos[0]=1100XXXXb  io 4220h-4227h  int 3
      choice "SERIAL_6"  pos[0]=1101XXXXb  io 4228h-422fh  int 3
      choice "SERIAL_7"  pos[0]=1110XXXXb  io 5220h-5227h  int 3
      choice "SERIAL_8"  pos[0]=1111XXXXb  io 5228h-522fh  int 3
   Help
"This connector on the Dual UART Adapter can be selected
to use Serial 1 through Serial 8.  Use the F5=Previous and
the F6=Next keys to change serial port assignments if you
are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."

