
AdapterId 06BCBh

AdapterName  "CONNECT ARCnet Adapter "

NumBytes 2

NamedItem
Prompt "Memory Address"
  Choice "Segment D000" pos[1]=0100XXXXb mem 0d0000h-0d3fffh
  Choice "Segment C000" pos[1]=0001XXXXb mem 0c0000h-0c3fffh
  Choice "Segment C400" pos[1]=0010XXXXb mem 0c4000h-0c7fffh
  Choice "Segment CC00" pos[1]=0011XXXXb mem 0cc000h-0cffffh
  Choice "Segment D400" pos[1]=0101XXXXb mem 0d4000h-0d7fffh
  Choice "Segment D800" pos[1]=0110XXXXb mem 0d8000h-0dbfffh
  Choice "Segment DC00" pos[1]=0111XXXXb mem 0dc000h-0dffffh
Help
"To be able to configure the CONNECT ARCnet adapter you must
select the memory address the ARCnet card shall use as buffer
RAM. You can select between seven different memory addresses.
Under normal conditions select  <Segment D000>."

NamedItem
Prompt  "Port Address"
  Choice "Port 02E0" pos[1]=XXXX0010b io 02e0h-02efh
  Choice "Port 02D0" pos[1]=XXXX0001b io 02d0h-02dfh
  Choice "Port 02F0" pos[1]=XXXX0011b io 02f0h-02ffh
  Choice "Port 0300" pos[1]=XXXX0100b io 0300h-030fh
  Choice "Port 0310" pos[1]=XXXX0101b io 0310h-031fh
  Choice "Port 32E0" pos[1]=XXXX0110b io 32e0h-42efh
  Choice "Port 42E0" pos[1]=XXXX0111b io 32e0h-42efh
Help
"To be able to configure the CONNECT ARCnet adapter you must
select the IO port address. You can select between seven different
IO addresses. Under normal conditions select  <Port 02E0>."

NamedItem
Prompt  "Interrupt Number"
  Choice "Int 9" pos[0]=XXXX000Xb int 9
  Choice "Int 3" pos[0]=XXXX001Xb int 3
  Choice "Int 4" pos[0]=XXXX010Xb int 4
  Choice "Int 5" pos[0]=XXXX011Xb int 5
  Choice "Int 7" pos[0]=XXXX100Xb int 7
  Choice "Int 10" pos[0]=XXXX101Xb int 10
  Choice "Int 11" pos[0]=XXXX110Xb int 11
  Choice "Int 12" pos[0]=XXXX111Xb int 12
Help
"To be able to configure the CONNECT ARCnet adapter you must
select interrupt. You can select between eight different
interrupts. Under normal conditions select  <Int 9>.
<Int 9> is equal to <Int 2> on PC/AT's "