AdapterID 06DACh

AdapterName "Logitech ScanMan Adapter"

NumBytes 4

NamedItem
     Prompt "Interrupt Level"
       choice "Int 3" pos[0]=00xxxxx1b int 3
       choice "Int 4" pos[0]=01xxxxx1b int 4
       choice "Int 5" pos[0]=10xxxxx1b int 5
     Help
"This is the Hardware Interrupt Level used by the ScanMan
Adapter, it can be shared with other adapters.
Use the F5=Previous and the F6=Next keys to change the
Hardware Interrupt Level if you are in the
'Change configuration' window."

NamedItem
     Prompt "DMA Channel (Arbitration Level)"
       choice "Level_1" pos[3]=xx110001b arb 1
       choice "Level_2" pos[3]=xx110010b arb 2
       choice "Level_3" pos[3]=xx110011b arb 3
     Help
"This is the DMA Channel used by the ScanMan Adapter.
Use the F5=Previous and the F6=Next keys to change the DMA
Channel if you are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."

NamedItem
     Prompt "I/O Address Range"
       choice "280h to 288h" pos[2]=00000010b pos[1]=10000000b io 280h-288h
       choice "2A0h to 2A8h" pos[2]=00000010b pos[1]=10100000b io 2A0h-2A8h
       choice "330h to 338h" pos[2]=00000011b pos[1]=00110000b io 330h-338h
       choice "340h to 348h" pos[2]=00000011b pos[1]=01000000b io 340h-348h
     Help
"This is the I/O Address Range used by the ScanMan Adapter.
Use the F5=Previous and the F6=Next keys to change the Base
Port Address if you are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."
