
AdapterID 0613Dh

AdapterName  "Rabbit RB75 Remote Communications Processor"
;
;**** combined 32k and 64k byte paged ***
;
NumBytes 4

fixedresources
	pos[3]=11000xxxb

nameditem
	Prompt	"Adapter Shared Ram Addressing"

	  Choice "D0000 thru DFFFF (64K bytes)"
	    pos[2]=XXXXX111b
	    pos[0]=1xxx0xxxb
	    mem 0d0000h-0dffffh

	  Choice "C0000 thru CFFFF (64K bytes)"
	    pos[2]=XXXXX110b
	    pos[0]=1xxx0xxxb
	    mem 0c0000h-0cffffh

	  Choice "A0000 thru AFFFF (64K bytes)"
	    pos[2]=XXXXX101b
	    pos[0]=1xxx0xxxb
	    mem 0a0000h-0affffh

	  Choice "D8000 thru DFFFF (32K bytes)"
	    pos[2]=XXXXX100b
	    pos[0]=1xxx1xxxb
	    mem 0d8000h-0dffffh

	  Choice "D0000 thru D7FFF (32K bytes)"
	    pos[2]=XXXXX011b
	    pos[0]=1xxx1xxxb
	    mem 0d0000h-0d7fffh

	  Choice "C8000 thru CFFFF (32K bytes)"
	    pos[2]=XXXXX010b
	    pos[0]=1xxx1xxxb
	    mem 0c8000h-0cffffh

	  Choice "C0000 thru C7FFF (32K bytes)"
	    pos[2]=XXXXX001b
	    pos[0]=1xxx1xxxb
	    mem 0c0000h-0c7fffh

	  Choice "A0000 thru A7FFF (32K bytes)"
	    pos[2]=XXXXX000b
	    pos[0]=1xxx1xxxb
	    mem 0a0000h-0a7fffh


	Help
	"Select the memory address range to be used by the RB75s shared RAM.
	 If no conflict exists, select the range <D0000 thru DFFFF>, 64K."


nameditem
	Prompt	"Adapter ROM/Control Location"
	  Choice "C8000 thru CBFFF"
	    pos[3]=XXXXX010b
	    mem 0c8000h-0cbfffh

	  Choice "CC000 thru CFFFF"
	    pos[3]=XXXXX011b
	    mem 0cc000h-0cffffh

	  Choice "D0000 thru D3FFF"
	    pos[3]=XXXXX100b
	    mem 0d0000h-0d3fffh

	  Choice "D4000 thru D7FFF"
	    pos[3]=XXXXX101b
	    mem 0d4000h-0d7fffh

	  Choice "D8000 thru DBFFF"
	    pos[3]=XXXXX110b
	    mem 0d8000h-0dbfffh

	  Choice "DC000 thru DFFFF"
	    pos[3]=XXXXX111b
	    mem 0dc000h-0dffffh

	  Choice "C0000 thru C3FFF"
	    pos[3]=XXXXX000b
	    mem 0c0000h-0c3fffh

	  Choice "C4000 thru C7FFF"
	    pos[3]=XXXXX001b
	    mem 0c4000h-0c7fffh

	Help
	"Select the memory address range to be used by the RB75 for its ROMS
	 and control logic.  If no conflict exists, select <C8000 thru CBFFF>."


nameditem
	Prompt	"Adapter Interrupt Level"
	  Choice "INT 5"
	    pos[0]=x001xxxxb
	    int 05h
	  Choice "INT 4"
	    pos[0]=x010xxxxb
	    int 04h
	  Choice "INT 3"
	    pos[0]=x011xxxxb
	    int 03h
	  Choice "INT 15"
	    pos[0]=x100xxxxb
	    int 0Fh
	  Choice "INT 11"
	    pos[0]=x110xxxxb
	    int 0Bh
	  Choice "INT 10"
	    pos[0]=x111xxxxb
	    int 0Ah
	Help
	"Select the hardware interrupt level to be used by the RB75 adapter.
	 There are six interrupts available, prioritized as
	 follows:
		  (highest)  10  11  15  3   4	 5   (lowest).

	 If no conflict exists, select <INT 5>"

nameditem
	Prompt	"Channel A DTR source selection"
	  Choice "DTRa = Z8530 Channel B"
	    pos[0]=xxxxxx0xb
	  Choice "DTRa = Z8530 Channel A"
	    pos[0]=xxxxxx1xb
	Help
	"Select the source for DTR on the primary serial channel.  Normally,
	 select DTRa = Z8530 Channel A."
