; Rev 1.0 - initial release
; Rev 1.1 - correspond to board release - no other changes

AdapterId 06792h

AdapterName  "NeoTecH 2 Serial / 1 Parallel Adapter, SPM121 / SPM321"

NumBytes 2

NamedItem
        Prompt "Serial Port A - I/O Address"

        Choice "Serial 2 (02F8h)" pos[0]=xx001xxxb io 02F8h-02FFh
        Choice "Serial 3 (3220h)" pos[0]=xx010xxxb io 3220h-3227h
        Choice "Serial 4 (3228h)" pos[0]=xx011xxxb io 3228h-322Fh
        Choice "Serial 5 (4220h)" pos[0]=xx100xxxb io 4220h-4227h
        Choice "Serial 6 (4228h)" pos[0]=xx101xxxb io 4228h-422Fh
        Choice "Serial 7 (5220h)" pos[0]=xx110xxxb io 5220h-5227h
        Choice "Serial 8 (5228h)" pos[0]=xx111xxxb io 5228h-522Fh
        Choice "Serial 1 (03F8h)" pos[0]=xx000xxxb io 03F8h-03FFh
Help
"This port can be assigned to Serial 1-8. Use the F5=Previous and 
F6=Next keys to change serial port assignments if you are in the 'Change 
configuration' window. Conflicting assignments are marked with an asterisk 
and must be changed to use the adapter."

NamedItem
        Prompt "Serial Port A - Interrupt"
        Choice "Level  3" pos[1]=xxx001xxb int 3
        Choice "Level  4" pos[1]=xxx010xxb int 4
        Choice "Level  5" pos[1]=xxx011xxb int 5
        Choice "Level  7" pos[1]=xxx100xxb int 7
        Choice "Level  9" pos[1]=xxx101xxb int 9
        Choice "Level 11" pos[1]=xxx110xxb int 11
        Choice "Level 12" pos[1]=xxx111xxb int 12
Help
"This port may be set to interrupt level 3,4,5,7,9,11 or 12.  Use the 
F5=Previous and F6=Next keys to change serial port assignments if you 
are in the 'Change configuration' window."
                                          
NamedItem
        Prompt "Serial Port B - I/O Address"

        Choice "Serial 3 (3220h)" pos[0]=10xxxxxxb 
                                  pos[1]=xxxxxxx0b io 3220h-3227h 
        Choice "Serial 4 (3228h)" pos[0]=11xxxxxxb 
                                  pos[1]=xxxxxxx0b io 3228h-322Fh 
        Choice "Serial 5 (4220h)" pos[0]=00xxxxxxb 
                                  pos[1]=xxxxxxx1b io 4220h-4227h 
        Choice "Serial 6 (4228h)" pos[0]=01xxxxxxb 
                                  pos[1]=xxxxxxx1b io 4228h-422Fh 
        Choice "Serial 7 (5220h)" pos[0]=10xxxxxxb 
                                  pos[1]=xxxxxxx1b io 5220h-5227h 
        Choice "Serial 8 (5228h)" pos[0]=11xxxxxxb 
                                  pos[1]=xxxxxxx1b io 5228h-522Fh 
        Choice "Serial 1 (03F8h)" pos[0]=00xxxxxxb 
                                  pos[1]=xxxxxxx0b io 03F8h-03FFh 
        Choice "Serial 2 (02F8h)" pos[0]=01xxxxxxb 
                                  pos[1]=xxxxxxx0b io 02F8h-02FFh 
Help
"This port can be assigned to Serial 1-8. Use the F5=Previous and 
F6=Next keys to change serial port assignments if you are in the 'Change 
configuration' window. Conflicting assignments are marked with an asterisk 
and must be changed to use the adapter."

NamedItem
        Prompt "Serial Port B - Interrupt"
        Choice "Level  3" pos[1]=001xxxxxb int 3
        Choice "Level  4" pos[1]=010xxxxxb int 4
        Choice "Level  5" pos[1]=011xxxxxb int 5
        Choice "Level  7" pos[1]=100xxxxxb int 7
        Choice "Level  9" pos[1]=101xxxxxb int 9
        Choice "Level 11" pos[1]=110xxxxxb int 11
        Choice "Level 12" pos[1]=111xxxxxb int 12
Help
"This port may be set to interrupt level 3,4,5,7,9,11 or 12.  Use the 
F5=Previous and F6=Next keys to change serial port assignments if you 
are in the 'Change configuration' window."

NamedItem
        Prompt "Parallel Port - I/O Address"
        Choice "Parallel 1 (03BCh)" pos[0]=xxxxx11xb io 03B0h-03BFh
        Choice "Parallel 2 (0378h)" pos[0]=xxxxx10xb io 0378h-037Fh
        Choice "Parallel 3 (0278h)" pos[0]=xxxxx01xb io 0278h-027Fh
        Choice "DISABLED          " pos[0]=xxxxx00xb
Help
"This port can be assigned to Parallel 1-3 or disabled. Use the F5=Previous 
and F6=Next keys to change serial port assignments if you are in the 'Change 
configuration' window. Conflicting assignments are marked with an asterisk 
and must be changed to use the adapter."

NamedItem
        Prompt "Parallel Port - Interrupt"
        Choice "Level  5" pos[1]=xxxxxx0xb int 5
        Choice "Level  7" pos[1]=xxxxxx1xb int 7
Help
"This port may be set to interrupt level 3,4,5,7,9,11 or 12.  Use the 
F5=Previous and F6=Next keys to change serial port assignments if you 
are in the 'Change configuration' window."


