
AdapterID 08EFEh

AdapterName  "IBM PS/2 SCSI Adapter"

NumBytes 3

fixedresources
        pos[2]=1X1000XXb
        pos[1]=XXXXXXXXb
        pos[0]=XXXXXXXXb
        int 0eh exec

nameditem
        Prompt "I/O Address"
          Choice  "3540-3547"
            pos[0]=XXXX000Xb
            io 3540h-3547h
          Choice  "3548-354F"
            pos[0]=XXXX001Xb
            io 3548h-354Fh
          Choice  "3550-3557"
            pos[0]=XXXX010Xb
            io 3550h-3557h
          Choice  "3558-355F"
            pos[0]=XXXX011Xb
            io 3558h-355Fh
          Choice  "3560-3567"
            pos[0]=XXXX100Xb
            io 3560h-3567h
          Choice  "3568-356F"
            pos[0]=XXXX101Xb
            io 3568h-356Fh
          Choice  "3570-3577"
            pos[0]=XXXX110Xb
            io 3570h-3577h
          Choice  "3578-357F"
            pos[0]=XXXX111Xb
            io 3578h-357Fh
        Help
         "This allows you to choose the I/O address for the adapter.
         Each adapter must have a unique address range.  Under normal
         circumstances, this address range does not need to be
         changed.  Use the F5=Previous or the F6=Next keys to change
         this assignment in the 'Change configuration' window.
         Conflicting assignments are marked with an asterisk and must
         be changed to use the adapter."

nameditem
        Prompt  "DMA Arbitration Level"
          Choice  "Level C"
            pos[1]=XXXX1100b
            arb 0ch
          Choice  "Level D"
            pos[1]=XXXX1101b
            arb 0dh
          Choice  "Level E"
            pos[1]=XXXX1110b
            arb 0eh
          Choice  "Level 1"
            pos[1]=XXXX0001b
            arb 1
          Choice  "Level 3"
            pos[1]=XXXX0011b
            arb 3
          Choice  "Level 5"
            pos[1]=XXXX0101b
            arb 5
          Choice  "Level 6"
            pos[1]=XXXX0110b
            arb 6
          Choice  "Level 7"
            pos[1]=XXXX0111b
            arb 7
          Choice  "Level 8"
            pos[1]=XXXX1000b
            arb 8
          Choice  "Level 9"
            pos[1]=XXXX1001b
            arb 9
          Choice  "Level A"
            pos[1]=XXXX1010b
            arb 0ah
          Choice  "Level B"
            pos[1]=XXXX1011b
            arb 0bh
        Help
        "This selects the DMA channel the adapter will use to transfer data.
         Under normal circumstances, select <Level C>.  Use the F5=Previous
         or the F6=Next keys to change this assignment in the 'Change
         configuration' window."

nameditem
        Prompt  "Fairness On/Off"
          Choice  "On"
            pos[1]=XXX1XXXXb
          Choice  "Off"
            pos[1]=XXX0XXXXb
        Help
        "Bus Arbitration Fairness.  This controls whether the adapter will
         release control of the bus when it has been using it exclusively.
         Under normal circumstances, select <On>.  Use the F5=Previous or
         the F6=Next keys to change this assignment in the 'Change
         configuration' window."

nameditem
        Prompt  "ROM Wait State Disable"
          Choice  "Enable Wait State"
            pos[2]=XXXXXXX0b
          Choice  "No Wait State"
            pos[2]=XXXXXXX1b
        Help
         "This allows you to set whether a wait state is added to
         accesses of the ROM on the adapter.  Adapter performance
         could be degraded if this is altered from the default.  Under
         normal circumstances, select <Enable Wait State>.  Use the
         F5=Previous or the F6=Next keys to change this assignment in
         the 'Change configuration' window."

nameditem
        Prompt  "SCSI Adapter Address (ID)"
          Choice "7"
            pos[1]=111XXXXXb
          Choice "6"
            pos[1]=110XXXXXb
          Choice "5"
            pos[1]=101XXXXXb
          Choice "4"
            pos[1]=100XXXXXb
          Choice "3"
            pos[1]=011XXXXXb
          Choice "2"
            pos[1]=010XXXXXb
          Choice "1"
            pos[1]=001XXXXXb
          Choice "0"
            pos[1]=000XXXXXb
        Help
        "This allows you to change the SCSI ID of the adapter.
         Under normal circumstances, select <7>.  Use the F5=Previous
         or the F6=Next keys to change this assignment in the 'Change
         configuration' window."
