AdapterId 0602Fh

AdapterName "ARCMASTER Microchannel/Arcnet Interface"

NumBytes 2

NamedItem

  Prompt "Memory or I/O Mapping"
    choice "Memory" pos[0]=XXXXXX11b
    choice "I/O"    pos[0]=XXXXXX01b
  Help
  "This adapter can be set for one of two operating modes.
  In the MEMORY mode, all of the card's resources are located
  entirely in the System Memory Map, compatible with the
  original ARCMASTER adapter.  In the I/O mode, the adapter
  is compatible with the SMC ARCNET adapter.
  Use F5 and F6 to select the operating mode"

NamedItem

  Prompt "I/O Base Address (for I/O Mode ONLY)"
    choice "02E0h" pos[0]=101110X1b
    choice "02F0h" pos[0]=101111X1b
    choice "0300h" pos[0]=110000X1b
    choice "0310h" pos[0]=110001X1b
    choice "0320h" pos[0]=110010X1b
    choice "0330h" pos[0]=110011X1b
    choice "0340h" pos[0]=110100X1b
    choice "0350h" pos[0]=110101X1b
    choice "0360h" pos[0]=110110X1b
    choice "0370h" pos[0]=110111X1b
    choice "0380h" pos[0]=111000X1b
    choice "0390h" pos[0]=111001X1b
    choice "03A0h" pos[0]=111010X1b
    choice "03B0h" pos[0]=111011X1b
    choice "03C0h" pos[0]=111100X1b
    choice "03D0h" pos[0]=111101X1b
    choice "03E0h" pos[0]=111110X1b
    choice "03F0h" pos[0]=111111X1b
    choice "0200h" pos[0]=100000X1b
    choice "0210h" pos[0]=100001X1b
    choice "0220h" pos[0]=100010X1b
    choice "0230h" pos[0]=100011X1b
    choice "0240h" pos[0]=100100X1b
    choice "0250h" pos[0]=100101X1b
    choice "0260h" pos[0]=100110X1b
    choice "0270h" pos[0]=100111X1b
    choice "0280h" pos[0]=101000X1b
    choice "0290h" pos[0]=101001X1b
    choice "02A0h" pos[0]=101010X1b
    choice "02B0h" pos[0]=101011X1b
    choice "02C0h" pos[0]=101100X1b
    choice "02D0h" pos[0]=101101X1b
  Help
  "Use F5 and F6 to select the I/O base address.  This setting
  is required only if the I/O operating mode is selected."

NamedItem

  Prompt "Interrupt Level"
    choice "3" pos[1]=XXXXXX00b
    choice "4" pos[1]=XXXXXX01b
    choice "5" pos[1]=XXXXXX10b
    choice "7" pos[1]=XXXXXX11b
  Help
  "Use F5 and F6 to select the interrupt level"

namedItem

  Prompt "Memory base address"
    choice "0D0000h" pos[1]=101000XXb
    choice "0D4000h" pos[1]=101010XXb
    choice "0D8000h" pos[1]=101100XXb
    choice "0DC000h" pos[1]=101110XXb
    choice "0C0000h" pos[1]=100000XXb
    choice "0C4000h" pos[1]=100010XXb
    choice "0C8000h" pos[1]=100100XXb
    choice "0CC000h" pos[1]=100110XXb
  Help
  "Use F5 and F6 to select the memory base address"
