;Rev. 01.1 07/23/93

AdapterId 06796h

AdapterName " NeoTecH Single Bidirectional Parallel Adapter, PM101"

NumBytes 3

NamedItem
        Prompt "Port Address"
        
        choice "PARALLEL 1 (03BCh)" pos[0]=XX1XXXXXb
                                    pos[1]=101111XXb
                                    pos[2]=00000011b  io 03B0h-03BFh 
        
        choice "PARALLEL 2 (0378h)" pos[0]=XX1XXXXXb
                                    pos[1]=011110XXb
                                    pos[2]=00000011b  io 0378h-037Fh 
        
        choice "PARALLEL 3 (0278h)" pos[0]=XX1XXXXXb
                                    pos[1]=011110XXb
                                    pos[2]=00000010b  io 0278h-027Fh 
        
Help
"This port can be assigned to Parallel 1, 2 or 3.  Use F5=Previous and the 
F6=Next keys to change parallel port assignments if you are in the 'Change 
configuration' window.  Conflicting assignments are marked with an asterisk 
and must be changed to use the adapter."

NamedItem
        Prompt "Interrupt Level"
        
        choice "Int  5" pos[0]=XXXXX11Xb  int 5
        
        choice "Int  7" pos[0]=XXXXX10Xb  int 7
        
        choice "Int 11" pos[0]=XXXXX01Xb  int 11  
        
        choice "Int 12" pos[0]=XXXXX00Xb  int 12 

Help
"This port can be assigned to Interrupt level 5, 7, 11 or 12. Use 
F5=Previous and the F6=Next keys to change serial port assignments if you are 
in the 'Change configuration' window. Conflicting assignments are marked 
with an asterisk and must be changed to use the adapter."

