AdapterID 0EFDCh

AdapterName "IBM ActionMedia (TM) II Display Adapter/A"

NumBytes 4

FixedResources
        POS[0]=XXXXXXX1b
        POS[1]=XXXXXXX1b
        POS[3]=1XXXXXXXb

Begin

NamedItem
  Prompt "Adapter I/O Addressing"
  Choice "I/O Addresses C000 - C03F"   POS[1]=110000XXb   IO 0C000h - 0C03Fh
  Choice "I/O Addresses C400 - C43F"   POS[1]=110001XXb   IO 0C400h - 0C5FFh
  Choice "I/O Addresses C800 - C83F"   POS[1]=110010XXb   IO 0C800h - 0C9FFh
  Choice "I/O Addresses CC00 - CC3F"   POS[1]=110011XXb   IO 0CC00h - 0CDFFh
  Choice "I/O Addresses B000 - B03F"   POS[1]=101100XXb   IO 0B000h - 0B1FFh
  Choice "I/O Addresses B400 - B43F"   POS[1]=101101XXb   IO 0B400h - 0B5FFh
  Choice "I/O Addresses B800 - B83F"   POS[1]=101110XXb   IO 0B800h - 0B9FFh
  Choice "I/O Addresses BC00 - BC3F"   POS[1]=101111XXb   IO 0BC00h - 0BDFFh
  Help
  "I/O ADDRESS RANGE:  This adapter occupies 64 bytes of I/O space.
   This may be located on any of the available 1024 byte boundaries.
   Use 'C000 - C03F' unless there is a conflict."


NamedItem
        Prompt "Extended Memory Window"
  Choice "8K  at Address C0000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0000XXXXb   MEM 0C0000h - 0C1FFFh
  Choice "8K  at Address C2000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0001XXXXb   MEM 0C2000h - 0C3FFFh
  Choice "8K  at Address C4000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0010XXXXb   MEM 0C4000h - 0C5FFFh
  Choice "8K  at Address C6000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0011XXXXb   MEM 0C6000h - 0C7FFFh
  Choice "8K  at Address C8000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0100XXXXb   MEM 0C8000h - 0C9FFFh
  Choice "8K  at Address CA000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0101XXXXb   MEM 0CA000h - 0CBFFFh
  Choice "8K  at Address CC000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0110XXXXb   MEM 0CC000h - 0CDFFFh
  Choice "8K  at Address CE000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=0111XXXXb   MEM 0CE000h - 0CFFFFh

  Choice "8K  at Address D0000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1000XXXXb   MEM 0D0000h - 0D1FFFh
  Choice "8K  at Address D2000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1001XXXXb   MEM 0D2000h - 0D3FFFh
  Choice "8K  at Address D4000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1010XXXXb   MEM 0D4000h - 0D5FFFh
  Choice "8K  at Address D6000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1011XXXXb   MEM 0D6000h - 0D7FFFh
  Choice "8K  at Address D8000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1100XXXXb   MEM 0D8000h - 0D9FFFh
  Choice "8K  at Address DA000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1101XXXXb   MEM 0DA000h - 0DBFFFh
  Choice "8K  at Address DC000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1110XXXXb   MEM 0DC000h - 0DDFFFh
  Choice "8K  at Address DE000"  POS[1]=XXXXXX0Xb   POS[0]=XXXX000Xb
                  POS[3]=X0000110b   POS[2]=1111XXXXb   MEM 0DE000h - 0DFFFFh

  Choice  "Disabled" POS[1]=XXXXXX1Xb   POS[0]=XXXX111Xb

  Choice "32K  at Address C0000"   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb
                    POS[3]=X0000110b   POS[2]=0000XXXXb   MEM 0C0000h - 0C7FFFh
  Choice "32K  at Address C8000"   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb
                    POS[3]=X0000110b   POS[2]=0100XXXXb   MEM 0C8000h - 0CFFFFh
  Choice "32K  at Address D0000"   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb
                    POS[3]=X0000110b   POS[2]=1000XXXXb   MEM 0D0000h - 0D7FFFh
  Choice "32K  at Address D8000"   POS[1]=XXXXXX0Xb   POS[0]=XXXX010Xb
                    POS[3]=X0000110b   POS[2]=1100XXXXb   MEM 0D8000h - 0DFFFFh


       Help
       "EXTENDED MEMORY WINDOW SIZE AND START ADDRESS: The OS/2 and
        Microsoft Windows drivers for this adapter require an 8K window
        to operate. Some other drivers may require a 32K window - see
        the information supplied with your driver in this case."

NamedItem
        Prompt "Capture Option Interrupt Level"
        Choice "Level 11"   POS[2]=XXXXXXX1b   INT 11d
        Choice "Level 10"   POS[2]=XXXXXXX0b   INT 10d
        Help
        "CAPTURE OPTION INTERRUPT LEVEL: The capture Option can use one of
         interrupt levels 10 or 11 for the capture Even/Odd interrupts."

NamedItem
        Prompt "Video Interrupt Level"
        Choice "Level 10"   POS[2]=XXXX01XXb   INT 10d
        Choice "Level 11"   POS[2]=XXXX10XXb   INT 11d
        Choice "Level  9"   POS[2]=XXXX11XXb   INT 09d
        Choice "Level 12"   POS[2]=XXXX00XXb   INT 12d
        Help
        "VIDEO INTERRUPT LEVEL:  This adapter can use one of interrupt
         levels 9 - 12 for Video interrupts."


NamedItem
        Prompt "Audio Interrupt Level"
        Choice "Level 10"   POS[2]=XXXXXX0Xb   INT 10d
        Choice "Level 11"   POS[2]=XXXXXX1Xb   INT 11d
        Help
        "AUDIO INTERRUPT LEVEL:  This adapter can use one of interrupt
         levels 10 or 11 for Audio interrupts."



NamedItem
        Prompt "Adapter Memory Location"
        Choice "C0000 - C1FFF"   POS[0]=0000XXXXb  MEM 0C0000h - 0C1FFFh
        Choice "C2000 - C3FFF"   POS[0]=0001XXXXb  MEM 0C2000h - 0C3FFFh
        Choice "C4000 - C5FFF"   POS[0]=0010XXXXb  MEM 0C4000h - 0C5FFFh
        Choice "C6000 - C7FFF"   POS[0]=0011XXXXb  MEM 0C6000h - 0C7FFFh
        Choice "C8000 - C9FFF"   POS[0]=0100XXXXb  MEM 0C8000h - 0C9FFFh
        Choice "CA000 - CBFFF"   POS[0]=0101XXXXb  MEM 0CA000h - 0CBFFFh
        Choice "CC000 - CDFFF"   POS[0]=0110XXXXb  MEM 0CC000h - 0CDFFFh
        Choice "CE000 - CFFFF"   POS[0]=0111XXXXb  MEM 0CE000h - 0CFFFFh

        Choice "D0000 - D1FFF"   POS[0]=1000XXXXb  MEM 0D0000h - 0D1FFFh
        Choice "D2000 - D3FFF"   POS[0]=1001XXXXb  MEM 0D2000h - 0D3FFFh
        Choice "D4000 - D5FFF"   POS[0]=1010XXXXb  MEM 0D4000h - 0D5FFFh
        Choice "D6000 - D7FFF"   POS[0]=1011XXXXb  MEM 0D6000h - 0D7FFFh
        Choice "D8000 - D9FFF"   POS[0]=1100XXXXb  MEM 0D8000h - 0D9FFFh
        Choice "DA000 - DBFFF"   POS[0]=1101XXXXb  MEM 0DA000h - 0DBFFFh
        Choice "DC000 - DDFFF"   POS[0]=1110XXXXb  MEM 0DC000h - 0DDFFFh
        Choice "DE000 - DFFFF"   POS[0]=1111XXXXb  MEM 0DE000h - 0DFFFFh

        Help
        "ADAPTER MEMORY LOCATION: The adapter needs an 8KB block of host
         address space for use only when the POST prom runs."

End
