
AdapterId	07522h
AdapterName     "ALR Micro Channel AT Imbedded Adapter"
NumBytes        4

FixedResources	pos[1]= XX000000b pos[2] = XXXXX1XXb pos[3] = XX100011b arb 3
   
NamedItem
Prompt  "Adapter ROM Location"
Choice   " Segment D000"   pos[2]=XX100XXXb    mem 0D0000h-0D3FFFh
Choice   " Segment C800"   pos[2]=XX010XXXb    mem 0C8000h-0CBFFFh
Choice   " Segment CC00"   pos[2]=XX011XXXb    mem 0CC000h-0CFFFFh
Choice   " Segment D400"   pos[2]=XX101XXXb    mem 0D4000h-0D7FFFh
Choice   " Segment D800"   pos[2]=XX110XXXb    mem 0D8000h-0DBFFFh
Choice   " Segment DC00"   pos[2]=XX111XXXb    mem 0DC000h-0DFFFFh
Help
"To configure this adapter you must choose the memory location
the adapter will use for its BIOS ROM. There are seven memory 
locations that can be selected.  Under normal circumstances, 
select <Segment C800>."

NamedItem
Prompt   "Adapter I/O Address"
Choice   "I/O Address 01F0h-01FFh"    pos[0]=XX00000Xb    io 01F0h-01FFh
Choice   "I/O Address 11F0h-11FFh"    pos[0]=XX00010Xb    io 11F0h-11FFh
Choice   "I/O Address 21F0h-21FFh"    pos[0]=XX00100Xb    io 21F0h-21FFh
Choice   "I/O Address 31F0h-31FFh"    pos[0]=XX00110Xb    io 31F0h-31FFh
Help
"You must choose the I/O location for the adapter to interface to
the imbedded drive. There are four possible I/O spaces. Under normal
circumstances, select <I/O Address 01F0h-01FFh>."

NamedItem
Prompt 	"Interrupt Level"
Choice 	"INT 14"		      pos[2]=XXXXXX0Xb	  int 14
Choice 	"INT 15"		      pos[2]=XXXXXX1Xb	  int 15
Help
"You must choose the interrupt level for the adapter to interrupt 
the system. Default condition is <INT 14>."

NamedItem
Prompt 	"Drive Type Assertion"
Choice 	"No Drive Type"		      pos[2]=XXXXXXX0b
Choice 	"Insert Drive Type 1"	      pos[2]=XXXXXXX1b	  
Help
"This option allows you to command the controller to control the assertion 
of the drive type into the system's CMOS. Default condition is no drive
type assertion "

