AdapterID 07064h

AdapterName "AW Computer Systems - RCP Adapter"

; Date 03-01-89  Rev B

NumBytes 3

NamedItem
Prompt "Control Port I/O"

choice "I/O 0110-0117" POS[0]=XXXX000Xb io 0110h - 0117h
choice "I/O 0120-0127" POS[0]=XXXX001Xb io 0120h - 0127h
choice "I/O 02B0-02B7" POS[0]=XXXX010Xb io 02B0h - 02B7h
choice "I/O 02D0-02D7" POS[0]=XXXX011Xb io 02D0h - 02D7h
choice "I/O 0310-0317" POS[0]=XXXX100Xb io 0310h - 0317h
choice "I/O 0360-0367" POS[0]=XXXX101Xb io 0360h - 0367h
choice "I/O 03A0-03A7" POS[0]=XXXX110Xb io 03A0h - 03A7h
choice "I/O 0150-0157" POS[0]=XXXX111Xb io 0150h - 0157h

HELP

" This assigns the I/O port address for PS2 - RCP control.
Use the F5=Previous and the F6=Next keys to change the I/O
address location.  Conflicting assignments are marked with
an asterisk and must be changed."


NamedItem
Prompt "Dual-Port Memory"

choice "FA0000-FA07FF" POS[2]=11111010b
                       POS[1]=00000XXXb mem 0FA0000h - 0FA07FFh
choice "FA2000-FA27FF" POS[2]=11111010b
                       POS[1]=00100XXXb mem 0FA2000h - 0FA27FFh
choice "FA4000-FA47FF" POS[2]=11111010b
                       POS[1]=01000XXXb mem 0FA4000h - 0FA47FFh
choice "FA6000-FA67FF" POS[2]=11111010b
                       POS[1]=01100XXXb mem 0FA6000h - 0FA67FFh
choice "08D000-08D7FF" POS[2]=00001000b
                       POS[1]=11010XXXb mem 08D000h - 08D7FFh
choice "09D000-09D7FF" POS[2]=00001001b
                       POS[1]=11010XXXb mem 09D000h - 09D7FFh
choice "0C0000-0C07FF" POS[2]=00001100b
                       POS[1]=00000XXXb mem 0C0000h - 0C07FFh
choice "0DD000-0DD7FF" POS[2]=00001101b
                       POS[1]=11010XXXb mem 0DD000h - 0DD7FFh
choice "DA0000-DA07FF" POS[2]=11011010b
                       POS[1]=00000XXXb mem 0DA0000h - 0DA07FFh
choice "DA2000-DA27FF" POS[2]=11011010b
                       POS[1]=00100XXXb mem 0DA2000h - 0DA27FFh
choice "DA4000-DA47FF" POS[2]=11011010b
                       POS[1]=01000XXXb mem 0DA4000h - 0DA47FFh
choice "DA6000-DA67FF" POS[2]=11011010b
                       POS[1]=01100XXXb mem 0DA6000h - 0DA67FFh
choice "EA0000-EA07FF" POS[2]=11101010b
                       POS[1]=00000XXXb mem 0EA0000h - 0EA07FFh
choice "EA2000-EA27FF" POS[2]=11101010b
                       POS[1]=00100XXXb mem 0EA2000h - 0EA27FFh
choice "EA4000-EA47FF" POS[2]=11101010b
                       POS[1]=01000XXXb mem 0EA4000h - 0EA47FFh
choice "EA6000-EA67FF" POS[2]=11101010b
                       POS[1]=01100XXXb mem 0EA6000h - 0EA67FFh

HELP

" This assigns the address block of the Dual Port Memory.
  Each address block is 2KX8 bits in size.
Use the F5=Previous and the F6=Next keys to change the address space.
Conflicting assignments are marked with an asterisk and must be changed."


NamedItem
Prompt "Interrupt Request "

choice "Interrupt 10"  POS[0]=XX01XXXXb  int 10
choice "Interrupt 11"  POS[0]=XX10XXXXb  int 11
choice "Interrupt 12"  POS[0]=XX11XXXXb  int 12

HELP

" This option is used to defined the interrupt level that is being
used by the RCP adapter.  Use the F5=Previous and the F6=Next keys
to change this assignmemt."
