AdapterId 06091h

AdapterName "Stallion Technologies ONboard2 Terminal Adapter [24 Feb 92]"

NumBytes 2

NamedItem
    Prompt "Memory Address"
	choice "0D0000-0DFFFF primary"
			pos[0]=XXX1101Xb pos[1]=0XXXXXXXb mem 00d0000h-00dffffh
	choice "0D0000-0DFFFF shared"
			pos[0]=XXX1101Xb pos[1]=1XXXXXXXb
	choice "0C0000-0CFFFF primary"
			pos[0]=XXX1100Xb pos[1]=0XXXXXXXb mem 00c0000h-00cffffh
	choice "0C0000-0CFFFF shared"
			pos[0]=XXX1100Xb pos[1]=1XXXXXXXb
	choice "E80000-E8FFFF primary"
			pos[0]=XXX0000Xb pos[1]=0XXXXXXXb mem 0e80000h-0e8ffffh
	choice "E80000-E8FFFF shared"
			pos[0]=XXX0000Xb pos[1]=1XXXXXXXb
	choice "E90000-E9FFFF primary"
			pos[0]=XXX0001Xb pos[1]=0XXXXXXXb mem 0e90000h-0e9ffffh
	choice "E90000-E9FFFF shared"
			pos[0]=XXX0001Xb pos[1]=1XXXXXXXb
	choice "EA0000-EAFFFF primary"
			pos[0]=XXX0010Xb pos[1]=0XXXXXXXb mem 0ea0000h-0eaffffh
	choice "EA0000-EAFFFF shared"
			pos[0]=XXX0010Xb pos[1]=1XXXXXXXb
	choice "EB0000-EBFFFF primary"
			pos[0]=XXX0011Xb pos[1]=0XXXXXXXb mem 0eb0000h-0ebffffh
	choice "EB0000-EBFFFF shared"
			pos[0]=XXX0011Xb pos[1]=1XXXXXXXb
	choice "EC0000-ECFFFF primary"
			pos[0]=XXX0100Xb pos[1]=0XXXXXXXb mem 0ec0000h-0ecffffh
	choice "EC0000-ECFFFF shared"
			pos[0]=XXX0100Xb pos[1]=1XXXXXXXb
	choice "ED0000-EDFFFF primary"
			pos[0]=XXX0101Xb pos[1]=0XXXXXXXb mem 0ed0000h-0edffffh
	choice "ED0000-EDFFFF shared"
			pos[0]=XXX0101Xb pos[1]=1XXXXXXXb
	choice "EE0000-EEFFFF primary"
			pos[0]=XXX0110Xb pos[1]=0XXXXXXXb mem 0ee0000h-0eeffffh
	choice "EE0000-EEFFFF shared"
			pos[0]=XXX0110Xb pos[1]=1XXXXXXXb
	choice "EF0000-EFFFFF primary"
			pos[0]=XXX0111Xb pos[1]=0XXXXXXXb mem 0ef0000h-0efffffh
	choice "EF0000-EFFFFF shared"
			pos[0]=XXX0111Xb pos[1]=1XXXXXXXb
    Help
"This option selects the 64KByte address space to be used by the ONboard2s
Dual Port Memory. Any memory conflicts with other adapters will be indicated. 
Use another memory address for your ONboard Dual Port Memory if a conflict 
occurs.

ONboard2s which are Revision 2.1 or later can share the same memory address
with other ONboard2s which are Revision 2.1 or later. This is often necessary
if the system has very limited free memory space. When installing multiple
ONboard2s at the same memory address, one board only should be set to use the
'primary' option and the others should all use the 'shared' option. This will
prevent the configuration utility from indicating a memory clash between the
ONboard2s located at the same address."


NamedItem
    Prompt "I/O Address"
	choice "780 - 78F" pos[1]=XXXXX000b io 780h-78fh
	choice "790 - 79F" pos[1]=XXXXX001b io 790h-79fh
	choice "7A0 - 7AF" pos[1]=XXXXX010b io 7a0h-7afh
	choice "7B0 - 7BF" pos[1]=XXXXX011b io 7b0h-7bfh
	choice "7C0 - 7CF" pos[1]=XXXXX100b io 7c0h-7cfh
	choice "7D0 - 7DF" pos[1]=XXXXX101b io 7d0h-7dfh
	choice "7E0 - 7EF" pos[1]=XXXXX110b io 7e0h-7efh
	choice "7F0 - 7FF" pos[1]=XXXXX111b io 7f0h-7ffh
    Help
"This option selects the I/O space used by the ONboard2 adapter. If installing
multiple ONboard2s, then each board should be set to use a unique I/O address.
(Note : Conflicts with other adapters should be resolved before saving the
configuration)"


NamedItem
    Prompt "Interrupt"
	choice "15" pos[0]=111XXXXXb int 15
	choice "12" pos[0]=110XXXXXb int 12
	choice "11" pos[0]=101XXXXXb int 11
	choice "10" pos[0]=100XXXXXb int 10
	choice " 7" pos[0]=011XXXXXb int 7
	choice " 3" pos[0]=000XXXXXb int 3
    Help
"This option sets the interrupt line used by the ONboard2 adapter.  If
installing multiple ONboard2s, then each board should be set to use a unique
interrupt line. (Note : Conflicts with other adapters should be resolved 
before saving the configuration. This utility may not show a conflict as shared
interrupts are allowed on the MCA bus, but ONboard2s do not support them.)"
