;
;
AdapterId 080E6h

AdapterName "RasterOps ColorBoard 1024MC"

NumBytes 4


FixedResources	
	
	pos[1]=XXXXXXXXb

	pos[2]=00000001b

	pos[3]=XXXXXXXXb





NamedItem

Prompt  "Enable/Disable Adapter"

Choice  " Adapter Enabled "  pos[0]=XXXXXXX1b

Choice  " Adapter Disabled " pos[0]=XXXXXXX0b

Help

"This controls whether the adapter is enabled or not.
Use the Enabled setting for normal use. Use the Disabled setting 
if you are not using the adapter and enabling it causes a conflict
with another device."





NamedItem	

Prompt	"Frame Buffer Starting Address"

choice " Base address: 00C00000h " pos[0]=X0XXXXXXb mem 0C00000h-0FFFFFFh

choice " Base address: 00800000h " pos[0]=X1XXXXXXb mem 0800000h-0BFFFFFh 

Help
"The Frame Buffer Address space can be selected by the user to be either
00800000h or 00C00000h.	Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window. Conflicting assignments
are marked with an asterisk and must be changed to use the adapter."





;NamedItem	
;
;Prompt	"Frame Buffer Starting Address"
;
;choice " Automatic Selection " pos[0]=XXXXXXXXb Exec
;
;
;Help
;"The Frame Buffer Address space will be selected to be either
;00800000h or 00C00000h.	Conflicting assignments	are marked with 
;an asterisk and must be changed to use the adapter."



NamedItem	

Prompt	"Frame Buffer I/O Starting Address"

choice " Base address: 5800h " pos[0]=XX11XXXXb	io 5800h-581Fh 

choice " Base address: 4000h " pos[0]=XX00XXXXb	io 4000h-401Fh 

choice " Base address: 4800h " pos[0]=XX01XXXXb io 4800h-481Fh

choice " Base address: 5000h " pos[0]=XX10XXXXb	io 5000h-501Fh 


Help
"The Frame Buffer I/O Address space can be selected by the user to be 4000h,
4800h, 5000h or 5800h.	Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window. Conflicting assignments
are marked with an asterisk and must be changed to use the adapter."



NamedItem	

Prompt	"PROM Starting Address"

choice " PROM Address: 0C0000h " 	pos[0]=XXXX1XXXb mem 0C0000h-0C3FFFh 

choice " PROM Address: 0C4000h "	pos[0]=XXXX0XXXb mem 0C4000h-0C7FFFh 


Help
"The Adapter PROM Address space can be selected by the user to be either
0C0000h or 0C4000h. Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window. Conflicting assignments
are marked with an asterisk and must be changed to use the adapter."










