
AdapterID 01B2h

AdapterName  "Cogent E/MASTER III MCA 32-bit Ethernet Adapter"

NumBytes 2

nameditem

Prompt  "Enable/Disable Adapter"

Choice  "Adapter Enabled "    pos[0]=XXXXXXX1b
Choice  "Adapter Disabled "   pos[0]=XXXXXXX0b

Help

"This controls whether the adapter is enabled or not.
Use the Enabled setting for normal use.
Use the Disabled setting if you are not using
the adapter and enabling it causes a conflict
with another device."

nameditem
        Prompt  "Interrupt Request Level"
          Choice  "IRQ 10"
            pos[0]=011XXXXXb
            int 10
          Choice  "IRQ 11"
            pos[0]=100XXXXXb
            int 11
          Choice  "IRQ 12"
            pos[0]=101XXXXXb
            int 12
          Choice  "IRQ 14"
            pos[0]=110XXXXXb
            int 14
          Choice  "IRQ 15"
            pos[0]=111XXXXXb
            int 15
          Choice  "IRQ 3"
            pos[0]=000XXXXXb
            int 3
          Choice  "IRQ 5"
            pos[0]=001XXXXXb
            int 5
          Choice  "IRQ 9"
            pos[0]=010XXXXXb
            int 9
        Help
        "This selects the interrupt request level the adapter will use.
         Under normal circumstances, select <IRQ 10>."

nameditem
        Prompt  "Adapter I/O Range"
          Choice  "1800-18FFh"
            pos[1]=X001XXXXb
            io 1800h-18ffh
          Choice  "5000-50FFh"
            pos[1]=X010XXXXb
            io 5000h-50ffh
          Choice  "5800-58FFh"
            pos[1]=X011XXXXb
            io 5800h-58ffh
          Choice  "9000-90FFh"
            pos[1]=X100XXXXb
            io 9000h-90ffh
          Choice  "9800-98FFh"
            pos[1]=X101XXXXb
            io 9800h-98ffh
          Choice  "D000-D0FFh"
            pos[1]=X110XXXXb
            io 0d000h-0d0ffh
          Choice  "D800-D8FFh"
            pos[1]=X111XXXXb
            io 0d800h-0d8ffh
        Help
        "This selects the I/O address range used by the adapter.
         Under normal circumstances, select <1000-10FFh>."

nameditem
        Prompt  "Master Mode Arbitration Level"
          Choice  "Level 8"
            pos[0]=XXXX000Xb
            arb 8
          Choice  "Level 9"
            pos[0]=XXXX001Xb
            arb 9
          Choice  "Level 10"
            pos[0]=XXXX010Xb
            arb 10
          Choice  "Level 11"
            pos[0]=XXXX011Xb
            arb 11
          Choice  "Level 12"
            pos[0]=XXXX100Xb
            arb 12
          Choice  "Level 13"
            pos[0]=XXXX101Xb
            arb 13
          Choice  "Level 14"
            pos[0]=XXXX110Xb
            arb 14
          Choice  "Level 15"
            pos[0]=XXXX111Xb
            arb 15
        Help
        "This selects the arbitration level the adapter will use during
         master mode data transfers.  Under normal circumstances, select
         <Level 8>."

nameditem
        Prompt  "Fairness On/Off"
          Choice  "On"
            pos[0]=XXX1XXXXb
          Choice  "Off"
            pos[0]=XXX0XXXXb
        Help
        "Bus Arbitration Fairness.  This controls whether the adapter will
         release control of the bus when it has been pre-empted.
         Under normal circumstances, select <On>."

nameditem
        Prompt  "Media Select"
          Choice  "Thin"
            pos[1]=1XXXXXXXb
          Choice  "Thick"
            pos[1]=0XXXXXXXb
        Help
        "Cable type selection.  This controls whether the adapter's
         network interface will use the Ethernet (thick) connector or the
         Cheapernet (thin) connector.  The default selection is <Thin>."
