
AdapterID 06018h

AdapterName  "Gateway Communications G/Ethernet Controller"

NumBytes 2

nameditem
        Prompt  "Interrupt Level Select"
          Choice  "IRQ Level 5" pos[0]=XXX0101Xb int 5
          Choice  "IRQ Level 4" pos[0]=XXX0100Xb int 4
          Choice  "IRQ Level 6" pos[0]=XXX0110Xb int 6
          Choice  "IRQ Level 7" pos[0]=XXX0111Xb int 7
          Choice  "IRQ Level 9" pos[0]=XXX1001Xb int 9
          Choice  "IRQ Level 10" pos[0]=XXX1010Xb int 10
          Choice  "IRQ Level 11" pos[0]=XXX1011Xb int 11
          Choice  "IRQ Level 12" pos[0]=XXX1100Xb int 12
        Help
        "This selects the interrupt level the adapter will use to request
	 service from the PS/2 computer. Under normal circumstances, 
	 select <Level 5>."

nameditem
        Prompt  "I/O Port Select"
         Choice  "I/O Base 280" pos[1]=00010100b io 0280h-029Fh 
         Choice  "I/O Base 2A0" pos[1]=00010101b io 02A0h-02BFh
         Choice  "I/O Base 2C0" pos[1]=00010110b io 02C0h-02DFh
         Choice  "I/O Base 2E0" pos[1]=00010111b io 02E0h-02FFh
         Choice  "I/O Base 300" pos[1]=00011000b io 0300h-031Fh
         Choice  "I/O Base 320" pos[1]=00011001b io 0320h-033Fh
         Choice  "I/O Base 340" pos[1]=00011010b io 0340h-035Fh
         Choice  "I/O Base 360" pos[1]=00011011b io 0360h-037Fh
         Choice  "I/O Base 380" pos[1]=00011100b io 0380h-039Fh
	Help
	"This selects the I/O address range to which the adapter will respond
	 when addressed by the PS/2 computer. Thirty-two contiguous addresses
	 are used by the adapter. More ranges can be defined if these conflict."
