;***************************************************************************
;* Copyright (C) 1993 by NCR Corporation    This program		   *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;*************************************************************************** 

; Prototype ADF file
; Not for release
; 3/26/93

AdapterId 05136h

AdapterName "NCR Audio Adapter w/o FM Synthesis"

NumBytes 4

FixedResources

; AT Compatibility bit
	pos[0]=XX1XXXXXb

NamedItem
   Prompt  "Adapter enable/disable"
	choice	"NCR Audio Adapter ENABLED"	pos[0]=XXXXXXX1b
	choice  "NCR Audio Adapter DISABLE"	pos[0]=XXXXXXX0b

Help
"This option will allow you to disable the audio adapter."

NamedItem
      Prompt "Adapter I/O Address range"
      choice "I/O Ports 530-537"  pos[0]=XXX00XXXb   io 00530h-00537h
      choice "I/O Ports 604-60B"  pos[0]=XXX11XXXb   io 00604h-0060Bh
      choice "I/O Ports E80-E87"  pos[0]=XXX01XXXb   io 00E80h-00E87h
      choice "I/O Ports F40-F47"  pos[0]=XXX10XXXb   io 00F40h-00F47h

Help
"You may set the adapter to any of the I/O addresses 
ranges listed.  The first choice is recommended.
If your selection conflicts with an I/O address already 
assigned in your system, it will be marked with an asterisk
and you must select an alternate address."

NamedItem
  Prompt "Adapter Interrupt Level"
      choice "Int Level 9"     pos[1]=XXX01XXXb   INT 9
      choice "Int Level 10"    pos[1]=XXX10XXXb   INT 10
      choice "Int Level 11"    pos[1]=XXX11XXXb   INT 11
      choice "Int Level 7"     pos[1]=XXX00XXXb   INT 7  
  Help
"Set the adapter Interrupt Level so it will not conflict with 
other interrupting devices.

If Interrupt Levels 7, 9, 10 and 11 are used by other devices, the best
choice may be to select Interrupt level 7 for the audio adapter rather
than conflict with other adapters.  Interrupt Level 7 is connected to the
system board Parallel Port, but its interrupt is often not used by software,
allowing use of Interrup Level 7 by the Audio Adapter's drivers."

NamedItem
      Prompt "Adapter DMA Level"
      choice "Play level 0, Record uses play level"
	    pos[0]=XXXXX00Xb   pos[1]=XXXXX11Xb   arb 0
      choice "Play level 1, Record uses play level"
	    pos[0]=XXXXX01Xb   pos[1]=XXXXX11Xb   arb 1
      choice "Play level 3, Record uses play level"
	    pos[0]=XXXXX10Xb   pos[1]=XXXXX11Xb   arb 3
      choice "Play level 0, Record level 1"
	    pos[0]=XXXXX00Xb   pos[1]=XXXXX01Xb   arb 0 arb 1
      choice "Play level 1, Record level 0"
	    pos[0]=XXXXX01Xb   pos[1]=XXXXX00Xb   arb 0 arb 1
      choice "Play level 3, Record level 0"
	    pos[0]=XXXXX10Xb   pos[1]=XXXXX00Xb   arb 0 arb 3

  Help
"The adapter supports the direct memory access (DMA) 
mode of data transfer. You may select any of the DMA 
levels listed.  We recommend you select one of the first
three levels listed. If your selection conflicts with a DMA level 
already assigned in the system, it will be marked with an 
asterisk and you must select an alternative level."

