
AdapterID 06B95h

AdapterName  "CORE ESDI Fixed Disk Controller"

NumBytes 2

fixedresources
	pos[0]=0XXXXXXXb
	pos[1]=00XXXXXXb

nameditem
	Prompt	"Adapter Memory Location"
	  Choice "Segment C800" pos[1]=XXXX0010b mem 0c8000h-0cbfffh
	  Choice "Segment CC00" pos[1]=XXXX0011b mem 0cc000h-0cffffh
	  Choice "Segment D000" pos[1]=XXXX0100b mem 0d0000h-0d3fffh
	  Choice "Segment D400" pos[1]=XXXX0101b mem 0d4000h-0d7fffh
	  Choice "Segment D800" pos[1]=XXXX0110b mem 0d8000h-0dbfffh
	  Choice "Segment DC00" pos[1]=XXXX0111b mem 0dc000h-0dffffh
	  Choice  "ROM Disabled" pos[1]=XXXX0000b
	Help
	"Select the ROM segment for the CORE MCA adapter.  If you have more than
	 one MCA adapter installed, be sure to disable the ROM on all adapters
	 except the first."


nameditem
	Prompt	"DMA Arbitration Level"
	  Choice  "Level 5" pos[0]=XX0101XXb arb 5
	  Choice  "Level 6" pos[0]=XX0110XXb arb 6
	  Choice  "Level 7" pos[0]=XX0111XXb arb 7
	  Choice  "Level 0" pos[0]=XX0000XXb arb 0
	  Choice  "Level 1" pos[0]=XX0001XXb arb 1
	  Choice  "Level 3" pos[0]=XX0011XXb arb 3
	  Choice  "Level 4" pos[0]=XX0100XXb arb 4
	  Choice  "Level 8" pos[0]=XX1000XXb arb 8
	  Choice  "Level 9" pos[0]=XX1001XXb arb 9
	  Choice  "Level 0A" pos[0]=XX1010XXb arb 0ah
	  Choice  "Level 0B" pos[0]=XX1011XXb arb 0bh
	  Choice  "Level 0C" pos[0]=XX1100XXb arb 0ch
	  Choice  "Level 0D" pos[0]=XX1101XXb arb 0dh
	  Choice  "Level 0E" pos[0]=XX1110XXb arb 0eh
	Help
	"This selects the Arbitration level that the controller will use when
	 competing for the channel."

nameditem
	Prompt	"DMA Burst Length"
	  Choice  "32 Word Burst" pos[1]=XX11XXXXb
	  Choice  " 4 Word Burst" pos[1]=XX00XXXXb
	  Choice  " 8 Word Burst" pos[1]=XX01XXXXb
	  Choice  "16 Word Burst" pos[1]=XX10XXXXb
	Help
	"This is the maximum number of words that the controller will
	 transfer per Bus Requset."

nameditem
	Prompt	"IO Address"
	  Choice    "2510-251F" pos[0]=XXXXXX0Xb io 02510h-0251fh
	  Choice    "2520-252F" pos[0]=XXXXXX1Xb io 02520h-0252fh
	Help
	"The controller may be located in one of the following I/O address
	 locations: 2510-251Fh or 2520-252Fh"

nameditem
	Prompt	"Fairness On/Off"
	  Choice  "On"  pos[0]=X1XXXXXXb
	  Choice  "Off" pos[0]=X0XXXXXXb
	Help
	"Bus Arbitration Fairness.  This controls whether the adapter will
	 release control of the bus when other adapters ask for the
	 bus."
