AdapterID       071D4h

AdapterName     "Kingston Technology DataCard 16"

NumBytes        4

NamedItem
prompt  "Controller I/O Address"
Choice  " I/O Base 8020 - 803f" pos[3]=1xxxxx00b    IO 08020h-0803fh
Choice  " I/O Base 8120 - 813f" pos[3]=1xxxxx01b    IO 08120h-0813fh
Choice  " I/O Base 8220 - 823f" pos[3]=1xxxxx10b    IO 08220h-0823fh
Choice  " I/O Base 8320 - 833f" pos[3]=1xxxxx11b    IO 08320h-0833fh
Help
"This selects the I/O address space of the adapter.  8020h-803fh is suggested."

NamedItem
Prompt  "BIOS Address"
Choice  "D4000h-Dos-OS/2 non-boot"   pos[3]=1xx110xxb   MEM 0D4000h-0D5FFFh
Choice  "D6000h-Dos-OS/2 bootable"   pos[3]=1xx111xxb   MEM 0D6000h-0D7FFFh
Choice  "C8000h-Dos-OS/2 bootable"   pos[3]=1xx000xxb   MEM 0C8000h-0C9FFFh
Choice  "CA000h-Dos-OS/2 non-boot"   pos[3]=1xx001xxb   MEM 0CA000h-0CBFFFh
Choice  "CC000h-Dos-OS/2 non-boot"   pos[3]=1xx010xxb   MEM 0CC000h-0CDFFFh
Choice  "CE000h-Dos-OS/2 non-boot"   pos[3]=1xx011xxb   MEM 0CE000h-0CFFFFh
Choice  "D0000h-Dos-NT   bootable"   pos[3]=1xx100xxb   MEM 0D0000h-0D1FFFh
Choice  "D2000h-Dos-NT   non-boot"   pos[3]=1xx101xxb   MEM 0D2000h-0D3FFFh
Help
"This selects the base address of the BIOS ROM.  D4000h is suggested."

NamedItem
Prompt  "Interrupt Level"
Choice  " Interrupt 15"   pos[3]=101xxxxxb      int 15
Choice  " Interrupt 14"   pos[3]=100xxxxxb      int 14
Choice  " Interrupt 11"   pos[3]=111xxxxxb      int 11
Choice  " Interrupt 10"   pos[3]=110xxxxxb      int 10
Help
"This selects the interrupt level for the adapter.  Level 15 is standard."
