AdapterId 57FEh

AdapterName "Everex Streaming Tape Controller (ID=57FE)"

NumBytes 3

NamedItem

Prompt "Port Addresses"
choice "0300h-0301h" pos[0]=0000000Xb pos[1]=00000011b io 00300h-00301h
choice "0302h-0303h" pos[0]=0000001Xb pos[1]=00000011b io 00302h-00303h
choice "0304h-0305h" pos[0]=0000010Xb pos[1]=00000011b io 00304h-00305h
choice "0306h-0307h" pos[0]=0000011Xb pos[1]=00000011b io 00306h-00307h
choice "0308h-0309h" pos[0]=0000100Xb pos[1]=00000011b io 00308h-00309h
choice "0280h-0281h" pos[0]=1000000Xb pos[1]=00000010b io 00280h-00281h
choice "0282h-0283h" pos[0]=1000001Xb pos[1]=00000010b io 00282h-00283h
choice "0284h-0285h" pos[0]=1000010Xb pos[1]=00000010b io 00284h-00285h
choice "0286h-0287h" pos[0]=1000011Xb pos[1]=00000010b io 00286h-00287h
choice "0288h-0289h" pos[0]=1000100Xb pos[1]=00000010b io 00288h-00289h
choice "7FF0h-7FF1h" pos[0]=1111000Xb pos[1]=01111111b io 07FF0h-07FF1h
choice "7FF2h-7FF3h" pos[0]=1111001Xb pos[1]=01111111b io 07FF2h-07FF3h
choice "7FF4h-7FF5h" pos[0]=1111010Xb pos[1]=01111111b io 07FF4h-07FF5h
choice "7FF6h-7FF7h" pos[0]=1111011Xb pos[1]=01111111b io 07FF6h-07FF7h
choice "7FF8h-7FF9h" pos[0]=1111100Xb pos[1]=01111111b io 07FF8h-07FF9h
choice "FFFEh-FFFFh" pos[0]=1111111Xb pos[1]=11111111b io 0FFFEh-0FFFFh

Help
"Each device attached to the computer requires one or
more port addresses to communicate with the computer.   
The Everex tape system can run in any two consecutive
port addresses between 0000H and FFFEH (H=HEX), provided
that the addresses are not occupied by another device.
If the selected port addresses are already occupied by
another device, they will be marked by an asterisk (*)
and must be changed to avoid conflict. Use F5 and F6
keys to change your selection. If all the ports listed
in this menu are already used by other devices, you can
use the Everex streaming tape software INSTALL/CONFIG
program to create a customized ADF file."

NamedItem

Prompt "Interrupt Request Line"
choice "IRQ 3" pos[2]=0011XXXXb int 3
choice "IRQ 4" pos[2]=0100XXXXb int 4
choice "IRQ 5" pos[2]=0101XXXXb int 5
choice "IRQ 6" pos[2]=0110XXXXb int 6
choice "IRQ 7" pos[2]=0111XXXXb int 7

Help
"In order for a device to alert the computer that it is
ready to receive instructions, it signals the computer
by using interrupts. The Everex streaming tape controller
can run on any interrupt request line between 3 and 7.
Although the Everex tape controller and utility software
are designed to allow sharing the interrupt with other
devices and software, we recommend you configure the tape
controller to an unused interrupt line for the maximun
system performance reason."

NamedItem

Prompt "Direct Memory Access channel"
choice "DMA 1                        " pos[2]=XXXX0001b arb 1
choice "DMA 0                        " pos[2]=XXXX0000b arb 0
choice "DMA 2 (share with Diskette)  " pos[2]=XXXX0010b
choice "DMA 3 (share with Fixed Disk)" pos[2]=XXXX0011b

Help
"The tape controller uses one of the system's DMA     
channels to transfer data between disk and tape. DMA0
and DMA1 may always be used if they do not conflict
with other devices in your system (no asterisk appears).
DMA2 and DMA3 are used by the diskette and fixed disk
controllers respectively. If necessary, the tape
controller can share DMA2 or DMA3, provided that: (1)
that disk and the tape do not use the same DMA channel
at the same time; OR (2) you configure the tape software
for Single DMA Mode (refer to manual). For example, if
you use DMA2 for the tape, you will not be able to back
up diskettes except in single DMA mode. WARNING: No
asterisk will appear next to DMA2 or DMA3, even if
another add-on device in your system (e.g. a network
card) is also trying to share the same DMA, but neither
the tape nor that add-on device will work in this case."

