AdapterId	060E5H

AdapterName "Boca Research Dual Async/Parallel Adapter 2"

NumBytes 3

NamedItem

Prompt "Serial Port A"

choice "SERIAL_1     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX000111b pos[2]=XXX1XXXXb io 03f8h-03ffh int 4
choice "SERIAL_1     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX000111b pos[2]=XXX1XXXXb io 03f8h-03ffh int 3
choice "SERIAL_2     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX000011b pos[2]=XXX1XXXXb io 02f8h-02ffh int 3
choice "SERIAL_2     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX000011b pos[2]=XXX1XXXXb io 02f8h-02ffh int 4
choice "SERIAL_3     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX011000b pos[2]=XXX1XXXXb io 3220h-3227h int 3
choice "SERIAL_3     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX011000b pos[2]=XXX1XXXXb io 3220h-3227h int 4
choice "SERIAL_4     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX011001b pos[2]=XXX1XXXXb io 3228h-322fh int 3
choice "SERIAL_4     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX011001b pos[2]=XXX1XXXXb io 3228h-322fh int 4
choice "SERIAL_5     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX100000b pos[2]=XXX1XXXXb io 4220h-4227h int 3
choice "SERIAL_5     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX100000b pos[2]=XXX1XXXXb io 4220h-4227h int 4
choice "SERIAL_6     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX100001b pos[2]=XXX1XXXXb io 4228h-422fh int 3
choice "SERIAL_6     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX100001b pos[2]=XXX1XXXXb io 4228h-422fh int 4
choice "SERIAL_7     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX101000b pos[2]=XXX1XXXXb io 5220h-5227h int 3
choice "SERIAL_7     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX101000b pos[2]=XXX1XXXXb io 5220h-5227h int 4
choice "SERIAL_8     INT 3"   pos[0]=X1XXXXXXb pos[1]=XX101001b pos[2]=XXX1XXXXb io 5228h-522fh int 3
choice "SERIAL_8     INT 4"   pos[0]=X0XXXXXXb pos[1]=XX101001b pos[2]=XXX1XXXXb io 5228h-522fh int 4
choice "DISABLED"                                               pos[2]=XXX0XXXXb

Help
"This serial port may be configured at any one of 8 standard base I/O port
addresses (SERIAL_1 through SERIAL_8) , or it may be disabled.	The
standard selections for interrupt levels in the PS/2 family is for SERIAL_1
to be set to INT 4 and for SERIAL_2 through SERIAL_8 to be set to INT 3.
The BOCAMCA.SSP supports the microchannel shared interrupt scheme.  This
means that more than one serial port may be configured to use the same
interrupt level."


NamedItem

Prompt "Serial Port B"

choice "SERIAL_1     INT 4" pos[1]=11XXXXXXb pos[2]=011X0001b io 03f8h-03ffh int 4
choice "SERIAL_1     INT 3" pos[1]=11XXXXXXb pos[2]=111X0001b io 03f8h-03ffh int 3
choice "SERIAL_2     INT 3" pos[1]=11XXXXXXb pos[2]=111X0000b io 02f8h-02ffh int 3
choice "SERIAL_2     INT 4" pos[1]=11XXXXXXb pos[2]=011X0000b io 02f8h-02ffh int 4
choice "SERIAL_3     INT 3" pos[1]=00XXXXXXb pos[2]=111X0110b io 3220h-3227h int 3
choice "SERIAL_3     INT 4" pos[1]=00XXXXXXb pos[2]=011X0110b io 3220h-3227h int 4
choice "SERIAL_4     INT 3" pos[1]=01XXXXXXb pos[2]=111X0110b io 3228h-322fh int 3
choice "SERIAL_4     INT 4" pos[1]=01XXXXXXb pos[2]=011X0110b io 3228h-322fh int 4
choice "SERIAL_5     INT 3" pos[1]=00XXXXXXb pos[2]=111X1000b io 4220h-4227h int 3
choice "SERIAL_5     INT 4" pos[1]=00XXXXXXb pos[2]=011X1000b io 4220h-4227h int 4
choice "SERIAL_6     INT 3" pos[1]=01XXXXXXb pos[2]=111X1000b io 4228h-422fh int 3
choice "SERIAL_6     INT 4" pos[1]=01XXXXXXb pos[2]=011X1000b io 4228h-422fh int 4
choice "SERIAL_7     INT 3" pos[1]=00XXXXXXb pos[2]=111X1010b io 5220h-5227h int 3
choice "SERIAL_7     INT 4" pos[1]=00XXXXXXb pos[2]=011X1010b io 5220h-5227h int 4
choice "SERIAL_8     INT 3" pos[1]=01XXXXXXb pos[2]=111X1010b io 5228h-522fh int 3
choice "SERIAL_8     INT 4" pos[1]=01XXXXXXb pos[2]=011X1010b io 5228h-522fh int 4
choice "DISABLED"                            pos[2]=X10XXXXXb

Help
"This serial port may be configured at any one of 8 standard base I/O port
addresses (SERIAL_1 through SERIAL_8) , or it may be disabled.	The
standard selections for interrupt levels in the PS/2 family is for SERIAL_1
to be set to INT 4 and for SERIAL_2 through SERIAL_8 to be set to INT 3.
The BOCAMCA.SSP supports the microchannel shared interrupt scheme.  This
means that more than one serial port may be configured to use the same
interrupt level."


NamedItem

Prompt "Parallel Port"

choice "PARALLEL_1   INT 7"     pos[0]=XX11101Xb        io 03bch-03bfh  int 7
choice "PARALLEL_2   INT 7"     pos[0]=XX11010Xb        io 0378h-037bh  int 7
choice "PARALLEL_3   INT 7"     pos[0]=XX10010Xb        io 0278h-027bh  int 7
choice "DISABLED"               pos[0]=XX0XXXXXb

Help
"This is an IBM PS/2 compatible bidirectional parallel port.  It may be
configured at any one of the three standard parallel port base I/O
addresses (PARALLEL_1 through PARALLEL_3) or it may be disabled.  All
parallel ports generate interrupts on INT 7."

NamedItem

Prompt "Parallel Port Mode"

choice "Unidirectional" pos[0]=1XXXXXXXb
choice "Bidirectional"  pos[0]=0XXXXXXXb

Help
"The BOCA.MCA parallel port, like the systemboard parallel port, has the
capability of operating in either bidirectional or unidirectional modes.
The bidirectional capability is a new feature of the PS/2 family and will
only be used by software specifically written to take advantage of it.	The
default for this setting is unidirectional mode to ensure backwards
compatibility with PC software."
