;
; ADF for Intel Above Board MC32 Version 1.00
;  to be used with ADP type programs

AdapterId 070B0h

AdapterName "Intel Above Board MC32"

NumBytes 4

sysmem 1024 32

NamedItem

Prompt "System Type"

choice "70/80s (except 80 type 1)"    pos[0]=XXXXXX0Xb
choice "Model 80 (16MHz type 1)  "    pos[0]=XXXXXX1Xb

Help

"A Model 80 (16MHz type 1) supports a fast memory cycle.  To see if you have
this model, check the front panel near the ON/OFF switch for a label reading
'TYPE 8580-041'.  If you are unsure what system you have,
choose the '70/80s (except 80 type 1)' option."

NamedItem

Prompt "SIMM (memory) Speed"

choice "Slow (100ns) memory     " pos[0]=XXXXX0XXb
choice "Fast (80 or 85ns) memory" pos[0]=XXXXX1XXb

Help

"The SIMMs in your Above Board supply the board's
memory.  The DRAMs (memory chips) on these modules are usually labeled
to show their speed.  This labeling typically consists of a part number,
a dash, and the speed number.  The speed number is usually shown without
the last zero.  For example '110000J-10' means a part number '110000J'
and a speed number '10' implying 100 nanoseconds.  If you are not sure what
speed memory you have, choose the 'Slow (100ns) memory' option."

