
AdapterId 060D0h

AdapterName "Hayes JT Fax 4800P "

NumBytes 1

NamedItem

    Prompt "Adapter I/O Location"
         Choice "300h-303h"
              pos[0]=0000000Xb
              io 300h-303h
         Choice "308h-30Bh"
              pos[0]=0000001Xb
              io 308h-30Bh
         Choice "310h-313h"
              pos[0]=0000010Xb
              io 310h-313h
         Choice "318h-31Bh"
              pos[0]=0000011Xb
              io 318h-31Bh
         Choice "320h-323h"
              pos[0]=0000100Xb
              io 320h-323h
         Choice "328h-32Bh"
              pos[0]=0000101Xb
              io 328h-32Bh
         Choice "330h-333h"
              pos[0]=0000110Xb
              io 330h-333h
         Choice "338h-33Bh"
              pos[0]=0000111Xb
              io 338h-33Bh
         Choice "340h-343h"
              pos[0]=0001000Xb
              io 340h-343h
         Choice "348h-34Bh"
              pos[0]=0001001Xb
              io 348h-34Bh
         Choice "350h-353h"
              pos[0]=0001010Xb
              io 350h-353h
         Choice "358h-35Bh"
              pos[0]=0001011Xb
              io 358h-35Bh
         Choice "360h-363h"
              pos[0]=0001100Xb
              io 360h-363h
         Choice "368h-36Bh"
              pos[0]=0001101Xb
              io 368h-36Bh
         Choice "370h-373h"
              pos[0]=0001110Xb
              io 370h-373h
         Choice "378h-37Bh"
              pos[0]=0001111Xb
              io 378h-37Bh

    Help
         "To configure this adapter, you must choose the I/O location
         that the adapter will use.  There are 16 locations that can
         be selected.  Under normal circumstances, the default
         selection, (Location 300h-303h), is adequate."
