
AdapterID 08DF1h

AdapterName "IBM Image Adapter/A with Printer/Scanner Option"

Numbytes 4

FixedResources
        POS[1]=0xxxxxxxb
        POS[0]=00xxxxx1b

Nameditem
        Prompt  "DMA Arbitration Level"
          Choice  "Level 14"
             POS[0]=xxx1110xb
             arb 14
        Help
        "This selects the DMA channel arbitration level that the adapter
        will use.
        The DMA channel arbitration level is fixed at 14."

nameditem
        Prompt  "Fairness On/Off"
        Choice  "On"
             POS[0]=xx1xxxxxb
        Choice  "Off"
             POS[0]=xx0xxxxxb
        Help
        "Bus Arbitration Fairness.  This controls whether the adapter
        will release control of the bus when it has been using it
        exclusively.  Under normal circumstances select ON."

Nameditem
        Prompt  "Adapter I/O Addressing"
        Choice  "I/O Addresses 1D00 to 1D7F"
             POS[1]=xxxxxx00b
             io 1D00h-1D7Fh
        Choice  "I/O Addresses 2D00 to 2D7F"
             POS[1]=xxxxxx01b
             io 2D00h-2D7Fh
        Choice  "I/O Addresses 3D00 to 3D7F"
             POS[1]=xxxxxx10b
             io 3D00h-3D7Fh
        Choice  "I/O Addresses 4D00 to 4D7F"
             POS[1]=xxxxxx11b
             io 4D00h-4D7Fh
        Help
        "This determines Adapter I/O Addressing locations."

nameditem
       Prompt  "Adapter Memory Location"
       Choice  "Segment C000"
            POS[1]=x00000xxb
            MEM  0C0000h-0C1FFFh
       Choice  "Segment C200"
            POS[1]=x00010xxb
            MEM  0C2000h-0C3FFFh
       Choice  "Segment C400"
            POS[1]=x00100xxb
            MEM  0C4000h-0C5FFFh
       Choice  "Segment C600"
            POS[1]=x00110xxb
            MEM  0C6000h-0C7FFFh
       Choice  "Segment C800"
            POS[1]=x01000xxb
            MEM  0C8000h-0C9FFFh
       Choice  "Segment CA00"
            POS[1]=x01010xxb
            MEM  0CA000h-0CBFFFh
       Choice  "Segment CC00"
            POS[1]=x01100xxb
            MEM  0CC000h-0CDFFFh
       Choice  "Segment CE00"
            POS[1]=x01110xxb
            MEM  0CE000h-0CFFFFh
       Choice  "Segment D000"
            POS[1]=x10000xxb
            MEM  0D0000h-0D1FFFh
       Choice  "Segment D200"
            POS[1]=x10010xxb
            MEM  0D2000h-0D3FFFh
       Choice  "Segment D400"
            POS[1]=x10100xxb
            MEM  0D4000h-0D5FFFh
       Choice  "Segment D600"
            POS[1]=x10110xxb
            MEM  0D6000h-0D7FFFh
       Choice  "Segment D800"
            POS[1]=x11000xxb
            MEM  0D8000h-0D9FFFh
       Choice  "Segment DA00"
            POS[1]=x11010xxb
            MEM  0DA000h-0DBFFFh
       Choice  "Segment DC00"
            POS[1]=x11100xxb
            MEM  0DC000h-0DDFFFh
       Choice  "Segment DE00"
            POS[1]=x11110xxb
            MEM  0DE000h-0DFFFFh
       Choice  "ROM Disable"
            POS[1]=x00001xxb
       Help
       "To configure this adapter you must choose the memory location
        the adapter will use for the BIOS ROM, and RAM window.  There
        are sixteen memory locations that can be selected.    Under
        normal circumstances a video adapter will select location
        C0000."

Nameditem
       Prompt  "Extended Memory Window"
       Choice  "Disabled"
            POS[2]=00000000b
       Choice  "1 Meg at Address E00000"
            POS[2]=00011111b
            POS[3]=11100000b
            MEM  0e00000h-0eFFFFFh
       Choice  "1 Meg at Address D00000"
            POS[2]=00011111b
            POS[3]=11010000b
            MEM  0d00000h-0dFFFFFh
       Choice  "1 Meg at Address C00000"
            POS[2]=00011111b
            POS[3]=11000000b
            MEM  0c00000h-0cFFFFFh
       Choice  "1 Meg at Address B00000"
            POS[2]=00011111b
            POS[3]=10110000b
            MEM  0b00000h-0bFFFFFh
       Choice  "1 Meg at Address A00000"
            POS[2]=00011111b
            POS[3]=10100000b
            MEM  0a00000h-0aFFFFFh
       Choice  "1 Meg at Address 900000"
            POS[2]=00011111b
            POS[3]=10010000b
            MEM  0900000h-09FFFFFh
       Choice  "1 Meg at Address 800000"
            POS[2]=00011111b
            POS[3]=10000000b
            MEM  0800000h-08FFFFFh
       Choice  "1 Meg at Address 700000"
            POS[2]=00011111b
            POS[3]=01110000b
            MEM  0700000h-07FFFFFh
       Choice  "1 Meg at Address 600000"
            POS[2]=00011111b
            POS[3]=01100000b
            MEM  0600000h-06FFFFFh
       Choice  "1 Meg at Address 500000"
            POS[2]=00011111b
            POS[3]=01010000b
            MEM  0500000h-05FFFFFh
       Choice  "1 Meg at Address 400000"
            POS[2]=00011111b
            POS[3]=01000000b
            MEM  0400000h-04FFFFFh
       Choice  "1 Meg at Address 300000"
            POS[2]=00011111b
            POS[3]=00110000b
            MEM  0300000h-03FFFFFh
       Choice  "1 Meg at Address 200000"
            POS[2]=00011111b
            POS[3]=00100000b
            MEM  0200000h-02FFFFFh
       Choice  "1 Meg at Address 100000"
            POS[2]=00011111b
            POS[3]=00010000b
            MEM  0100000h-01FFFFFh
       Choice  "2 Meg at Address D00000"
            POS[2]=00111111b
            POS[3]=11010000b
            MEM  0d00000h-0eFFFFFh
       Choice  "2 Meg at Address C00000"
            POS[2]=00111111b
            POS[3]=11000000b
            MEM  0c00000h-0dFFFFFh
       Choice  "2 Meg at Address B00000"
            POS[2]=00111111b
            POS[3]=10110000b
            MEM  0b00000h-0cFFFFFh
       Choice  "2 Meg at Address A00000"
            POS[2]=00111111b
            POS[3]=10100000b
            MEM  0a00000h-0bFFFFFh
       Choice  "2 Meg at Address 900000"
            POS[2]=00111111b
            POS[3]=10010000b
            MEM  0900000h-0aFFFFFh
       Choice  "2 Meg at Address 800000"
            POS[2]=00111111b
            POS[3]=10000000b
            MEM  0800000h-09FFFFFh
       Choice  "2 Meg at Address 700000"
            POS[2]=00111111b
            POS[3]=01110000b
            MEM  0700000h-08FFFFFh
       Choice  "2 Meg at Address 600000"
            POS[2]=00111111b
            POS[3]=01100000b
            MEM  0600000h-07FFFFFh
       Choice  "2 Meg at Address 500000"
            POS[2]=00111111b
            POS[3]=01010000b
            MEM  0500000h-06FFFFFh
       Choice  "2 Meg at Address 400000"
            POS[2]=00111111b
            POS[3]=01000000b
            MEM  0400000h-05FFFFFh
       Choice  "2 Meg at Address 300000"
            POS[2]=00111111b
            POS[3]=00110000b
            MEM  0300000h-04FFFFFh
       Choice  "2 Meg at Address 200000"
            POS[2]=00111111b
            POS[3]=00100000b
            MEM  0200000h-03FFFFFh
       Choice  "2 Meg at Address 100000"
            POS[2]=00111111b
            POS[3]=00010000b
            MEM  0100000h-02FFFFFh
       Help
       "Some applications may require an Extended Memory Window into
        Image Adapter/A RAM to appear high in the system address space.
        Use F6 to enable/disable and set the size/location. Under normal
        circumstances select disable."

NamedItem
       Prompt "Interrupt Level"
       Choice "Interrupt 2"
            POS[1]=XXXXXXXXb
            POS[2]=XXXXXXXXb
            INT 2d

       Help
       "This selects the Interrupt level that the adapter will use.
        The Interrupt level is fixed at 2."

